0
Checking if there is a USB storage with update file wb6_update.fit
dev: usb1_vbus @ regulator@0
starting USB...
USB0:   USB EHCI 1.00
USB1:   USB EHCI 1.00
scanning bus 0 for devices... 1 USB Device(s) found
scanning bus 1 for devices... EHCI timed out on TD - token=0x80008c80
unable to get device descriptor (error=-1)
1 USB Device(s) found
       scanning usb for storage devices... 0 Storage Device(s) found
No storage devices, perhaps not 'usb start'ed..?
No USB update detected, continuing boot
switch to partitions #0, OK
mmc0(part 0) is current device
SD/MMC found on device 0
324 bytes read in 66 ms (3.9 KiB/s)
Importing environment from 0x82000000...
Checking if uenvcmd is set ...
Running default loadzimage ...
6304616 bytes read in 5618 ms (1.1 MiB/s)

MMC read: dev # 0, block # 2016, count 32 ... 32 blocks read: OK
Reading overlays list from eMMC
Reading factory fdt name from eMMC
Loading factory fdt imx6ul-wirenboard690
47776 bytes read in 122 ms (381.8 KiB/s)
485 bytes read in 195 ms (2 KiB/s)
Applying DT overlay wb6-nogsm
597 bytes read in 219 ms (2 KiB/s)
Applying DT overlay wb6-wifi-rtl8723bu
509 bytes read in 200 ms (2 KiB/s)
Applying DT overlay wb6-noradio
334 bytes read in 159 ms (2 KiB/s)
Applying DT overlay wb6-eth1
254 bytes read in 100 ms (2 KiB/s)
Applying DT overlay temp-industrial
Applying extra overlay
Booting from mmc ...
## Flattened Device Tree blob at 83000000
   Booting using the fdt blob at 0x83000000
   Loading Device Tree to bef4c000, end bef6efff ... OK

Starting kernel ...

[    0.000000] Booting Linux on physical CPU 0x0
[    0.000000] Linux version 5.10.35-wb172 (root@wbdevenv) (arm-linux-gnueabihf-gcc (Debian 10.2.1-6) 10.2.1 20210110, GNU ld (GNU Binutils for Debian) 2.35.2) #1 Wed Oct 16 09:17:25 UTC 2024
[    0.000000] CPU: ARMv7 Processor [410fc075] revision 5 (ARMv7), cr=10c53c7d
[    0.000000] CPU: div instructions available: patching division code
[    0.000000] CPU: PIPT / VIPT nonaliasing data cache, VIPT aliasing instruction cache
[    0.000000] OF: fdt: Machine model: Wiren Board rev. 6.9.0 (i.MX6UL/ULL)
[    0.000000] Memory policy: Data cache writeback
[    0.000000] cma: Reserved 16 MiB at 0xbf000000
[    0.000000] Zone ranges:
[    0.000000]   Normal   [mem 0x0000000080000000-0x00000000bfffffff]
[    0.000000] Movable zone start for each node
[    0.000000] Early memory node ranges
[    0.000000]   node   0: [mem 0x0000000080000000-0x00000000bfffffff]
[    0.000000] Initmem setup node 0 [mem 0x0000000080000000-0x00000000bfffffff]
[    0.000000] CPU: All CPU(s) started in SVC mode.
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 259840
[    0.000000] Kernel command line: console=ttymxc0,115200 root=/dev/mmcblk0p2 rootwait ro
[    0.000000] Dentry cache hash table entries: 131072 (order: 7, 524288 bytes, linear)
[    0.000000] Inode-cache hash table entries: 65536 (order: 6, 262144 bytes, linear)
[    0.000000] mem auto-init: stack:off, heap alloc:off, heap free:off
[    0.000000] Memory: 1008652K/1048576K available (8192K kernel code, 728K rwdata, 2776K rodata, 1024K init, 283K bss, 23540K reserved, 16384K cma-reserved)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=1, Nodes=1
[    0.000000] NR_IRQS: 16, nr_irqs: 16, preallocated irqs: 16
[    0.000000] random: get_random_bytes called from start_kernel+0x234/0x3dc with crng_init=0
[    0.000000] Switching to timer-based delay loop, resolution 41ns
[    0.000018] sched_clock: 32 bits at 24MHz, resolution 41ns, wraps every 89478484971ns
[    0.000058] clocksource: mxc_timer1: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 79635851949 ns
[    0.002803] Console: colour dummy device 80x30
[    0.002864] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=240000)
[    0.002901] pid_max: default: 32768 minimum: 301
[    0.003314] Mount-cache hash table entries: 2048 (order: 1, 8192 bytes, linear)
[    0.003357] Mountpoint-cache hash table entries: 2048 (order: 1, 8192 bytes, linear)
[    0.005085] CPU: Testing write buffer coherency: ok
[    0.006326] Setting up static identity map for 0x80100000 - 0x80100078
[    0.007334] devtmpfs: initialized
[    0.025280] VFP support v0.3: implementor 41 architecture 2 part 30 variant 7 rev 5
[    0.025790] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 19112604462750000 ns
[    0.025833] futex hash table entries: 256 (order: -1, 3072 bytes, linear)
[    0.027214] pinctrl core: initialized pinctrl subsystem
[    0.029223] NET: Registered protocol family 16
[    0.031512] DMA: preallocated 256 KiB pool for atomic coherent allocations
[    0.033521] thermal_sys: Registered thermal governor 'step_wise'
[    0.033808] cpuidle: using governor menu
[    0.221506] vdd1p1: supplied by regulator-dummy
[    0.233593] vdd3p0: supplied by regulator-dummy
[    0.245704] cpu: supplied by regulator-dummy
[    0.257861] vddsoc: supplied by regulator-dummy
[    0.600377] No ATAGs?
[    0.600438] hw-breakpoint: found 5 (+1 reserved) breakpoint and 4 watchpoint registers.
[    0.600458] hw-breakpoint: maximum watchpoint size is 8 bytes.
[    0.601065] debugfs: Directory 'dummy-iomuxc-gpr@20e4000' with parent 'regmap' already present!
[    0.601725] imx6ul-pinctrl 20e0000.pinctrl: initialized IMX pinctrl driver
[    0.603277] imx6ul-pinctrl 2290000.iomuxc-snvs: no groups defined in /soc/bus@2200000/iomuxc-snvs@2290000
[    0.603319] imx6ul-pinctrl 2290000.iomuxc-snvs: initialized IMX pinctrl driver
[    0.646147] mxs-dma 1804000.dma-apbh: initialized
[    0.651429] SCSI subsystem initialized
[    0.651918] usbcore: registered new interface driver usbfs
[    0.652041] usbcore: registered new interface driver hub
[    0.652174] usbcore: registered new device driver usb
[    0.653009] gpio-48 (i2c_rtc): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.653137] gpio-49 (i2c_rtc): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.654554] i2c-gpio i2c_rtc: using lines 48 (SDA) and 49 (SCL)
[    0.655441] gpio-76 (i2c_eeprom1): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.655570] gpio-67 (i2c_eeprom1): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.656164] i2c-gpio i2c_eeprom1: using lines 76 (SDA) and 67 (SCL)
[    0.656859] gpio-70 (i2c_eeprom2): enforced open drain please flag it properly in DT/ACPI DSDT/board fi▒
U-Boot SPL 2017.03-wb1.3.0-g520058c326 (Jan 18 2022 - 10:56:38)
DRAM init ok, rows:16, ncs:1, size: 1024MB
.p0_mpdgctrl0   = 0x010f010c
.p0_mpdgctrl1   = 0x0e3f0e3f
.p0_mprddlctl   = 0x3f3f3e3b
.p0_mpwrdlctl   = 0x3f3f3731
.p0_mpwldectrl0 = 0x000c000c
.p0_mpwldectrl1 = 0x000d000d
Trying to boot from MMC1
Warning - USDHC2 controller not supporting

U-Boot 2017.03-wb1.3.0-g520058c326 (Jan 18 2022 - 10:56:38 +0000)

CPU:   Freescale i.MX6ULL rev1.1 792 MHz (running at 396 MHz)
CPU:   Industrial temperature grade (-40C to 105C) at 48C
Reset cause: POR
Model: Wiren Board rev. 6.1 (i.MX6UL)
Board: Wiren Board MX6UL
DRAM:  1 GiB
MMC:   FSL_SDHC: 0
Using default environment

In:    serial
Out:   serial
Err:   serial
Net:   No ethernet found.
Hit any key to stop autoboot:  0
Checking if there is a USB storage with update file wb6_update.fit
dev: usb1_vbus @ regulator@0
starting USB...
USB0:   USB EHCI 1.00
USB1:   USB EHCI 1.00
scanning bus 0 for devices... 1 USB Device(s) found
scanning bus 1 for devices... EHCI timed out on TD - token=0x80008c80
unable to get device descriptor (error=-1)
1 USB Device(s) found
       scanning usb for storage devices... 0 Storage Device(s) found
No storage devices, perhaps not 'usb start'ed..?
No USB update detected, continuing boot
switch to partitions #0, OK
mmc0(part 0) is current device
SD/MMC found on device 0
324 bytes read in 66 ms (3.9 KiB/s)
Importing environment from 0x82000000...
Checking if uenvcmd is set ...
Running default loadzimage ...
6304616 bytes read in 5618 ms (1.1 MiB/s)

MMC read: dev # 0, block # 2016, count 32 ... 32 blocks read: OK
Reading overlays list from eMMC
Reading factory fdt name from eMMC
Loading factory fdt imx6ul-wirenboard690
47776 bytes read in 122 ms (381.8 KiB/s)
485 bytes read in 195 ms (2 KiB/s)
Applying DT overlay wb6-nogsm
597 bytes read in 219 ms (2 KiB/s)
Applying DT overlay wb6-wifi-rtl8723bu
509 bytes read in 200 ms (2 KiB/s)
Applying DT overlay wb6-noradio
334 bytes read in 160 ms (2 KiB/s)
Applying DT overlay wb6-eth1
254 bytes read in 100 ms (2 KiB/s)
Applying DT overlay temp-industrial
Applying extra overlay
Booting from mmc ...
## Flattened Device Tree blob at 83000000
   Booting using the fdt blob at 0x83000000
   Loading Device Tree to bef4c000, end bef6efff ... OK

Starting kernel ...

[    0.000000] Booting Linux on physical CPU 0x0
[    0.000000] Linux version 5.10.35-wb172 (root@wbdevenv) (arm-linux-gnueabihf-gcc (Debian 10.2.1-6) 10.2.1 20210110, GNU ld (GNU Binutils for Debian) 2.35.2) #1 Wed Oct 16 09:17:25 UTC 2024
[    0.000000] CPU: ARMv7 Processor [410fc075] revision 5 (ARMv7), cr=10c53c7d
[    0.000000] CPU: div instructions available: patching division code
[    0.000000] CPU: PIPT / VIPT nonaliasing data cache, VIPT aliasing instruction cache
[    0.000000] OF: fdt: Machine model: Wiren Board rev. 6.9.0 (i.MX6UL/ULL)
[    0.000000] Memory policy: Data cache writeback
[    0.000000] cma: Reserved 16 MiB at 0xbf000000
[    0.000000] Zone ranges:
[    0.000000]   Normal   [mem 0x0000000080000000-0x00000000bfffffff]
[    0.000000] Movable zone start for each node
[    0.000000] Early memory node ranges
[    0.000000]   node   0: [mem 0x0000000080000000-0x00000000bfffffff]
[    0.000000] Initmem setup node 0 [mem 0x0000000080000000-0x00000000bfffffff]
[    0.000000] CPU: All CPU(s) started in SVC mode.
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 259840
[    0.000000] Kernel command line: console=ttymxc0,115200 root=/dev/mmcblk0p2 rootwait ro
[    0.000000] Dentry cache hash table entries: 131072 (order: 7, 524288 bytes, linear)
[    0.000000] Inode-cache hash table entries: 65536 (order: 6, 262144 bytes, linear)
[    0.000000] mem auto-init: stack:off, heap alloc:off, heap free:off
[    0.000000] Memory: 1008652K/1048576K available (8192K kernel code, 728K rwdata, 2776K rodata, 1024K init, 283K bss, 23540K reserved, 16384K cma-reserved)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=1, Nodes=1
[    0.000000] NR_IRQS: 16, nr_irqs: 16, preallocated irqs: 16
[    0.000000] random: get_random_bytes called from start_kernel+0x234/0x3dc with crng_init=0
[    0.000000] Switching to timer-based delay loop, resolution 41ns
[    0.000019] sched_clock: 32 bits at 24MHz, resolution 41ns, wraps every 89478484971ns
[    0.000059] clocksource: mxc_timer1: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 79635851949 ns
[    0.002802] Console: colour dummy device 80x30
[    0.002865] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=240000)
[    0.002903] pid_max: default: 32768 minimum: 301
[    0.003323] Mount-cache hash table entries: 2048 (order: 1, 8192 bytes, linear)
[    0.003366] Mountpoint-cache hash table entries: 2048 (order: 1, 8192 bytes, linear)
[    0.005092] CPU: Testing write buffer coherency: ok
[    0.006350] Setting up static identity map for 0x80100000 - 0x80100078
[    0.007357] devtmpfs: initialized
[    0.025332] VFP support v0.3: implementor 41 architecture 2 part 30 variant 7 rev 5
[    0.025845] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 19112604462750000 ns
[    0.025889] futex hash table entries: 256 (order: -1, 3072 bytes, linear)
[    0.027270] pinctrl core: initialized pinctrl subsystem
[    0.029294] NET: Registered protocol family 16
[    0.031594] DMA: preallocated 256 KiB pool for atomic coherent allocations
[    0.033611] thermal_sys: Registered thermal governor 'step_wise'
[    0.033897] cpuidle: using governor menu
[    0.221674] vdd1p1: supplied by regulator-dummy
[    0.233765] vdd3p0: supplied by regulator-dummy
[    0.245915] cpu: supplied by regulator-dummy
[    0.258043] vddsoc: supplied by regulator-dummy
[    0.600510] No ATAGs?
[    0.600570] hw-breakpoint: found 5 (+1 reserved) breakpoint and 4 watchpoint registers.
[    0.600591] hw-breakpoint: maximum watchpoint size is 8 bytes.
[    0.601194] debugfs: Directory 'dummy-iomuxc-gpr@20e4000' with parent 'regmap' already present!
[    0.601852] imx6ul-pinctrl 20e0000.pinctrl: initialized IMX pinctrl driver
[    0.603408] imx6ul-pinctrl 2290000.iomuxc-snvs: no groups defined in /soc/bus@2200000/iomuxc-snvs@2290000
[    0.603448] imx6ul-pinctrl 2290000.iomuxc-snvs: initialized IMX pinctrl driver
[    0.646336] mxs-dma 1804000.dma-apbh: initialized
[    0.651625] SCSI subsystem initialized
[    0.652097] usbcore: registered new interface driver usbfs
[    0.652219] usbcore: registered new interface driver hub
[    0.652352] usbcore: registered new device driver usb
[    0.653188] gpio-48 (i2c_rtc): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.653316] gpio-49 (i2c_rtc): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.654721] i2c-gpio i2c_rtc: using lines 48 (SDA) and 49 (SCL)
[    0.655611] gpio-76 (i2c_eeprom1): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.655739] gpio-67 (i2c_eeprom1): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.656318] i2c-gpio i2c_eeprom1: using lines 76 (SDA) and 6▒
U-Boot SPL 2017.03-wb1.3.0-g520058c326 (Jan 18 2022 - 10:56:38)
DRAM init ok, rows:16, ncs:1, size: 1024MB
.p0_mpdgctrl0   = 0x01120109
.p0_mpdgctrl1   = 0x0e3f0e3f
.p0_mprddlctl   = 0x3f3f3d3b
.p0_mpwrdlctl   = 0x3f3f3832
.p0_mpwldectrl0 = 0x000c000c
.p0_mpwldectrl1 = 0x000d000d
Trying to boot from MMC1
Warning - USDHC2 controller not supporting

U-Boot 2017.03-wb1.3.0-g520058c326 (Jan 18 2022 - 10:56:38 +0000)

CPU:   Freescale i.MX6ULL rev1.1 792 MHz (running at 396 MHz)
CPU:   Industrial temperature grade (-40C to 105C) at 48C
Reset cause: POR
Model: Wiren Board rev. 6.1 (i.MX6UL)
Board: Wiren Board MX6UL
DRAM:  1 GiB
MMC:   FSL_SDHC: 0
Using default environment

In:    serial
Out:   serial
Err:   serial
Net:   No ethernet found.
Hit any key to stop autoboot:  0
Checking if there is a USB storage with update file wb6_update.fit
dev: usb1_vbus @ regulator@0
starting USB...
USB0:   USB EHCI 1.00
USB1:   USB EHCI 1.00
scanning bus 0 for devices... 1 USB Device(s) found
scanning bus 1 for devices... EHCI timed out on TD - token=0x80008c80
unable to get device descriptor (error=-1)
1 USB Device(s) found
       scanning usb for storage devices... 0 Storage Device(s) found
No storage devices, perhaps not 'usb start'ed..?
No USB update detected, continuing boot
switch to partitions #0, OK
mmc0(part 0) is current device
SD/MMC found on device 0
324 bytes read in 66 ms (3.9 KiB/s)
Importing environment from 0x82000000...
Checking if uenvcmd is set ...
Running default loadzimage ...
6304616 bytes read in 5618 ms (1.1 MiB/s)

MMC read: dev # 0, block # 2016, count 32 ... 32 blocks read: OK
Reading overlays list from eMMC
Reading factory fdt name from eMMC
Loading factory fdt imx6ul-wirenboard690
47776 bytes read in 122 ms (381.8 KiB/s)
485 bytes read in 195 ms (2 KiB/s)
Applying DT overlay wb6-nogsm
597 bytes read in 219 ms (2 KiB/s)
Applying DT overlay wb6-wifi-rtl8723bu
509 bytes read in 200 ms (2 KiB/s)
Applying DT overlay wb6-noradio
334 bytes read in 160 ms (2 KiB/s)
Applying DT overlay wb6-eth1
254 bytes read in 100 ms (2 KiB/s)
Applying DT overlay temp-industrial
Applying extra overlay
Booting from mmc ...
## Flattened Device Tree blob at 83000000
   Booting using the fdt blob at 0x83000000
   Loading Device Tree to bef4c000, end bef6efff ... OK

Starting kernel ...

[    0.000000] Booting Linux on physical CPU 0x0
[    0.000000] Linux version 5.10.35-wb172 (root@wbdevenv) (arm-linux-gnueabihf-gcc (Debian 10.2.1-6) 10.2.1 20210110, GNU ld (GNU Binutils for Debian) 2.35.2) #1 Wed Oct 16 09:17:25 UTC 2024
[    0.000000] CPU: ARMv7 Processor [410fc075] revision 5 (ARMv7), cr=10c53c7d
[    0.000000] CPU: div instructions available: patching division code
[    0.000000] CPU: PIPT / VIPT nonaliasing data cache, VIPT aliasing instruction cache
[    0.000000] OF: fdt: Machine model: Wiren Board rev. 6.9.0 (i.MX6UL/ULL)
[    0.000000] Memory policy: Data cache writeback
[    0.000000] cma: Reserved 16 MiB at 0xbf000000
[    0.000000] Zone ranges:
[    0.000000]   Normal   [mem 0x0000000080000000-0x00000000bfffffff]
[    0.000000] Movable zone start for each node
[    0.000000] Early memory node ranges
[    0.000000]   node   0: [mem 0x0000000080000000-0x00000000bfffffff]
[    0.000000] Initmem setup node 0 [mem 0x0000000080000000-0x00000000bfffffff]
[    0.000000] CPU: All CPU(s) started in SVC mode.
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 259840
[    0.000000] Kernel command line: console=ttymxc0,115200 root=/dev/mmcblk0p2 rootwait ro
[    0.000000] Dentry cache hash table entries: 131072 (order: 7, 524288 bytes, linear)
[    0.000000] Inode-cache hash table entries: 65536 (order: 6, 262144 bytes, linear)
[    0.000000] mem auto-init: stack:off, heap alloc:off, heap free:off
[    0.000000] Memory: 1008652K/1048576K available (8192K kernel code, 728K rwdata, 2776K rodata, 1024K init, 283K bss, 23540K reserved, 16384K cma-reserved)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=1, Nodes=1
[    0.000000] NR_IRQS: 16, nr_irqs: 16, preallocated irqs: 16
[    0.000000] random: get_random_bytes called from start_kernel+0x234/0x3dc with crng_init=0
[    0.000000] Switching to timer-based delay loop, resolution 41ns
[    0.000018] sched_clock: 32 bits at 24MHz, resolution 41ns, wraps every 89478484971ns
[    0.000057] clocksource: mxc_timer1: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 79635851949 ns
[    0.002802] Console: colour dummy device 80x30
[    0.002866] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=240000)
[    0.002904] pid_max: default: 32768 minimum: 301
[    0.003317] Mount-cache hash table entries: 2048 (order: 1, 8192 bytes, linear)
[    0.003360] Mountpoint-cache hash table entries: 2048 (order: 1, 8192 bytes, linear)
[    0.005089] CPU: Testing write buffer coherency: ok
[    0.006314] Setting up static identity map for 0x80100000 - 0x80100078
[    0.007336] devtmpfs: initialized
[    0.025327] VFP support v0.3: implementor 41 architecture 2 part 30 variant 7 rev 5
[    0.025841] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 19112604462750000 ns
[    0.025886] futex hash table entries: 256 (order: -1, 3072 bytes, linear)
[    0.027273] pinctrl core: initialized pinctrl subsystem
[    0.029267] NET: Registered protocol family 16
[    0.031563] DMA: preallocated 256 KiB pool for atomic coherent allocations
[    0.033581] thermal_sys: Registered thermal governor 'step_wise'
[    0.033868] cpuidle: using governor menu
[    0.221651] vdd1p1: supplied by regulator-dummy
[    0.233769] vdd3p0: supplied by regulator-dummy
[    0.245919] cpu: supplied by regulator-dummy
[    0.258087] vddsoc: supplied by regulator-dummy
[    0.600604] No ATAGs?
[    0.600665] hw-breakpoint: found 5 (+1 reserved) breakpoint and 4 watchpoint registers.
[    0.600686] hw-breakpoint: maximum watchpoint size is 8 bytes.
[    0.601288] debugfs: Directory 'dummy-iomuxc-gpr@20e4000' with parent 'regmap' already present!
[    0.601954] imx6ul-pinctrl 20e0000.pinctrl: initialized IMX pinctrl driver
[    0.603513] imx6ul-pinctrl 2290000.iomuxc-snvs: no groups defined in /soc/bus@2200000/iomuxc-snvs@2290000
[    0.603555] imx6ul-pinctrl 2290000.iomuxc-snvs: initialized IMX pinctrl driver
[    0.646405] mxs-dma 1804000.dma-apbh: initialized
[    0.651662] SCSI subsystem initialized
[    0.652138] usbcore: registered new interface driver usbfs
[    0.652268] usbcore: registered new interface driver hub
[    0.652395] usbcore: registered new device driver usb
[    0.653231] gpio-48 (i2c_rtc): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.653442] gpio-49 (i2c_rtc): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.654768] i2c-gpio i2c_rtc: using lines 48 (SDA) and 49 (SCL)
[    0.655653] gpio-76 (i2c_eeprom1): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.655784] gpio-67 (i2c_eeprom1): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.656379] i2c-gpio i2c_eeprom1▒
U-Boot SPL 2017.03-wb1.3.0-g520058c326 (Jan 18 2022 - 10:56:38)
DRAM init ok, rows:16, ncs:1, size: 1024MB
.p0_mpdgctrl0   = 0x010f0109
.p0_mpdgctrl1   = 0x0e3f0e3f
.p0_mprddlctl   = 0x3f3f3d3b
.p0_mpwrdlctl   = 0x3f3f3832
.p0_mpwldectrl0 = 0x000c000c
.p0_mpwldectrl1 = 0x000d000d
Trying to boot from MMC1
Warning - USDHC2 controller not supporting

U-Boot 2017.03-wb1.3.0-g520058c326 (Jan 18 2022 - 10:56:38 +0000)

CPU:   Freescale i.MX6ULL rev1.1 792 MHz (running at 396 MHz)
CPU:   Industrial temperature grade (-40C to 105C) at 48C
Reset cause: POR
Model: Wiren Board rev. 6.1 (i.MX6UL)
Board: Wiren Board MX6UL
DRAM:  1 GiB
MMC:   FSL_SDHC: 0
Using default environment

In:    serial
Out:   serial
Err:   serial
Net:   No ethernet found.
Hit any key to stop autoboot:  0
Checking if there is a USB storage with update file wb6_update.fit
dev: usb1_vbus @ regulator@0
starting USB...
USB0:   USB EHCI 1.00
USB1:   USB EHCI 1.00
scanning bus 0 for devices... 1 USB Device(s) found
scanning bus 1 for devices... EHCI timed out on TD - token=0x80008c80
unable to get device descriptor (error=-1)
1 USB Device(s) found
       scanning usb for storage devices... 0 Storage Device(s) found
No storage devices, perhaps not 'usb start'ed..?
No USB update detected, continuing boot
switch to partitions #0, OK
mmc0(part 0) is current device
SD/MMC found on device 0
324 bytes read in 66 ms (3.9 KiB/s)
Importing environment from 0x82000000...
Checking if uenvcmd is set ...
Running default loadzimage ...
6304616 bytes read in 5618 ms (1.1 MiB/s)

MMC read: dev # 0, block # 2016, count 32 ... 32 blocks read: OK
Reading overlays list from eMMC
Reading factory fdt name from eMMC
Loading factory fdt imx6ul-wirenboard690
47776 bytes read in 122 ms (381.8 KiB/s)
485 bytes read in 195 ms (2 KiB/s)
Applying DT overlay wb6-nogsm
597 bytes read in 219 ms (2 KiB/s)
Applying DT overlay wb6-wifi-rtl8723bu
509 bytes read in 200 ms (2 KiB/s)
Applying DT overlay wb6-noradio
334 bytes read in 160 ms (2 KiB/s)
Applying DT overlay wb6-eth1
254 bytes read in 100 ms (2 KiB/s)
Applying DT overlay temp-industrial
Applying extra overlay
Booting from mmc ...
## Flattened Device Tree blob at 83000000
   Booting using the fdt blob at 0x83000000
   Loading Device Tree to bef4c000, end bef6efff ... OK

Starting kernel ...

[    0.000000] Booting Linux on physical CPU 0x0
[    0.000000] Linux version 5.10.35-wb172 (root@wbdevenv) (arm-linux-gnueabihf-gcc (Debian 10.2.1-6) 10.2.1 20210110, GNU ld (GNU Binutils for Debian) 2.35.2) #1 Wed Oct 16 09:17:25 UTC 2024
[    0.000000] CPU: ARMv7 Processor [410fc075] revision 5 (ARMv7), cr=10c53c7d
[    0.000000] CPU: div instructions available: patching division code
[    0.000000] CPU: PIPT / VIPT nonaliasing data cache, VIPT aliasing instruction cache
[    0.000000] OF: fdt: Machine model: Wiren Board rev. 6.9.0 (i.MX6UL/ULL)
[    0.000000] Memory policy: Data cache writeback
[    0.000000] cma: Reserved 16 MiB at 0xbf000000
[    0.000000] Zone ranges:
[    0.000000]   Normal   [mem 0x0000000080000000-0x00000000bfffffff]
[    0.000000] Movable zone start for each node
[    0.000000] Early memory node ranges
[    0.000000]   node   0: [mem 0x0000000080000000-0x00000000bfffffff]
[    0.000000] Initmem setup node 0 [mem 0x0000000080000000-0x00000000bfffffff]
[    0.000000] CPU: All CPU(s) started in SVC mode.
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 259840
[    0.000000] Kernel command line: console=ttymxc0,115200 root=/dev/mmcblk0p2 rootwait ro
[    0.000000] Dentry cache hash table entries: 131072 (order: 7, 524288 bytes, linear)
[    0.000000] Inode-cache hash table entries: 65536 (order: 6, 262144 bytes, linear)
[    0.000000] mem auto-init: stack:off, heap alloc:off, heap free:off
[    0.000000] Memory: 1008652K/1048576K available (8192K kernel code, 728K rwdata, 2776K rodata, 1024K init, 283K bss, 23540K reserved, 16384K cma-reserved)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=1, Nodes=1
[    0.000000] NR_IRQS: 16, nr_irqs: 16, preallocated irqs: 16
[    0.000000] random: get_random_bytes called from start_kernel+0x234/0x3dc with crng_init=0
[    0.000000] Switching to timer-based delay loop, resolution 41ns
[    0.000020] sched_clock: 32 bits at 24MHz, resolution 41ns, wraps every 89478484971ns
[    0.000061] clocksource: mxc_timer1: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 79635851949 ns
[    0.002799] Console: colour dummy device 80x30
[    0.002865] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=240000)
[    0.002904] pid_max: default: 32768 minimum: 301
[    0.003317] Mount-cache hash table entries: 2048 (order: 1, 8192 bytes, linear)
[    0.003362] Mountpoint-cache hash table entries: 2048 (order: 1, 8192 bytes, linear)
[    0.005091] CPU: Testing write buffer coherency: ok
[    0.006327] Setting up static identity map for 0x80100000 - 0x80100078
[    0.007327] devtmpfs: initialized
[    0.025293] VFP support v0.3: implementor 41 architecture 2 part 30 variant 7 rev 5
[    0.025801] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 19112604462750000 ns
[    0.025845] futex hash table entries: 256 (order: -1, 3072 bytes, linear)
[    0.027236] pinctrl core: initialized pinctrl subsystem
[    0.029246] NET: Registered protocol family 16
[    0.031549] DMA: preallocated 256 KiB pool for atomic coherent allocations
[    0.033559] thermal_sys: Registered thermal governor 'step_wise'
[    0.033844] cpuidle: using governor menu
[    0.221525] vdd1p1: supplied by regulator-dummy
[    0.233623] vdd3p0: supplied by regulator-dummy
[    0.245741] cpu: supplied by regulator-dummy
[    0.257897] vddsoc: supplied by regulator-dummy
[    0.600211] No ATAGs?
[    0.600270] hw-breakpoint: found 5 (+1 reserved) breakpoint and 4 watchpoint registers.
[    0.600292] hw-breakpoint: maximum watchpoint size is 8 bytes.
[    0.600894] debugfs: Directory 'dummy-iomuxc-gpr@20e4000' with parent 'regmap' already present!
[    0.601554] imx6ul-pinctrl 20e0000.pinctrl: initialized IMX pinctrl driver
[    0.603025] imx6ul-pinctrl 2290000.iomuxc-snvs: no groups defined in /soc/bus@2200000/iomuxc-snvs@2290000
[    0.603138] imx6ul-pinctrl 2290000.iomuxc-snvs: initialized IMX pinctrl driver
[    0.645986] mxs-dma 1804000.dma-apbh: initialized
[    0.651271] SCSI subsystem initialized
[    0.651750] usbcore: registered new interface driver usbfs
[    0.651872] usbcore: registered new interface driver hub
[    0.652007] usbcore: registered new device driver usb
[    0.652849] gpio-48 (i2c_rtc): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.652980] gpio-49 (i2c_rtc): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.654378] i2c-gpio i2c_rtc: using lines 48 (SDA) and 49 (SCL)
[    0.655276] gpio-76 (i2c_eeprom1): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.655407] gpio-67 (i2c_eeprom1): enforced open drain please flag it properly in DT/A▒
U-Boot SPL 2017.03-wb1.3.0-g520058c326 (Jan 18 2022 - 10:56:38)
DRAM init ok, rows:16, ncs:1, size: 1024MB
.p0_mpdgctrl0   = 0x010c0106
.p0_mpdgctrl1   = 0x0e3f0e3f
.p0_mprddlctl   = 0x3f3f3d3b
.p0_mpwrdlctl   = 0x3f3f3731
.p0_mpwldectrl0 = 0x000c000c
.p0_mpwldectrl1 = 0x000d000d
Trying to boot from MMC1
Warning - USDHC2 controller not supporting

U-Boot 2017.03-wb1.3.0-g520058c326 (Jan 18 2022 - 10:56:38 +0000)

CPU:   Freescale i.MX6ULL rev1.1 792 MHz (running at 396 MHz)
CPU:   Industrial temperature grade (-40C to 105C) at 48C
Reset cause: POR
Model: Wiren Board rev. 6.1 (i.MX6UL)
Board: Wiren Board MX6UL
DRAM:  1 GiB
MMC:   FSL_SDHC: 0
Using default environment

In:    serial
Out:   serial
Err:   serial
Net:   No ethernet found.
Hit any key to stop autoboot:  1