wirenboard-AIBYLRXZ login:
wirenboard-AIBYLRXZ login: root
Password:
          _                _                         _
__      _(_)_ __ ___ _ __ | |__   ___   __ _ _ __ __| |
\ \ /\ / / | '__/ _ \ '_ \| '_ \ / _ \ / _` | '__/ _` |
 \ V  V /| | | |  __/ | | | |_) | (_) | (_| | | | (_| |
  \_/\_/ |_|_|  \___|_| |_|_.__/ \___/ \__,_|_|  \__,_|

Welcome to Wiren Board 8.4.3 (s/n AIBYLRXZ), release wb-2602 (as stable)
Linux wirenboard-AIBYLRXZ 6.8.0-wb153 #1 SMP Wed Mar  4 13:38:44 UTC 2026 aarch6                                                                                      4 GNU/Linux

System load:   0.29 0.53 0.46   Up time:       40 min
Memory usage:  23% of 3.84G     Usage of /:    64% of 2.0G      /mnt/data:     2                                                                                      8% of 55G

eth1 ip: 200a

Last login: Tue Mar 24 12:13:59 UTC 2026 from 192.168.1.38 on pts/0
root@wirenboard-AIBYLRXZ:~# [ 2587.287071] input input0: power key press detecte                                                                                      d
         Stopping Session 3 of user root.
[  OK  ] Removed slice system-modprobe.slice.
[  OK  ] Removed slice system-wb\x2dcloud\x2dagent\x2dfrpc.slice.
[  OK  ] Stopped target Bluetooth.
[  OK  ] Stopped target Graphical Interface.
[  OK  ] Stopped target Timers.
[  OK  ] Stopped Daily apt upgrade and clean activities.
[  OK  ] Stopped Daily apt download activities.
[  OK  ] Stopped Periodic ext4 Onli…ata Check for All Filesystems.
[  OK  ] Stopped Discard unused blocks once a week.
[  OK  ] Stopped Daily rotation of log files.
[  OK  ] Stopped Clean PHP session files every 30 mins.
[  OK  ] Stopped Daily Cleanup of Temporary Directories.
[  OK  ] Stopped target Hardware activated USB gadget.
[  OK  ] Closed Load/Save RF Kill Switch Status /dev/rfkill Watch.
         Stopping Bluetooth service...
         Stopping Load/Save Random Seed...
         Stoppin[ 2587.747005] wbec-watchdog 5011000.spi:wbec@0:wbec-watchdog@0:                                                                                       stop watchdog, but actually EC watchdog is always running, timeout set to 300 s                                                                                      econds
g watchdog daemon...
[  OK  ] Stopped Bluetooth service.
[  OK  ] Stopped Serial Getty on ttyS0.
[  OK  ] Stopped Load/Save Random Seed.
[  OK  ] Stopped Session 3 of user root.
[  OK  ] Removed slice system-serial\x2dgetty.slice.
         Stopping User Manager for UID 0...
[  OK  ] Stopped watchdog daemon.
[  OK  ] Stopped User Manager for UID 0.
[  OK  ] Stopped target Multi-User System.
[  OK  ] Stopped target Login Prompts.
         Stopping Avahi mDNS/DNS-SD Stack...
         Stopping Regular background program processing daemon...
         Stopping Docker Application Container Engine...
         Stopping Getty on tty1...
         Stopping Access point and …rver for Wi-Fi and Ethernet...
         Stopping LSB: Brings up/down network automatically...
         Stopping The PHP 7.4 FastCGI Process Manager...
         Stopping User Login Management...
         Stopping User Runtime Directory /run/user/0...
         Stopping telegraf metric s…rd Cloud (wirenboard.cloud)...
         Stopping Wiren Board Cloud Agent (wirenboard.cloud)...
         Stopping Wiren Board modbus devices manager...
         Stopping one-click diagnos…enerating archive with data...
         Stopping Initialize Wiren Board on successful boot...
[  OK  ] Stopped KNXD Configurator for Wiren Board.
         Stopping MQTT Driver for ADC...
         Stopping Wiren Board configuration editor backend...
         Stopping Wiren Board database logger...
         Stopping MQTT Driver for GPIO-controlled switches...
         Stopping Wiren Board MQTT KNX bridge...
         Stopping Wiren Board journald to MQTT gateway...
         Stopping metrics sender...
         Stopping Kernel 1-Wire MQTT driver for WB-HomA...
         Stopping MQTT Rule engine for Wiren Board...
         Stopping Wiren Board firmware update service...
[  OK  ] Unmounted /run/user/0.
[  OK  ] Stopped Regular background program processing daemon.
[  OK  ] Stopped Avahi mDNS/DNS-SD Stack.
[  OK  ] Stopped Getty on tty1.
[  OK  ] Stopped one-click diagnost… generating archive with data.
[  OK  ] Stopped Wiren Board configuration editor backend.
[  OK  ] Stopped Wiren Board database logger.
[  OK  ] Stopped Wiren Board journald to MQTT gateway.
[  OK  ] Stopped MQTT Rule engine for Wiren Board.
[  OK  ] Stopped Wiren Board firmware update service.
[  OK  ] Stopped Access point and a…server for Wi-Fi and Ethernet.
[  OK  ] Stopped telegraf metric se…oard Cloud (wirenboard.cloud).
[  OK  ] Stopped Kernel 1-Wire MQTT driver for WB-HomA.
[  OK  ] Stopped Wiren Board Cloud Agent (wirenboard.cloud).
[  OK  ] Stopped User Runtime Directory /run/user/0.
[  OK  ] Stopped Initialize Wiren Board on successful boot.
[  OK  ] Stopped The PHP 7.4 FastCGI Process Manager.
[  OK  ] Removed slice system-getty.slice.
[  OK  ] Removed slice system-wb\x2dcloud\x2dagent.slice.
[  OK  ] Removed slice system-wb\x2…ud\x2dagent\x2dtelegraf.slice.
[  OK  ] Removed slice User Slice of UID 0.
         Stopping A high performanc… and a reverse proxy server...
         Stopping Network Time Service...
         Stopping OpenBSD Secure Shell server...
         Stopping Permit User Sessions...
[  OK  ] Stopped User Login Management.
[  OK  ] Stopped Network Tim[ 2589.200616] br-3af99fd9d4d7: port 1(vethec604cc)                                                                                       entered disabled state
e Service.
[ 2589.207971] vethfafef4c: renamed from eth0
[  OK  ] Stopped OpenBSD Secure Shell server.
[  OK  ] Stopped Permit User Sessions.
[  OK  ] Stopped A high performance…er and[ 2589.267465] br-3af99fd9d4d7: port 1                                                                                      (vethec604cc) entered disabled state
 a reverse proxy server.
[ 2589.277143] vethec604cc (unregistering): left allmulticast mode
[ 2589.283828] vethec604cc (unregistering): left promiscuous mode
[ 2589.289852] br-3af99fd9d4d7: port 1(vethec604cc) entered disabled state
[  OK  ] Stopped LSB: Brings up/down network automatically.
[  OK  ] Stopped target Remote File Systems.
[  OK  ] Unmounted /run/docker/netns/9de752634296.
[  OK  ] Unmounted /mnt/data/.docke…cad6fb070d2a536f488790/merged.
[  OK  ] Stopped MQTT Driver for ADC.
[  OK  ] Unmounted /mnt/data/.docke…e7f5271cb9abada9236b2e/merged.
[  OK  ] Stopped Wiren Board modbus devices manager.
         Stopping MQTT Driver for serial devices...
[  OK  ] Stopped MQTT Driver for GPIO-controlled switches.
[  OK  ] Stopped MQTT Driver for serial devices.
[  OK  ] Stopped metrics sender.
[  OK  ] Stopped Wiren Board MQTT KNX bridge.
         Stopping Mosquitto MQTT Broker...
[  OK  ] Stopped Mosquitto MQTT Broker.
[  OK  ] Unmounted /mnt/data/.docke…5678f947d11359308fd87a/merged.
[ 2598.319190] br-3af99fd9d4d7: port 2(veth8046ad3) entered disabled state
[ 2598.326127] veth9d75ce5: renamed from eth0
[ 2598.482156] br-3af99fd9d4d7: port 2(veth8046ad3) entered disabled state
[ 2598.490076] veth8046ad3 (unregistering): left allmulticast mode
[ 2598.496093] veth8046ad3 (unregistering): left promiscuous mode
[ 2598.501977] br-3af99fd9d4d7: port 2(veth8046ad3) entered disabled state
[  OK  ] Unmounted /run/docker/netns/945791f899a1.
[  OK  ] Unmounted /mnt/data/.docke…07a2c8ae6882dbac2f441c/merged.
[  OK  ] Stopped Docker Application Container Engine.
[  OK  ] Stopped target Network is Online.
[  OK  ] Stopped target Host and Network Name Lookups.
         Stopping containerd container runtime...
[  OK  ] Stopped KNX Daemon.
[  OK  ] Stopped containerd container runtime.
[  OK  ] Stopped target Network.
         Stopping Raise network interfaces...
         Stopping WPA supplicant...
[  OK  ] Stopped WPA supplicant.
         Stopping D-Bus System Message Bus...
[  OK  ] Stopped D-Bus System Message Bus.
[  OK  ] Stopped Raise network interfaces.
[  OK  ] Stopped Initialize Wiren Board Device Tree overlays.
         Stopping watch config files...
[  OK  ] Stopped watch config files.
[  OK  ] Stopped target Basic System.
[  OK  ] Stopped target Paths.
[  OK  ] Stopped target Slices.
[  OK  ] Removed slice User and Session Slice.
[  OK  ] Stopped target Sockets.
[  OK  ] Closed Avahi mDNS/DNS-SD Stack Activation Socket.
[  OK  ] Closed D-Bus System Message Bus Socket.
[  OK  ] Closed Docker Socket for the API.
[  OK  ] Closed fcgiwrap Socket.
[  OK  ] Closed KNXnet/IP socket.
[  OK  ] Closed KNX Daemon (socket).
[  OK  ] Stopped target System Initialization.
[  OK  ] Stopped target Local Encrypted Volumes.
[  OK  ] Stopped Dispatch Password …ts to Console Directory Watch.
[  OK  ] Stopped Forward Password R…uests to Wall Directory Watch.
[  OK  ] Stopped target Swap.
         Deactivating swap /dev/dis…mmc-MMC64G_0x6d673edd-part5...
[  OK  ] Stopped Apply Kernel Variables.
[  OK  ] Stopped Load Kernel Modules.
         Stopping Update UTMP about System Boot/Shutdown...
[  OK  ] Deactivated swap /dev/disk…7-1849-4bf1-8942-14d37e214a7d.
[  OK  ] Deactivated swap /dev/disk/by-partuuid/358bab35-05.
[  OK  ] Deactivated swap /dev/disk…th/platform-4022000.mmc-part5.
[  OK  ] Deactivated swap /dev/disk…d/mmc-MMC64G_0x6d673edd-part5.
[  OK  ] Deactivated swap /dev/mmcblk0p5.
[  OK  ] Stopped Update UTMP about System Boot/Shutdown.
[  OK  ] Stopped Create Volatile Files and Directories.
         Stopping Flush Journal to Persistent Storage...
         Stopping prepare mounts and symlinks to config files...
[ 2599.683564] systemd-journald[117]: Received client request to relinquish /var                                                                                      /log/journal/a79bfb4d25da4edfbf66fe79e5084323 access.
[  OK  ] Stopped prepare mounts and symlinks to config files.
[  OK  ] Stopped target Local File Systems.
[  OK  ] Unset automount mnt-sdcard.automount.
         Unmounting /run/docker/netns/default...
[  OK  ] Stopped Flush Journal to Persistent Storage.
[  OK  ] Unmounted /run/docker/netns/default.
         Unmounting /var/log...
[  OK  ] Unmounted /var/log.
         Unmounting /mnt/data...
[ 2600.497768] EXT4-fs (mmcblk0p6): unmounting filesystem 991b53c7-28c9-4ca5-a75                                                                                      9-c4d686cfc653.
[  OK  ] Unmounted /mnt/data.
[  OK  ] Reached target Unmount All Filesystems.
[  OK  ] Stopped File System Check on /dev/mmcblk0p6.
[  OK  ] Removed slice system-systemd\x2dfsck.slice.
[  OK  ] Stopped target Local File Systems (Pre).
[  OK  ] Stopped Create Static Device Nodes in /dev.
[  OK  ] Stopped Create System Users.
[  OK  ] Stopped Remount Root and Kernel File Systems.
[  OK  ] Stopped File System Check on Root Device.
[  OK  ] Reached target Shutdown.
[  OK  ] Reached target Final Step.
[  OK  ] Finished Power-Off.
[  OK  ] Reached target Power-Off.
[ 2600.977293] systemd-shutdown[1]: Syncing filesystems and block devices.
[ 2600.988505] systemd-shutdown[1]: Sending SIGTERM to remaining processes...
[ 2601.008698] systemd-journald[117]: Received SIGTERM from PID 1 (systemd-shutd                                                                                      ow).
[ 2601.027963] systemd-shutdown[1]: Sending SIGKILL to remaining processes...
[ 2601.051579] systemd-shutdown[1]: Unmounting file systems.
[ 2601.059626] [30523]: Remounting '/' read-only in with options 'discard,errors                                                                                      =remount-ro,stripe=1024'.
[ 2601.105264] EXT4-fs (mmcblk0p2): re-mounted 3b8e8efe-a6ab-4e65-9131-1a0af1c14                                                                                      0f6 ro. Quota mode: none.
[ 2601.124143] systemd-shutdown[1]: All filesystems unmounted.
[ 2601.129763] systemd-shutdown[1]: Deactivating swaps.
[ 2601.134922] systemd-shutdown[1]: All swaps deactivated.
[ 2601.140165] systemd-shutdown[1]: Detaching loop devices.
[ 2601.149082] systemd-shutdown[1]: All loop devices detached.
[ 2601.154680] systemd-shutdown[1]: Stopping MD devices.
[ 2601.160022] systemd-shutdown[1]: All MD devices stopped.
[ 2601.165361] systemd-shutdown[1]: Detaching DM devices.
[ 2601.170836] systemd-shutdown[1]: All DM devices detached.
[ 2601.176252] systemd-shutdown[1]: All filesystems, swaps, loop devices, MD dev                                                                                      ices and DM devices detached.
[ 2601.192922] systemd-shutdown[1]: Syncing filesystems and block devices.
[ 2601.199682] systemd-shutdown[1]: Powering off.
[ 2601.226491] RTW: stop cmd thread during rtw_dev_shutdown
[ 2601.257108] RTW: cmd thread is stopped during rtw_dev_shutdown
[ 2601.278381] kvm: exiting hardware virtualization
[ 2601.283018] reboot: Power down

[EC] Power off request from Linux.
[EC] Alarm: not set
[EC] Power status: powered from external supply
[EC] Powering off
[EC] 5V line status: voltage present
[EC] Power off and go to standby now▒

[EC] Starting up...

[EC] Wiren Board Embedded Controller
[EC] Firmware version: 1.3.1
[EC] Git info: 616f549_HEAD
[EC] Power on reason: Power button
[EC] RTC time: 2026-03-24 15:56:13
[EC] Board temperature: 42.2ºC
[EC] Vin: 12.2V, USB Net: 0.5V, USB Console: 5.1V
[EC] Turning on the main CPU; all future debug messages will originate from the                                                                                       CPU.

U-Boot SPL 2024.01-g93c03f11a3 (May 23 2024 - 08:58:29 +0000)
DRAM: 4096 MiB
Trying to boot from MMC2
NOTICE:  BL31: v2.10.0  (debug):v2.10.0+dfsg-1+wb1-1-g9db2f29f3
NOTICE:  BL31: Built : 13:16:33, Feb 29 2024
NOTICE:  BL31: Detected Allwinner H616 SoC (1823)
NOTICE:  BL31: Found U-Boot DTB at 0x4a07d108, model: Wiren Board 8.x
INFO:    ARM GICv2 driver initialized
INFO:    Configuring SPC Controller
INFO:    BL31: Platform setup done
INFO:    BL31: Initializing runtime services
INFO:    BL31: cortex_a53: CPU workaround for erratum 855873 was applied
INFO:    BL31: cortex_a53: CPU workaround for erratum 1530924 was applied
INFO:    PSCI: Suspend is unavailable
INFO:    BL31: Preparing for EL3 exit to normal world
INFO:    Entry point address = 0x4a000000
INFO:    SPSR = 0x3c9
INFO:    Changed devicetree.
ns16550_serial serial@5000000: pinctrl_select_state_full: uclass_get_device_by_p                                                                                      handle_id: err=-19

U-Boot 2024.01-g93c03f11a3 (May 23 2024 - 08:58:29 +0000) Allwinner Technology

CPU:   Allwinner H616 (SUN50I)
Model: Wiren Board 8.x
DRAM:  4 GiB
Core:  68 devices, 19 uclasses, devicetree: separate
WDT:   Not starting watchdog@30090a0
MMC:   mmc@4020000: 0, mmc@4022000: 1
Loading Environment from MMC... OK
In:    serial@5000000
Out:   serial@5000000
Err:   serial@5000000
Will only keep env vars: mmcpart bootcount upgrade_available uenvcmd wb_webupd o                                                                                      tp_program otp_aes_program
## Info: input data size = 43 = 0x2B
bootcount=0
mmcpart=2
upgrade_available=0

Environment size: 43/49148 bytes
## Resetting to default environment
## Info: input data size = 43 = 0x2B
Net:   No ethernet found.
Hit <SPACE> to stop autoboot... (2 s)
## Info: input data size = 4329 = 0x10E9
switch to partitions #0, OK
mmc1(part 0) is current device
eMMC found on device 1
Press FW button to enter firmware update mode
................................................
328 bytes read in 1 ms (320.3 KiB/s)
Importing environment from 0x40080000...
Checking if uenvcmd is set ...
Running default loadzimage ...
10096655 bytes read in 1845 ms (5.2 MiB/s)

MMC read: dev # 1, block # 2016, count 32 ... 32 blocks read: OK
Working FDT set to 4fe00000
Reading overlays list from eMMC
Reading factory fdt name from eMMC
Loading factory fdt allwinner/sun50i-h616-wirenboard843
51031 bytes read in 12 ms (4.1 MiB/s)
Working FDT set to 4fa00000
254 bytes read in 1 ms (248 KiB/s)
Applying DT overlay temp-industrial
Applying extra overlay
Booting from mmc ...
   Uncompressing Kernel Image
Moving Image from 0x40080000 to 0x40200000, end=41a50000
## Flattened Device Tree blob at 4fa00000
   Booting using the fdt blob at 0x4fa00000
Working FDT set to 4fa00000
   Loading Device Tree to 0000000049fdd000, end 0000000049ffffff ... OK
Working FDT set to 49fdd000

Starting kernel ...

[    0.000000] Booting Linux on physical CPU 0x0000000000 [0x410fd034]
[    0.000000] Linux version 6.8.0-wb153 (root@wbdevenv) (aarch64-linux-gnu-gcc                                                                                       (Debian 10.2.1-6) 10.2.1 20210110, GNU ld (GNU Binutils for Debian) 2.35.2) #1 S                                                                                      MP Wed Mar  4 13:38:44 UTC 2026
[    0.000000] KASLR disabled due to lack of seed
[    0.000000] Machine model: Wiren Board rev. 8.4.3 (T507)
[    0.000000] efi: UEFI not found.
[    0.000000] OF: reserved mem: 0x0000000040000000..0x000000004003ffff (256 KiB                                                                                      ) nomap non-reusable secmon@40000000
[    0.000000] NUMA: No NUMA configuration found
[    0.000000] NUMA: Faking a node at [mem 0x0000000040000000-0x000000013fffffff                                                                                      ]
[    0.000000] NUMA: NODE_DATA [mem 0x13f7af9c0-0x13f7b1fff]
[    0.000000] Zone ranges:
[    0.000000]   DMA      [mem 0x0000000040000000-0x00000000ffffffff]
[    0.000000]   DMA32    empty
[    0.000000]   Normal   [mem 0x0000000100000000-0x000000013fffffff]
[    0.000000] Movable zone start for each node
[    0.000000] Early memory node ranges
[    0.000000]   node   0: [mem 0x0000000040000000-0x000000004003ffff]
[    0.000000]   node   0: [mem 0x0000000040040000-0x000000013fffffff]
[    0.000000] Initmem setup node 0 [mem 0x0000000040000000-0x000000013fffffff]
[    0.000000] cma: Reserved 32 MiB at 0x00000000fe000000 on node -1
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: PSCIv1.1 detected in firmware.
[    0.000000] psci: Using standard PSCI v0.2 function IDs
[    0.000000] psci: MIGRATE_INFO_TYPE not supported.
[    0.000000] psci: SMC Calling Convention v1.4
[    0.000000] percpu: Embedded 22 pages/cpu s50152 r8192 d31768 u90112
[    0.000000] Detected VIPT I-cache on CPU0
[    0.000000] CPU features: detected: ARM erratum 845719
[    0.000000] alternatives: applying boot alternatives
[    0.000000] Kernel command line: console=ttyS0,115200 root=/dev/mmcblk0p2 roo                                                                                      twait ro
[    0.000000] Dentry cache hash table entries: 524288 (order: 10, 4194304 bytes                                                                                      , linear)
[    0.000000] Inode-cache hash table entries: 262144 (order: 9, 2097152 bytes,                                                                                       linear)
[    0.000000] Fallback order for Node 0: 0
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1032192
[    0.000000] Policy zone: Normal
[    0.000000] mem auto-init: stack:off, heap alloc:off, heap free:off
[    0.000000] software IO TLB: area num 4.
[    0.000000] software IO TLB: mapped [mem 0x00000000fa000000-0x00000000fe00000                                                                                      0] (64MB)
[    0.000000] Memory: 3989480K/4194304K available (14208K kernel code, 1468K rw                                                                                      data, 5188K rodata, 3328K init, 542K bss, 172056K reserved, 32768K cma-reserved)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] rcu: Hierarchical RCU implementation.
[    0.000000] rcu:     RCU event tracing is enabled.
[    0.000000] rcu:     RCU restricting CPUs from NR_CPUS=256 to nr_cpu_ids=4.
[    0.000000]  Tracing variant of Tasks RCU enabled.
[    0.000000] rcu: RCU calculated value of scheduler-enlistment delay is 25 jif                                                                                      fies.
[    0.000000] rcu: Adjusting geometry for rcu_fanout_leaf=16, nr_cpu_ids=4
[    0.000000] NR_IRQS: 64, nr_irqs: 64, preallocated irqs: 0
[    0.000000] Root IRQ handler: gic_handle_irq
[    0.000000] GIC: Using split EOI/Deactivate mode
[    0.000000] rcu: srcu_init: Setting srcu_struct sizes based on contention.
[    0.000000] arch_timer: cp15 timer(s) running at 24.00MHz (phys).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles:                                                                                       0x588fe9dc0, max_idle_ns: 440795202592 ns
[    0.000001] sched_clock: 56 bits at 24MHz, resolution 41ns, wraps every 43980                                                                                      46511097ns
[    0.000639] Console: colour dummy device 80x25
[    0.000725] Calibrating delay loop (skipped), value calculated using timer fr                                                                                      equency.. 48.00 BogoMIPS (lpj=96000)
[    0.000739] pid_max: default: 32768 minimum: 301
[    0.000817] LSM: initializing lsm=capability,integrity
[    0.000927] Mount-cache hash table entries: 8192 (order: 4, 65536 bytes, line                                                                                      ar)
[    0.000951] Mountpoint-cache hash table entries: 8192 (order: 4, 65536 bytes,                                                                                       linear)
[    0.001997] cacheinfo: Unable to detect cache hierarchy for CPU 0
[    0.002709] RCU Tasks Trace: Setting shift to 2 and lim to 1 rcu_task_cb_adju                                                                                      st=1.
[    0.002937] rcu: Hierarchical SRCU implementation.
[    0.002941] rcu:     Max phase no-delay instances is 1000.
[    0.003445] EFI services will not be available.
[    0.003686] smp: Bringing up secondary CPUs ...
[    0.004228] Detected VIPT I-cache on CPU1
[    0.004307] CPU1: Booted secondary processor 0x0000000001 [0x410fd034]
[    0.004830] Detected VIPT I-cache on CPU2
[    0.004877] CPU2: Booted secondary processor 0x0000000002 [0x410fd034]
[    0.005353] Detected VIPT I-cache on CPU3
[    0.005397] CPU3: Booted secondary processor 0x0000000003 [0x410fd034]
[    0.005469] smp: Brought up 1 node, 4 CPUs
[    0.005476] SMP: Total of 4 processors activated.
[    0.005479] CPU: All CPU(s) started at EL2
[    0.005504] CPU features: detected: 32-bit EL0 Support
[    0.005507] CPU features: detected: 32-bit EL1 Support
[    0.005513] CPU features: detected: CRC32 instructions
[    0.005554] alternatives: applying system-wide alternatives
[    0.008280] devtmpfs: initialized
[    0.017631] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, ma                                                                                      x_idle_ns: 7645041785100000 ns
[    0.017657] futex hash table entries: 1024 (order: 4, 65536 bytes, linear)
[    0.018992] pinctrl core: initialized pinctrl subsystem
[    0.019431] DMI not present or invalid.
[    0.020164] NET: Registered PF_NETLINK/PF_ROUTE protocol family
[    0.021039] DMA: preallocated 512 KiB GFP_KERNEL pool for atomic allocations
[    0.021169] DMA: preallocated 512 KiB GFP_KERNEL|GFP_DMA pool for atomic allo                                                                                      cations
[    0.021348] DMA: preallocated 512 KiB GFP_KERNEL|GFP_DMA32 pool for atomic al                                                                                      locations
[    0.021379] audit: initializing netlink subsys (disabled)
[    0.021511] audit: type=2000 audit(0.020:1): state=initialized audit_enabled=                                                                                      0 res=1
[    0.021930] thermal_sys: Registered thermal governor 'step_wise'
[    0.021935] thermal_sys: Registered thermal governor 'power_allocator'
[    0.021976] cpuidle: using governor menu
[    0.022116] hw-breakpoint: found 6 breakpoint and 4 watchpoint registers.
[    0.022196] ASID allocator initialised with 65536 entries
[    0.022384] Serial: AMBA PL011 UART driver
[    0.027318] platform 3001000.clock: Fixed dependency cycle(s) with /soc/rtc@7                                                                                      000000
[    0.031383] platform 6510000.tcon-top: Fixed dependency cycle(s) with /soc/lc                                                                                      d-controller@6515000
[    0.031401] platform 6510000.tcon-top: Fixed dependency cycle(s) with /soc/bu                                                                                      s@1000000/mixer@100000
[    0.031567] platform 6510000.tcon-top: Fixed dependency cycle(s) with /soc/lc                                                                                      d-controller@6515000
[    0.031630] platform 6515000.lcd-controller: Fixed dependency cycle(s) with /                                                                                      soc/tcon-top@6510000
[    0.031885] platform 3001000.clock: Fixed dependency cycle(s) with /soc/rtc@7                                                                                      000000
[    0.031941] platform 7000000.rtc: Fixed dependency cycle(s) with /soc/clock@3                                                                                      001000
[    0.031999] platform 7000000.rtc: Fixed dependency cycle(s) with /soc/clock@7                                                                                      010000
[    0.032109] platform 7000000.rtc: Fixed dependency cycle(s) with /soc/clock@7                                                                                      010000
[    0.032162] platform 7010000.clock: Fixed dependency cycle(s) with /soc/clock                                                                                      @3001000
[    0.032219] platform 7010000.clock: Fixed dependency cycle(s) with /soc/rtc@7                                                                                      000000
[    0.036882] Modules: 26544 pages in range for non-PLT usage
[    0.036887] Modules: 518064 pages in range for PLT usage
[    0.037685] HugeTLB: registered 1.00 GiB page size, pre-allocated 0 pages
[    0.037690] HugeTLB: 0 KiB vmemmap can be freed for a 1.00 GiB page
[    0.037696] HugeTLB: registered 32.0 MiB page size, pre-allocated 0 pages
[    0.037700] HugeTLB: 0 KiB vmemmap can be freed for a 32.0 MiB page
[    0.037705] HugeTLB: registered 2.00 MiB page size, pre-allocated 0 pages
[    0.037708] HugeTLB: 0 KiB vmemmap can be freed for a 2.00 MiB page
[    0.037713] HugeTLB: registered 64.0 KiB page size, pre-allocated 0 pages
[    0.037717] HugeTLB: 0 KiB vmemmap can be freed for a 64.0 KiB page
[    0.038976] ACPI: Interpreter disabled.
[    0.039582] iommu: Default domain type: Translated
[    0.039586] iommu: DMA domain TLB invalidation policy: strict mode
[    0.039939] SCSI subsystem initialized
[    0.040310] usbcore: registered new interface driver usbfs
[    0.040338] usbcore: registered new interface driver hub
[    0.040368] usbcore: registered new device driver usb
[    0.040742] pps_core: LinuxPPS API ver. 1 registered
[    0.040746] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giome                                                                                      tti <giometti@linux.it>
[    0.040759] PTP clock support registered
[    0.040794] EDAC MC: Ver: 3.0.0
[    0.041125] scmi_core: SCMI protocol bus registered
[    0.041426] FPGA manager framework
[    0.041518] Advanced Linux Sound Architecture Driver Initialized.
[    0.042515] clocksource: Switched to clocksource arch_sys_counter
[    0.042733] VFS: Disk quotas dquot_6.6.0
[    0.042765] VFS: Dquot-cache hash table entries: 512 (order 0, 4096 bytes)
[    0.042945] pnp: PnP ACPI: disabled
[    0.049782] NET: Registered PF_INET protocol family
[    0.050004] IP idents hash table entries: 65536 (order: 7, 524288 bytes, line                                                                                      ar)
[    0.053310] tcp_listen_portaddr_hash hash table entries: 2048 (order: 3, 3276                                                                                      8 bytes, linear)
[    0.053359] Table-perturb hash table entries: 65536 (order: 6, 262144 bytes,                                                                                       linear)
[    0.053373] TCP established hash table entries: 32768 (order: 6, 262144 bytes                                                                                      , linear)
[    0.053630] TCP bind hash table entries: 32768 (order: 8, 1048576 bytes, line                                                                                      ar)
[    0.054927] TCP: Hash tables configured (established 32768 bind 32768)
[    0.055038] UDP hash table entries: 2048 (order: 4, 65536 bytes, linear)
[    0.055130] UDP-Lite hash table entries: 2048 (order: 4, 65536 bytes, linear)
[    0.055310] NET: Registered PF_UNIX/PF_LOCAL protocol family
[    0.055754] RPC: Registered named UNIX socket transport module.
[    0.055759] RPC: Registered udp transport module.
[    0.055762] RPC: Registered tcp transport module.
[    0.055764] RPC: Registered tcp-with-tls transport module.
[    0.055767] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.056154] kvm [1]: IPA Size Limit: 40 bits
[    0.057564] kvm [1]: vgic interrupt IRQ9
[    0.057601] kvm [1]: Hyp mode initialized successfully
[    0.058858] Initialise system trusted keyrings
[    0.059013] workingset: timestamp_bits=42 max_order=20 bucket_order=0
[    0.059331] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.059542] NFS: Registering the id_resolver key type
[    0.059589] Key type id_resolver registered
[    0.059593] Key type id_legacy registered
[    0.059617] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
[    0.059623] nfs4flexfilelayout_init: NFSv4 Flexfile Layout Driver Registering                                                                                      ...
[    0.059739] 9p: Installing v9fs 9p2000 file system support
[    0.122638] Key type asymmetric registered
[    0.122643] Asymmetric key parser 'x509' registered
[    0.122686] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 2                                                                                      45)
[    0.122693] io scheduler mq-deadline registered
[    0.122697] io scheduler kyber registered
[    0.122729] io scheduler bfq registered
[    0.126156] EINJ: ACPI disabled.
[    0.136448] Serial: 8250/16550 driver, 6 ports, IRQ sharing enabled
[    0.147345] loop: module loaded
[    0.151920] tun: Universal TUN/TAP device driver, 1.6
[    0.153334] VFIO - User Level meta-driver version: 0.3
[    0.154765] usbcore: registered new interface driver usb-storage
[    0.154829] usbcore: registered new interface driver usbserial_generic
[    0.154852] usbserial: USB Serial support registered for generic
[    0.154874] usbcore: registered new interface driver ch341
[    0.154894] usbserial: USB Serial support registered for ch341-uart
[    0.157789] sun6i-rtc 7000000.rtc: registered as rtc1
[    0.158192] i2c_dev: i2c /dev entries driver
[    0.158451] mv64xxx_i2c 7081400.i2c: can't get pinctrl, bus recovery not supp                                                                                      orted
[    0.159106] axp20x-i2c 0-0036: AXP20x variant AXP15060 found
[    0.159360] axp20x-i2c 0-0036: AXP20X driver loaded
[    0.162296] sdhci: Secure Digital Host Controller Interface driver
[    0.162301] sdhci: Copyright(c) Pierre Ossman
[    0.162684] Synopsys Designware Multimedia Card Interface Driver
[    0.163483] sdhci-pltfm: SDHCI platform and OF driver helper
[    0.164581] ledtrig-cpu: registered to indicate activity on CPUs
[    0.165045] SMCCC: SOC_ID: ID = jep106:091e:1823 Revision = 0x00000002
[    0.165460] usbcore: registered new interface driver usbhid
[    0.165465] usbhid: USB HID core driver
[    0.167120] hw perfevents: enabled with armv8_cortex_a53 PMU driver, 7 counte                                                                                      rs available
[    0.169462] usbcore: registered new interface driver snd-usb-audio
[    0.170379] NET: Registered PF_PACKET protocol family
[    0.170384] can: controller area network core
[    0.170425] NET: Registered PF_CAN protocol family
[    0.170717] 9pnet: Installing 9P2000 support
[    0.170775] Key type dns_resolver registered
[    0.180220] registered taskstats version 1
[    0.180385] Loading compiled-in X.509 certificates
[    0.199898] gpio gpiochip0: Static allocation of GPIO base is deprecated, use                                                                                       dynamic allocation.
[    0.207697] sun50i-h616-pinctrl 300b000.pinctrl: initialized sunXi PIO driver
[    0.208383] gpio gpiochip1: Static allocation of GPIO base is deprecated, use                                                                                       dynamic allocation.
[    0.208647] sun50i-h616-r-pinctrl 7022000.pinctrl: initialized sunXi PIO driv                                                                                      er
[    0.209392] sun50i-h616-pinctrl 300b000.pinctrl: supply vcc-ph not found, usi                                                                                      ng dummy regulator
[    0.209881] printk: legacy console [ttyS0] disabled
[    0.230468] dw-apb-uart 5000000.serial: detected caps 00000100 should be 0004                                                                                      0100
[    0.230479] 5000000.serial: ttyS0 at MMIO 0x5000000 (irq = 284, base_baud = 1                                                                                      500000) is a 16550A
[    0.230530] printk: legacy console [ttyS0] enabled
[    1.477516] dw-apb-uart 5000400.serial: detected caps 00000100 should be 0004                                                                                      0100
[    1.485003] 5000400.serial: ttyS1 at MMIO 0x5000400 (irq = 285, base_baud = 1                                                                                      500000) is a 16550A
[    1.515053] dw-apb-uart 5000800.serial: detected caps 00000100 should be 0004                                                                                      0100
[    1.522538] 5000800.serial: ttyS2 at MMIO 0x5000800 (irq = 286, base_baud = 1                                                                                      500000) is a 16550A
[    1.532117] sun6i-spi 5011000.spi: Failed to request TX DMA channel
[    1.538395] sun6i-spi 5011000.spi: Failed to request RX DMA channel
[    1.545334] wbec spi0.0: WBEC not found with v2 protocol, trying v1
[    1.551742] wbec spi0.0: WBEC found with v1 protocol
[    1.557873] input: wbec pwrkey as /devices/platform/soc/5011000.spi/spi_maste                                                                                      r/spi0/spi0.0/5011000.spi:wbec@0:wbec-pwrkey@0/input/input0
[    1.571513] wbec-rtc 5011000.spi:wbec@0:wbec-rtc@0: registered as rtc0
[    1.578193] wbec-rtc 5011000.spi:wbec@0:wbec-rtc@0: setting system clock to 2                                                                                      026-03-24T15:56:25 UTC (1774367785)
[    1.590660] wbec spi0.0: WBEC device added
[    1.598820] i2c i2c-1: using pinctrl states for GPIO recovery
[    1.604752] gpio-10 (scl): enforced open drain please flag it properly in DT/                                                                                      ACPI DSDT/board file
[    1.613638] i2c i2c-1: using generic GPIOs for recovery
[    1.625238] iio-rescale vin-volt: using raw+scale/offset source channel
[    1.632197] iio-rescale v33-volt: using raw+scale/offset source channel
[    1.639082] iio-rescale v50-volt: using raw+scale/offset source channel
[    1.645946] iio-rescale vbus-debug-volt: using raw+scale/offset source channe                                                                                      l
[    1.650518] sunxi-mmc 4022000.mmc: initialized, max. request size: 2048 KB, u                                                                                      ses new timings mode
[    1.653419] iio-rescale vbus-network-volt: using raw+scale/offset source chan                                                                                      nel
[    1.669653] iio-rescale a1-volt: using raw+scale/offset source channel
[    1.676429] iio-rescale a2-volt: using raw+scale/offset source channel
[    1.683201] iio-rescale a3-volt: using raw+scale/offset source channel
[    1.689975] iio-rescale a4-volt: using raw+scale/offset source channel
[    1.697477] gpio-109 (sda): enforced open drain please flag it properly in DT                                                                                      /ACPI DSDT/board file
[    1.704438] mmc0: new HS200 MMC card at address 0001
[    1.706876] axp20x-i2c 3-0034: AXP20x variant AXP221 found
[    1.711966] mmcblk0: mmc0:0001 MMC64G 58.2 GiB
[    1.717380] axp20x-adc axp22x-adc: DMA mask not set
[    1.723393]  mmcblk0: p1 p2 p3 p4 < p5 p6 >
[    1.731266] mmcblk0boot0: mmc0:0001 MMC64G 4.00 MiB
[    1.731378] axp20x-battery-power-supply axp20x-battery-power-supply: DMA mask                                                                                       not set
[    1.737231] mmcblk0boot1: mmc0:0001 MMC64G 4.00 MiB
[    1.749714] mmcblk0rpmb: mmc0:0001 MMC64G 4.00 MiB, chardev (240:0)
[    1.755254] axp20x-i2c 3-0034: AXP20X driver loaded
[    1.760911] i2c i2c-3: Not I2C compliant: can't read SCL
[    1.766224] i2c i2c-3: Bus may be unreliable
[    1.770493] i2c-gpio i2c_wbmz: using lines 109 (SDA) and 76 (SCL, no clock st                                                                                      retching)
[    1.778528] gpio-147 (sda): enforced open drain please flag it properly in DT                                                                                      /ACPI DSDT/board file
[    1.787500] gpio-128 (scl): enforced open drain please flag it properly in DT                                                                                      /ACPI DSDT/board file
[    1.796631] i2c-gpio i2c_atecc_rtc: using lines 147 (SDA) and 128 (SCL)
[    1.862524] mdio_bus gpio-0: ethernet-phy has invalid PHY address
[    1.868620] mdio_bus gpio-0: scan phy ethernet-phy at address 0
[    1.934610] mdio_bus gpio-1: ethernet-phy has invalid PHY address
[    1.940725] mdio_bus gpio-1: scan phy ethernet-phy at address 0
[    1.947800] sun4i-usb-phy 5100400.phy: phy0 dr_mode=3
[    1.956794] ehci-platform 5101000.usb: EHCI Host Controller
[    1.957626] ehci-platform 5200000.usb: EHCI Host Controller
[    1.958893] ehci-platform 5310000.usb: EHCI Host Controller
[    1.958929] ehci-platform 5310000.usb: new USB bus registered, assigned bus n                                                                                      umber 1
[    1.959125] ehci-platform 5310000.usb: irq 293, io mem 0x05310000
[    1.960568] ohci-platform 5101400.usb: Generic Platform OHCI controller
[    1.960599] ohci-platform 5101400.usb: new USB bus registered, assigned bus n                                                                                      umber 2
[    1.960744] ohci-platform 5101400.usb: irq 294, io mem 0x05101400
[    1.961012] usb_phy_generic usb_phy_generic.1.auto: dummy supplies not allowe                                                                                      d for exclusive requests
[    1.961796] ohci-platform 5200400.usb: Generic Platform OHCI controller
[    1.961839] ohci-platform 5200400.usb: new USB bus registered, assigned bus n                                                                                      umber 3
[    1.961967] ohci-platform 5200400.usb: irq 296, io mem 0x05200400
[    1.962439] ehci-platform 5101000.usb: new USB bus registered, assigned bus n                                                                                      umber 4
[    1.965422] ohci-platform 5310400.usb: Generic Platform OHCI controller
[    1.965433] ohci-platform 5310400.usb: new USB bus registered, assigned bus n                                                                                      umber 5
[    1.965524] ohci-platform 5310400.usb: irq 297, io mem 0x05310400
[    1.968003] ehci-platform 5200000.usb: new USB bus registered, assigned bus n                                                                                      umber 6
[    1.973619] ehci-platform 5101000.usb: irq 291, io mem 0x05101000
[    1.974514] ehci-platform 5310000.usb: USB 2.0 started, EHCI 1.00
[    1.975085] hub 1-0:1.0: USB hub found
[    1.975113] hub 1-0:1.0: 1 port detected
[    1.975802] sun50i-h616-pinctrl 300b000.pinctrl: supply vcc-pf not found, usi                                                                                      ng dummy regulator
[    1.976613] sunxi-mmc 4020000.mmc: Got CD GPIO
[    1.981366] ehci-platform 5200000.usb: irq 292, io mem 0x05200000
[    1.987759] of_cfs_init
[    2.002516] ehci-platform 5101000.usb: USB 2.0 started, EHCI 1.00
[    2.006639] sunxi-mmc 4020000.mmc: initialized, max. request size: 16384 KB,                                                                                       uses new timings mode
[    2.007898] of_cfs_init: OK
[    2.017558] hub 4-0:1.0: USB hub found
[    2.024104] clk: Disabling unused clocks
[    2.026518] ehci-platform 5200000.usb: USB 2.0 started, EHCI 1.00
[    2.031413] hub 4-0:1.0: 1 port detected
[    2.037600] ALSA device list:
[    2.045808] hub 3-0:1.0: USB hub found
[    2.051827]   No soundcards found.
[    2.160539] hub 3-0:1.0: 1 port detected
[    2.165089] hub 2-0:1.0: USB hub found
[    2.168867] hub 2-0:1.0: 1 port detected
[    2.173386] hub 6-0:1.0: USB hub found
[    2.177162] hub 6-0:1.0: 1 port detected
[    2.181681] hub 5-0:1.0: USB hub found
[    2.185454] hub 5-0:1.0: 1 port detected
[    2.197705] EXT4-fs (mmcblk0p2): mounted filesystem 3b8e8efe-a6ab-4e65-9131-1                                                                                      a0af1c140f6 ro with ordered data mode. Quota mode: none.
[    2.209767] VFS: Mounted root (ext4 filesystem) readonly on device 179:2.
[    2.218693] devtmpfs: mounted
[    2.222761] Freeing unused kernel memory: 3328K
[    2.227364] Run /sbin/init as init process
[    2.438565] usb 6-1: new high-speed USB device number 2 using ehci-platform
[    2.446406] NET: Registered PF_INET6 protocol family
[    2.452158] Segment Routing with IPv6
[    2.455861] In-situ OAM (IOAM) with IPv6
[    2.484645] systemd[1]: systemd 247.3-7+deb11u7 running in system mode. (+PAM                                                                                       +AUDIT +SELINUX +IMA +APPARMOR +SMACK +SYSVINIT +UTMP +LIBCRYPTSETUP +GCRYPT +G                                                                                      NUTLS +ACL +XZ +LZ4 +ZSTD +SECCOMP +BLKID +ELFUTILS +KMOD +IDN2 -IDN +PCRE2 defa                                                                                      ult-hierarchy=unified)
[    2.508280] systemd[1]: Detected architecture arm64.

Welcome to Debian GNU/Linux 11 (bullseye)!

[    2.531140] systemd[1]: Set hostname to <wirenboard-AIBYLRXZ>.
[    3.013105] systemd[1]: Queued start job for default target Graphical Interfa                                                                                      ce.
[    5.378519] random: crng init done
[    5.402995] systemd[1]: Created slice system-getty.slice.
[  OK  ] Created slice system-getty.slice.
[    5.428174] systemd[1]: Created slice system-modprobe.slice.
[  OK  ] Created slice system-modprobe.slice.
[    5.452128] systemd[1]: Created slice system-serial\x2dgetty.slice.
[  OK  ] Created slice system-serial\x2dgetty.slice.
[    5.476450] systemd[1]: Created slice system-systemd\x2dfsck.slice.
[  OK  ] Created slice system-systemd\x2dfsck.slice.
[    5.499646] systemd[1]: Created slice system-wb\x2dcloud\x2dagent.slice.
[  OK  ] Created slice system-wb\x2dcloud\x2dagent.slice.
[    5.524488] systemd[1]: Created slice system-wb\x2dcloud\x2dagent\x2dfrpc.sli                                                                                      ce.
[  OK  ] Created slice system-wb\x2dcloud\x2dagent\x2dfrpc.slice.
[    5.552560] systemd[1]: Created slice system-wb\x2dcloud\x2dagent\x2dtelegraf                                                                                      .slice.
[  OK  ] Created slice system-wb\x2…ud\x2dagent\x2dtelegraf.slice.
[    5.580906] systemd[1]: Created slice User and Session Slice.
[  OK  ] Created slice User and Session Slice.
[    5.603419] systemd[1]: Started Dispatch Password Requests to Console Directo                                                                                      ry Watch.
[  OK  ] Started Dispatch Password …ts to Console Directory Watch.
[    5.631302] systemd[1]: Started Forward Password Requests to Wall Directory W                                                                                      atch.
[  OK  ] Started Forward Password R…uests to Wall Directory Watch.
[    5.655298] systemd[1]: Condition check resulted in Arbitrary Executable File                                                                                       Formats File System Automount Point being skipped.
[    5.667429] systemd[1]: Reached target Local Encrypted Volumes.
[  OK  ] Reached target Local Encrypted Volumes.
[    5.691415] systemd[1]: Reached target Paths.
[  OK  ] Reached target Paths.
[    5.711000] systemd[1]: Reached target Remote File Systems.
[  OK  ] Reached target Remote File Systems.
[    5.730853] systemd[1]: Reached target Slices.
[  OK  ] Reached target Slices.
[    5.752766] systemd[1]: Listening on fsck to fsckd communication Socket.
[  OK  ] Listening on fsck to fsckd communication Socket.
[    5.779381] systemd[1]: Listening on initctl Compatibility Named Pipe.
[  OK  ] Listening on initctl Compatibility Named Pipe.
[    5.804709] systemd[1]: Listening on Journal Audit Socket.
[  OK  ] Listening on Journal Audit Socket.
[    5.828128] systemd[1]: Listening on Journal Socket (/dev/log).
[  OK  ] Listening on Journal Socket (/dev/log).
[    5.852099] systemd[1]: Listening on Journal Socket.
[  OK  ] Listening on Journal Socket.
[    5.872344] systemd[1]: Listening on udev Control Socket.
[  OK  ] Listening on udev Control Socket.
[    5.895743] systemd[1]: Listening on udev Kernel Socket.
[  OK  ] Listening on udev Kernel Socket.
[    5.943008] systemd[1]: Mounting Huge Pages File System...
         Mounting Huge Pages File System...
[    5.972265] systemd[1]: Mounting POSIX Message Queue File System...
         Mounting POSIX Message Queue File System...
[    6.000832] systemd[1]: Mounting /sys/kernel/config...
         Mounting /sys/kernel/config...
[    6.022649] systemd[1]: Mounting Kernel Debug File System...
         Mounting Kernel Debug File System...
[    6.043520] systemd[1]: Condition check resulted in Kernel Trace File System                                                                                       being skipped.
[    6.083162] systemd[1]: Starting Create list of static device nodes for the c                                                                                      urrent kernel...
         Starting Create list of st…odes for the current kernel...
[    6.117057] systemd[1]: Starting Load Kernel Module drm...
         Starting Load Kernel Module drm...
[    6.145242] systemd[1]: Starting Load Kernel Module fuse...
         Starting Load Kernel Module fuse...
[    6.164219] fuse: init (API version 7.39)
[    6.169961] systemd[1]: Condition check resulted in Set Up Additional Binary                                                                                       Formats being skipped.
[    6.185808] systemd[1]: Starting File System Check on Root Device...
         Starting File System Check on Root Device...
[    6.214309] systemd[1]: Starting Journal Service...
         Starting Journal Service...
[    6.225941] systemd[1]: Starting Load Kernel Modules...
         Starting Load Kernel Modules...
[    6.236032] systemd[1]: Starting Coldplug All udev Devices...
         Starting Coldplug All udev Devices...
[    6.249740] systemd[1]: Mounted Huge Pages File System.
[  OK      6.255830] systemd[1]: Mounted POSIX Message Queue File System.
0m] Mounted     6.263707] systemd[1]: Mounted /sys/kernel/config.
1;39mHuge Pages [    6.269779] systemd[1]: Mounted Kernel Debug File System.
File System.
[  OK  [    6.277460] systemd[1]: Finished Create list of static device nodes fo                                                                                      r the current kernel.
] Mounted POSIX Mes[    6.288156] systemd[1]: modprobe@drm.service: Succeeded.
sage Queue File [    6.295945] systemd[1]: Finished Load Kernel Module drm.
System.
[  OK  ] Mounted /sys/kernel/config.
[  OK  ] Mounted Kernel Debug File System.
[  OK  ] Finished Create list of st… nodes for the current kernel.
[  OK  ] Finished Load Kernel Module drm.
[    6.347803] systemd[1]: modprobe@fuse.service: Succeeded.
[    6.354146] systemd[1]: Finished Load Kernel Module fuse.
[  OK  ] Finished Load Kernel Module fuse.
[    6.375278] systemd[1]: Started Journal Service.
[  OK  ] Started Journal Service.
[  OK  ] Finished File System Check on Root Device.
[  OK  ] Finished Load Kernel Modules.
         Mounting FUSE Control File System...
[  OK  ] Started File System Check Daemon to report status.
         Starting Remount Root and Kernel File Systems...
         Starting Apply Kernel Variables...
[  OK  ] Mounted FUSE Control File System.
[  OK  ] Finished Apply Kernel Variables.
[    6.601830] EXT4-fs (mmcblk0p2): re-mounted 3b8e8efe-a6ab-4e65-9131-1a0af1c14                                                                                      0f6 r/w. Quota mode: none.
[  OK  ] Finished Remount Root and Kernel File Systems.
         Starting Load/Save Random Seed...
         Starting Create System Users...
[  OK  ] Finished Load/Save Random Seed.
[  OK  ] Finished Create System Users.
         Starting Create Static Device Nodes in /dev...
[  OK  ] Finished Coldplug All udev Devices.
         Starting Helper to synchronize boot up for ifupdown...
[  OK  ] Finished Create Static Device Nodes in /dev.
[  OK  ] Finished Helper to synchronize boot up for ifupdown.
[  OK  ] Reached target Local File Systems (Pre).
[  OK  ] Set up automount mnt-sdcard.automount.
         Starting Rule-based Manage…for Device Events and Files...
[  OK  ] Started Rule-based Manager for Device Events and Files.
[    7.181900] Driver for 1-wire Dallas network protocol.
[  OK  ] Found device /dev/ttyS0.
[    7.294042] dwmac-sun8i 5020000.ethernet: IRQ eth_wake_irq not found
[    7.300462] dwmac-sun8i 5020000.ethernet: IRQ eth_lpi not found
[    7.306556] dwmac-sun8i 5020000.ethernet: No regulator found
[    7.312418] dwmac-sun8i 5020000.ethernet: PTP uses main clock
[    7.312927] sunxi-wdt 30090a0.watchdog: Watchdog enabled (timeout=16 sec, now                                                                                      ayout=0)
[    7.318242] dwmac-sun8i 5020000.ethernet: Current syscon value is not the def                                                                                      ault 58000 (expect 0)
[    7.335534] dwmac-sun8i 5020000.ethernet: No HW DMA feature register supporte                                                                                      d
[    7.342834] dwmac-sun8i 5020000.ethernet: RX Checksum Offload Engine supporte                                                                                      d
[    7.350079] dwmac-sun8i 5020000.ethernet: COE Type 2
[    7.355062] dwmac-sun8i 5020000.ethernet: TX Checksum insertion supported
[    7.361900] dwmac-sun8i 5020000.ethernet: Normal descriptors
[    7.367596] dwmac-sun8i 5020000.ethernet: Chain mode enabled
[  OK  ] Reached target Hardware activated USB gadget.
[  OK  ] Found device /dev/mmcblk0p5.
[  OK  ] Found device /dev/mmcblk0p6.
[    7.569732] Bluetooth: Core ver 2.22
[    7.575057] NET: Registered PF_BLUETOOTH protocol family
[    7.580441] Bluetooth: HCI device and connection manager initialized
[    7.586860] Bluetooth: HCI socket layer initialized
[    7.591778] Bluetooth: L2CAP socket layer initialized
[    7.596890] Bluetooth: SCO socket layer initialized
[    7.614084] cfg80211: Loading compiled-in X.509 certificates for regulatory d                                                                                      atabase
[    7.619607] dwmac-sun8i 5030000.ethernet: IRQ eth_wake_irq not found
[    7.628292] dwmac-sun8i 5030000.ethernet: IRQ eth_lpi not found
[    7.634396] dwmac-sun8i 5030000.ethernet: No regulator found
[    7.640342] dwmac-sun8i 5030000.ethernet: PTP uses main clock
[    7.646198] dwmac-sun8i 5030000.ethernet: Current syscon value is not the def                                                                                      ault 58000 (expect 0)
         Activat[    7.655666] dwmac-sun8i 5030000.ethernet: No HW DMA feature r                                                                                      egister supported
ing swap     7.664117] dwmac-sun8i 5030000.ethernet: RX Checksum Offload Engine                                                                                       supported
9m/dev/mmcblk0p5[    7.666590] Loaded X.509 cert 'sforshee: 00b28ddf47aef9cea7'
...
[    7.672699] dwmac-sun8i 5030000.ethernet: COE Type 2
[    7.681784] Loaded X.509 cert 'wens: 61c038651aabdcf94bd0ac7ff06c7248db18c600                                                                                      '
[    7.685469] dwmac-sun8i 5030000.ethernet: TX Checksum insertion supported
[    7.685476] dwmac-sun8i 5030000.ethernet: Normal descriptors
[    7.705164] dwmac-sun8i 5030000.ethernet: Chain mode enabled
         Starting File System Check on /dev/mmcblk0p6...
[    7.801011] Adding 262140k swap on /dev/mmcblk0p5.  Priority:-2 extents:1 acr                                                                                      oss:262140k SSDsc
[    7.801086] usbcore: registered new interface driver btusb
[    7.820314] Bluetooth: hci0: RTL: examining hci_ver=08 hci_rev=000f lmp_ver=0                                                                                      8 lmp_subver=8723
[    7.822444] RTW: rtl8733bu v5.15.12-126-gb999e6008.20240911_COEX20230616-330e
[    7.835250] Bluetooth: hci0: RTL: rom_version status=0 version=2
[    7.836277] RTW: rtl8733bu BT-Coex version = COEX20230616-330e
[    7.842272] Bluetooth: hci0: RTL: loading rtl_bt/rtl8723fu_fw.bin
[  OK  ] Activated sw[    7.855974] Bluetooth: hci0: RTL: loading rtl_bt/rtl8723                                                                                      fu_config.bin
ap /dev[    7.861161] RTW: [HALMAC]138
[    7.861161] HALMAC_MAJOR_VER = 1
[    7.861161] HALMAC_PROTOTYPE_VER = 6
[    7.861161] HALMAC_MINOR_VER = 6
[    7.861161] HALMAC_PATCH_VER = 42
[    7.864743] Bluetooth: hci0: RTL: cfg_sz 14, total sz 45619

[  OK  ] Finished File System Check on /dev/mmcblk0p6.
[  OK  ] Reached target Swap.
[  OK  ] Listening on Load/Save RF …itch Status /dev/rfkill Watch.
         Mounting /mnt/data...
         Starting Load/Save RF Kill Switch Status...
[    8.035625] EXT4-fs (mmcblk0p6): mounted filesystem 991b53c7-28c9-4ca5-a759-c                                                                                      4d686cfc653 r/w with ordered data mode. Quota mode: none.
[  OK  ] Started Load/Save RF Kill Switch Status.
[  OK  ] Mounted /mnt/data.
         Mounting /var/log...
[  OK  ] Mounted /var/log.
[  OK  ] Reached target Local File Systems.
[    8.174996] RTW: rtw_rfctl_decide_init_chplan chplan:0x7F
         Starting Flush[    8.184143] RTW: rtw_set_country_cmd country_code:"KZ"
 Journal to Pers[    8.189690] RTW: default domain:0x5e applied, txpwr_lmt:?ETSI
istent Storage    8.196811] RTW: world wide applied, txpwr_lmt:WW
0m...
[    8.204103] RTW: rtw_ndev_init(wlan0) if1 mac_addr=98:03:cf:e9:f1:25
[    8.211615] RTW: rtw_ndev_init(wlan1) if2 mac_addr=9a:03:cf:e9:f1:25
[    8.219000] usbcore: registered new interface driver rtl8733bu
[    8.222770] systemd-journald[117]: Received client request to flush runtime j                                                                                      ournal.
         Starting prepare mounts and symlinks to config files...
[    8.316163] Bluetooth: hci0: RTL: fw version 0xd9d73187
[  OK  ] Finished Flush Journal to Persistent Storage.
[  OK  ] Finished prepare mounts and symlinks to config files.
         Starting Create Volatile Files and Directories...
[  OK  ] Finished Create Volatile Files and Directories.
         Starting Update UTMP about System Boot/Shutdown...
[  OK  ] Finished Update UTMP about System Boot/Shutdown.
[  OK  ] Reached target System Initialization.
[  OK  ] Started Daily apt download activities.
[  OK  ] Started Daily apt upgrade and clean activities.
[  OK  ] Started Periodic ext4 Onli…ata Check for All Filesystems.
[  OK  ] Started Discard unused blocks once a week.
[  OK  ] Started Daily rotation of log files.
[  OK  ] Started Clean PHP session files every 30 mins.
[  OK  ] Started Daily Cleanup of Temporary Directories.
[  OK  ] Reached target Timers.
[  OK  ] Listening on Avahi mDNS/DNS-SD Stack Activation Socket.
[  OK  ] Listening on D-Bus System Message Bus Socket.
         Starting Docker Socket for the API.
[  OK  ] Listening on fcgiwrap Socket.
         Starting KNXnet/IP socket.
[  OK  ] Listening on KNX Daemon (socket).
[  OK  ] Listening on Docker Socket for the API.
[  OK  ] Listening on KNXnet/IP socket.
[  OK  ] Reached target Sockets.
[  OK  ] Reached target Basic System.
         Starting Bluetooth service...
[  OK  ] Started Regular background program processing daemon.
[  OK  ] Started D-Bus System Message Bus.
         Starting Remove Stale Onli…t4 Metadata Check Snapshots...
         Starting User Login Management...
         Starting fast reverse prox…rd Cloud (wirenboard.cloud)...
[    9.660407] Bluetooth: BNEP (Ethernet Emulation) ver 1.3
[    9.665765] Bluetooth: BNEP filters: protocol multicast
[    9.671018] Bluetooth: BNEP socket layer initialized
         Starting telegraf metric s…rd Cloud (wirenbo[    9.684585] Bluetooth: M                                                                                      GMT ver 1.22
ard.cloud)...
[    9.697755] NET: Registered PF_ALG protocol family
[  OK  ] Started watch config files.
         Starting Initialize Wiren Board Device Tree overlays...
         Starting Avahi mDNS/DNS-SD Stack...
         Starting WPA supplicant...
[  OK  ] Finished Remove Stale Onli…ext4 Metadata Check Snapshots.
[  OK  ] Started fast reverse proxy…oard Cloud (wirenboard.cloud).
[  OK  ] Started telegraf metric se…oard Cloud (wirenboard.cloud).
[  OK  ] Started User Login Management.
[  OK  ] Started Avahi mDNS/DNS-SD Stack.
[  OK  ] Started WPA supplicant.
[  OK  ] Started Bluetooth service.
[  OK  ] Reached target Bluetooth.
         Starting Hostname Service...
[  OK  ] Started Hostname Service.
[  OK  ] Finished Initialize Wiren Board Device Tree overlays.
         Starting Raise network interfaces...
         Starting Power on GSM modem...
         Starting KNXD Configurator for Wiren Board...
[  OK  ] Finished Raise network interfaces.
[  OK  ] Reached target Network.
         Starting containerd container runtime...
         Starting dnsmasq - A light…DHCP and caching DNS server...
         Starting Access point and …rver for Wi-Fi and Ethernet...
         Starting KNX Daemon...
         Starting Mosquitto MQTT Broker...
         Starting Network Time Service...
         Starting The PHP 7.4 FastCGI Process Manager...
         Starting OpenBSD Secure Shell server...
         Starting Permit User Sessions...
         Starting MQTT Driver for ADC...
         Starting MQTT Driver for GPIO-controlled switches...
         Starting MQTT Driver for serial devices...
[  OK  ] Started Kernel 1-Wire MQTT driver for WB-HomA.
[  OK  ] Started KNX Daemon.
[  OK  ] Started Network Time Service.
[  OK  ] Finished Permit User Sessions.
[  OK  ] Started MQTT Driver for serial devices.
[  OK  ] Reached target Network is Online.
[  OK  ] Started Getty on tty1.
         Starting LSB: Brings up/down network automatically...
[  OK  ] Started Serial Getty on ttyS0.
[  OK  ] Reached target Login Prompts.
[   15.061414] process '/usr/sbin/netplugd' started with executable stack
[  OK  ] Started MQTT Driver for GPIO-controlled switches.
[  OK  ] Stopped KNX Daemon.
         Starting KNX Daemon...
[  OK  ] Started The PHP 7.4 FastCGI Process Manager.
[   15.932810] RTW: start_addr=(0x0), end_addr=(0x20000), buffer_size=(0x20000),                                                                                       smp_number_max=(16384)
[   16.018936] dwmac-sun8i 5020000.ethernet eth0: Register MEM_TYPE_PAGE_POOL Rx                                                                                      Q-0
[   16.028769] dwmac-sun8i 5020000.ethernet eth0: PHY [gpio-0:00] driver [Generi                                                                                      c PHY] (irq=POLL)
[   16.037561] dwmac-sun8i 5020000.ethernet eth0: No Safety Features support fou                                                                                      nd
[   16.044951] dwmac-sun8i 5020000.ethernet eth0: No MAC Management Counters ava                                                                                      ilable
[   16.052713] dwmac-sun8i 5020000.ethernet eth0: PTP not supported by HW
[  OK  ] Started OpenBSD Secure Shell server.
[   16.072006] dwmac-sun8i 5020000.ethernet eth0: configuring for phy/rmii link                                                                                       mode
[  OK  ] Started KNX Daemon.
[   16.091360] dwmac-sun8i 5030000.ethernet eth1: Register MEM_TYPE_PAGE_POOL Rx                                                                                      Q-0
[   16.101040] dwmac-sun8i 5030000.ethernet eth1: PHY [gpio-1:00] driver [Generi                                                                                      c PHY] (irq=POLL)
[   16.109867] dwmac-sun8i 5030000.ethernet eth1: No Safety Features support fou                                                                                      nd
[   16.117311] dwmac-sun8i 5030000.ethernet eth1: No MAC Management Counters ava                                                                                      ilable
[   16.125167] dwmac-sun8i 5030000.ethernet eth1: PTP not supported by HW
[   16.127746] dwmac-sun8i 5030000.ethernet eth1: configuring for phy/rmii link                                                                                       mode
[FAILED] Failed to start dnsmasq - …t DHCP and caching DNS server.
See 'systemctl status dnsmasq.service' for details.
[  OK  ] Started Mosquitto MQTT Broker.
[  OK  ] Started containerd container runtime.
[  OK  ] Finished KNXD Configurator for Wiren Board.
[  OK  ] Reached target Host and Network Name Lookups.
         Starting Docker Application Container Engine...
         Starting A high performanc… and a reverse proxy server...
         Starting Wiren Board Cloud Agent (wirenboard.cloud)...
[  OK  ] Started Wiren Board modbus devices manager.
[  OK  ] Started one-click diagnost… generating archive with data.
[  OK  ] Started Wiren Board configuration editor backend.
[  OK  ] Started Wiren Board database logger.
         Starting Wiren Board MQTT to IEC 60870-5-104 gateway...
[  OK  ] Started Wiren Board MQTT KNX bridge.
[  OK  ] Started Wiren Board journald to MQTT gateway.
[  OK  ] Started metrics sender.
         Starting Wiren Board MQTT to OPC UA gateway...
[  OK  ] Started MQTT Rule engine for Wiren Board.
[  OK  ] Started Wiren Board firmware update service.
[   16.822452] RTW: assoc success
[  OK  ] Started Access point and a…server for Wi-Fi and Ethernet.
[  OK  ] Started LSB: Brings up/down network automatically.
[  OK  ] Started Wiren Board MQTT to IEC 60870-5-104 gateway.
[  OK  ] Started Wiren Board MQTT to OPC UA gateway.
[   18.178942] dwmac-sun8i 5030000.ethernet eth1: Link is Up - 100Mbps/Full - fl                                                                                      ow control rx/tx
[  OK  ] Started MQTT Driver for ADC.
[  OK  ] Started A high performance…er and a reverse proxy server.
         Starting Initialize Wiren Board on successful boot...
         Starting USB Debug Network...
[  OK  ] Started Wiren Board Cloud Agent (wirenboard.cloud).

Debian GNU/Linux 11 wirenboard-AIBYLRXZ ttyS0

wirenboard-AIBYLRXZ login: [   23.653449] Initializing XFRM netlink socket
[   23.688748] bridge: filtering via arp/ip/ip6tables is no longer available by                                                                                       default. Update your scripts to load br_netfilter if you need this.
[   24.819988] br-3af99fd9d4d7: port 1(vethc99dd98) entered blocking state
[   24.826756] br-3af99fd9d4d7: port 1(vethc99dd98) entered disabled state
[   24.833505] vethc99dd98: entered allmulticast mode
[   24.838746] vethc99dd98: entered promiscuous mode
[   24.905717] br-3af99fd9d4d7: port 2(vethd9aaae3) entered blocking state
[   24.912460] br-3af99fd9d4d7: port 2(vethd9aaae3) entered disabled state
[   24.919167] vethd9aaae3: entered allmulticast mode
[   24.924298] vethd9aaae3: entered promiscuous mode
[   25.017381] eth0: renamed from veth024717e
[   25.039006] br-3af99fd9d4d7: port 1(vethc99dd98) entered blocking state
[   25.045721] br-3af99fd9d4d7: port 1(vethc99dd98) entered forwarding state
[   25.053466] eth0: renamed from vethdab4ba4
[   25.076667] br-3af99fd9d4d7: port 2(vethd9aaae3) entered blocking state
[   25.083348] br-3af99fd9d4d7: port 2(vethd9aaae3) entered forwarding state
[   33.762267] dcdc4: disabling