U-Boot 2021.10-wb1.4.1-gbb7b28ca54 (Aug 16 2022 - 09:51:23 +0000)

CPU:   Allwinner R40 (SUN8I 1701)
Model: Wiren Board rev. 7.2.0 (A40i)
I2C:   ready
DRAM:  1 GiB
MMC:   mmc@1c0f000: 0, mmc@1c11000: 1
Loading Environment from MMC... OK
In:    serial@1c28000
Out:   serial@1c28000
Err:   serial@1c28000
Will only keep env vars: mmcpart bootcount upgrade_available uenvcmd otp_program otp_aes_program
## Info: input data size = 142 = 0x8E
bootcount=0
mmcpart=2
uenvcmd=true ; echo reset environment; env default -a; setenv mmcdev 0; saveenv; bmode emmc; reset
upgrade_available=0

Environment size: 142/131068 bytes
## Resetting to default environment
## Info: input data size = 142 = 0x8E
Net:   No ethernet found.
Hit any key to stop autoboot:  0
switch to partitions #0, OK
mmc1(part 0) is current device
eMMC found on device 1
Press FW button to enter firmware update mode

Entering firmware update mode.
Checking if ubootenv part is present
## Loading FIT header to 0x42000000 ...
** File not found .wb-restore/factoryreset.fit **
Read failed: -1Extracting kernel
## Loading FIT header to 0x42000000 ...
** File not found .wb-restore/factoryreset.fit **
Read failed: -1Extracting DTB
## Loading FIT header to 0x43000000 ...
** File not found .wb-restore/factoryreset.fit **
Read failed: -1zimage: Bad magic!
ERROR: Failed to enter update mode!
ERROR: /mnt/data/.wb-restore/factoryreset.fit missing or corrupt
Checking if there is a microSD card with update file
MMC: no card present
Couldn't find partition mmc 0:1
Can't set block device
MMC: no card present
Couldn't find partition mmc 0:1
Can't set block device
No update detected on microSD card, continuing boot
326 bytes read in 3 ms (105.5 KiB/s)
Importing environment from 0x42000000...
Checking if uenvcmd is set ...
test - minimal test like /bin/sh

Usage:
test [args..]
Running default loadzimage ...
6502360 bytes read in 175 ms (35.4 MiB/s)

MMC read: dev # 1, block # 2016, count 32 ... 32 blocks read: OK
Reading overlays list from eMMC
Reading factory fdt name from eMMC
Loading factory fdt sun8i-r40-wirenboard733
55022 bytes read in 6 ms (8.7 MiB/s)
254 bytes read in 2 ms (124 KiB/s)
Applying DT overlay temp-industrial
Applying extra overlay
Booting from mmc ...
Kernel image @ 0x42000000 [ 0x000000 - 0x6337d8 ]
## Flattened Device Tree blob at 43000000
   Booting using the fdt blob at 0x43000000
   Loading Device Tree to 49fdd000, end 49ffffff ... OK

Starting kernel ...

[    0.000000] Booting Linux on physical CPU 0x0
[    0.000000] Linux version 5.10.35-wb172 (root@wbdevenv) (arm-linux-gnueabihf-gcc (Debian 10.2.1-6) 10.2.1 20210110, GNU ld (GNU Binutils for Debian) 2.35.2) #1 SMP Wed Oct 16 09:19:27 UTC 2024
[    0.000000] CPU: ARMv7 Processor [410fc075] revision 5 (ARMv7), cr=10c5387d
[    0.000000] CPU: div instructions available: patching division code
[    0.000000] CPU: PIPT / VIPT nonaliasing data cache, VIPT aliasing instruction cache
[    0.000000] OF: fdt: Machine model: Wiren Board rev. 7.3.3 (A40i)
[    0.000000] Memory policy: Data cache writealloc
[    0.000000] cma: Reserved 16 MiB at 0x7ec00000
[    0.000000] Zone ranges:
[    0.000000]   Normal   [mem 0x0000000040000000-0x000000006fffffff]
[    0.000000]   HighMem  [mem 0x0000000070000000-0x000000007fffffff]
[    0.000000] Movable zone start for each node
[    0.000000] Early memory node ranges
[    0.000000]   node   0: [mem 0x0000000040000000-0x000000007fffffff]
[    0.000000] Initmem setup node 0 [mem 0x0000000040000000-0x000000007fffffff]
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: Using PSCI v0.1 Function IDs from DT
[    0.000000] percpu: Embedded 20 pages/cpu s50444 r8192 d23284 u81920
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 260416
[    0.000000] Kernel command line: console=ttyS0,115200 bootmode=update_auto root=/dev/mmcblk0p2 rootwait ro
[    0.000000] Dentry cache hash table entries: 131072 (order: 7, 524288 bytes, linear)
[    0.000000] Inode-cache hash table entries: 65536 (order: 6, 262144 bytes, linear)
[    0.000000] mem auto-init: stack:off, heap alloc:off, heap free:off
[    0.000000] Memory: 1004500K/1048576K available (10240K kernel code, 1478K rwdata, 3236K rodata, 1024K init, 306K bss, 27692K reserved, 16384K cma-reserved, 245748K highmem)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] ftrace: allocating 31979 entries in 63 pages
[    0.000000] ftrace: allocated 63 pages with 6 groups
[    0.000000] rcu: Hierarchical RCU implementation.
[    0.000000] rcu:     RCU event tracing is enabled.
[    0.000000] rcu:     RCU restricting CPUs from NR_CPUS=8 to nr_cpu_ids=4.
[    0.000000]  Rude variant of Tasks RCU enabled.
[    0.000000]  Tracing variant of Tasks RCU enabled.
[    0.000000] rcu: RCU calculated value of scheduler-enlistment delay is 10 jiffies.
[    0.000000] rcu: Adjusting geometry for rcu_fanout_leaf=16, nr_cpu_ids=4
[    0.000000] NR_IRQS: 16, nr_irqs: 16, preallocated irqs: 16
[    0.000000] GIC: Using split EOI/Deactivate mode
[    0.000000] random: get_random_bytes called from start_kernel+0x660/0x844 with crng_init=0
[    0.000000] clocksource: timer: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 79635851949 ns
[    0.000000] arch_timer: cp15 timer(s) running at 24.00MHz (phys).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x588fe9dc0, max_idle_ns: 440795202592 ns
[    0.000008] sched_clock: 56 bits at 24MHz, resolution 41ns, wraps every 4398046511097ns
[    0.000022] Switching to timer-based delay loop, resolution 41ns
[    0.000352] Console: colour dummy device 80x30
[    0.000604] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=240000)
[    0.000857] pid_max: default: 32768 minimum: 301
[    0.001725] Mount-cache hash table entries: 2048 (order: 1, 8192 bytes, linear)
[    0.001796] Mountpoint-cache hash table entries: 2048 (order: 1, 8192 bytes, linear)
[    0.003748] CPU: Testing write buffer coherency: ok
[    0.004265] /cpus/cpu@0 missing clock-frequency property
[    0.004324] /cpus/cpu@1 missing clock-frequency property
[    0.004378] /cpus/cpu@2 missing clock-frequency property
[    0.004436] /cpus/cpu@3 missing clock-frequency property
[    0.004457] CPU0: thread -1, cpu 0, socket 0, mpidr 80000000
[    0.005662] Setting up static identity map for 0x40100000 - 0x40100060
[    0.005867] rcu: Hierarchical SRCU implementation.
[    0.008369] smp: Bringing up secondary CPUs ...
[    0.019908] CPU1: thread -1, cpu 1, socket 0, mpidr 80000001
[    0.031479] CPU2: thread -1, cpu 2, socket 0, mpidr 80000002
[    0.042820] CPU3: thread -1, cpu 3, socket 0, mpidr 80000003
[    0.043042] smp: Brought up 1 node, 4 CPUs
[    0.043084] SMP: Total of 4 processors activated (192.00 BogoMIPS).
[    0.043099] CPU: All CPU(s) started in HYP mode.
[    0.043113] CPU: Virtualization extensions available.
[    0.044693] devtmpfs: initialized
[    0.066982] VFP support v0.3: implementor 41 architecture 2 part 30 variant 7 rev 5
[    0.067728] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 19112604462750000 ns
[    0.067797] futex hash table entries: 1024 (order: 4, 65536 bytes, linear)
[    0.069289] pinctrl core: initialized pinctrl subsystem
[    0.071050] NET: Registered protocol family 16
[    0.075841] DMA: preallocated 256 KiB pool for atomic coherent allocations
[    0.078222] thermal_sys: Registered thermal governor 'step_wise'
[    0.079214] No ATAGs?
[    0.079568] hw-breakpoint: found 5 (+1 reserved) breakpoint and 4 watchpoint registers.
[    0.079594] hw-breakpoint: maximum watchpoint size is 8 bytes.
[    0.164218] SCSI subsystem initialized
[    0.165435] usbcore: registered new interface driver usbfs
[    0.165653] usbcore: registered new interface driver hub
[    0.165834] usbcore: registered new device driver usb
[    0.166581] mc: Linux media interface: v0.10
[    0.166671] videodev: Linux video capture interface: v2.00
[    0.166801] pps_core: LinuxPPS API ver. 1 registered
[    0.166825] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.166874] PTP clock support registered
[    0.167339] Advanced Linux Sound Architecture Driver Initialized.
[    0.168777] clocksource: Switched to clocksource arch_sys_counter
[    1.316167] NET: Registered protocol family 2
[    1.318371] tcp_listen_portaddr_hash hash table entries: 512 (order: 0, 6144 bytes, linear)
[    1.318489] TCP established hash table entries: 8192 (order: 3, 32768 bytes, linear)
[    1.318665] TCP bind hash table entries: 8192 (order: 4, 65536 bytes, linear)
[    1.318975] TCP: Hash tables configured (established 8192 bind 8192)
[    1.319242] UDP hash table entries: 512 (order: 2, 16384 bytes, linear)
[    1.319342] UDP-Lite hash table entries: 512 (order: 2, 16384 bytes, linear)
[    1.319709] NET: Registered protocol family 1
[    1.320727] RPC: Registered named UNIX socket transport module.
[    1.320755] RPC: Registered udp transport module.
[    1.320771] RPC: Registered tcp transport module.
[    1.320786] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    1.323782] hw perfevents: enabled with armv7_cortex_a7 PMU driver, 5 counters available
[    1.326213] Initialise system trusted keyrings
[    1.326522] workingset: timestamp_bits=14 max_order=18 bucket_order=4
[    1.342434] NFS: Registering the id_resolver key type
[    1.342501] Key type id_resolver registered
[    1.342518] Key type id_legacy registered
[    1.515961] Key type asymmetric registered
[    1.515999] Asymmetric key parser 'x509' registered
[    1.516235] bounce: pool size: 64 pages
[    1.516347] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 247)
[    1.516373] io scheduler mq-deadline registered
[    1.516393] io scheduler kyber registered
[    1.517782] sun4i-usb-phy 1c13400.phy: Couldn't request ID GPIO
[    1.559309] Serial: 8250/16550 driver, 8 ports, IRQ sharing disabled
[    1.583510] brd: module loaded
[    1.602840] loop: module loaded
[    1.611481] libphy: Fixed MDIO Bus: probed
[    1.614589] sun4i-mdio 1c0b080.mdio: supply phy not found, using dummy regulator
[    1.615467] libphy: sun4i_mii_bus: probed
[    1.619378] CAN device driver interface
[    1.622012] PPP generic driver version 2.4.2
[    1.622290] ehci_hcd: USB 2.0 'Enhanced' Host Controller (EHCI) Driver
[    1.622310] ehci-platform: EHCI generic platform driver
[    1.625044] ohci_hcd: USB 1.1 'Open' Host Controller (OHCI) Driver
[    1.625100] ohci-platform: OHCI generic platform driver
[    1.626583] usbcore: registered new interface driver usb-storage
[    1.626718] usbcore: registered new interface driver usbserial_generic
[    1.626766] usbserial: USB Serial support registered for generic
[    1.630686] sun6i-rtc 1c20400.rtc: registered as rtc1
[    1.630719] sun6i-rtc 1c20400.rtc: RTC enabled
[    1.631629] i2c /dev entries driver
[    1.642571] sunxi-wdt 1c20c90.watchdog: Watchdog enabled (timeout=16 sec, nowayout=0)
[    1.647839] ledtrig-cpu: registered to indicate activity on CPUs
[    1.648594] sun8i-ce 1c15000.crypto: Set mod clock to 300000000 (300 Mhz) from 24000000 (24 Mhz)
[    1.649131] sun8i-ce 1c15000.crypto: will run requests pump with realtime priority
[    1.649637] sun8i-ce 1c15000.crypto: will run requests pump with realtime priority
[    1.650554] sun8i-ce 1c15000.crypto: will run requests pump with realtime priority
[    1.651184] sun8i-ce 1c15000.crypto: will run requests pump with realtime priority
[    1.651568] sun8i-ce 1c15000.crypto: Register cbc(aes)
[    1.651972] sun8i-ce 1c15000.crypto: Register ecb(aes)
[    1.652304] sun8i-ce 1c15000.crypto: Register cbc(des3_ede)
[    1.652602] sun8i-ce 1c15000.crypto: Register ecb(des3_ede)
[    1.652912] sun8i-ce 1c15000.crypto: CryptoEngine Die ID 0
[    1.655055] usbcore: registered new interface driver usbhid
[    1.655075] usbhid: USB HID core driver
[    1.659962] iio-rescale a1-volt: using raw+scale source channel
[    1.660406] iio-rescale a2-volt: using raw+scale source channel
[    1.661570] iio-rescale a3-volt: using raw+scale source channel
[    1.662493] iio-rescale vin-volt: using raw+scale source channel
[    1.666812] Initializing XFRM netlink socket
[    1.668480] NET: Registered protocol family 10
[    1.670106] Segment Routing with IPv6
[    1.670261] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    1.671112] NET: Registered protocol family 17
[    1.671145] can: controller area network core
[    1.671273] NET: Registered protocol family 29
[    1.671289] can: raw protocol
[    1.671305] can: broadcast manager protocol
[    1.671326] can: netlink gateway - max_hops=1
[    1.671483] can: SAE J1939
[    1.672689] Key type dns_resolver registered
[    1.672907] Registering SWP/SWPB emulation handler
[    1.673152] registered taskstats version 1
[    1.673280] Loading compiled-in X.509 certificates
[    1.706974] sun4i-usb-phy 1c13400.phy: Couldn't request ID GPIO
[    1.714189] sun4i-pinctrl 1c20800.pinctrl: initialized sunXi PIO driver
[    1.715061] sun4i-pinctrl 1c20800.pinctrl: supply vcc-pb not found, using dummy regulator
[    1.722486] printk: console [ttyS0] disabled
[    1.722792] 1c28000.serial: ttyS0 at MMIO 0x1c28000 (irq = 52, base_baud = 1500000) is a Allwinner sun4i
[    2.692221] printk: console [ttyS0] enabled
[    2.697571] sun4i-pinctrl 1c20800.pinctrl: Couldn't get bank PI regulator
[    2.704545] sun4i-pinctrl 1c20800.pinctrl: request() failed for pin 274
[    2.711263] sun4i-pinctrl 1c20800.pinctrl: pin-274 (1c28800.serial) status -517
[    2.718585] sun4i-pinctrl 1c20800.pinctrl: could not request pin 274 (PI18) from group PI18  on device 1c20800.pinctrl
[    2.729299] dw-apb-uart 1c28800.serial: Error applying setting, reverse things back
[    2.738876] sun4i-mdio 1c0b080.mdio: supply phy not found, using dummy regulator
[    2.747038] libphy: sun4i_mii_bus: probed
[    2.752288] sun4i-pinctrl 1c20800.pinctrl: Couldn't get bank PH regulator
[    2.759241] sun4i-pinctrl 1c20800.pinctrl: request() failed for pin 236
[    2.765896] sun4i-pinctrl 1c20800.pinctrl: pin-236 (1c20800.pinctrl:236) status -517
[    2.777054] sun4i-pinctrl 1c20800.pinctrl: Couldn't get bank PH regulator
[    2.783892] sun4i-pinctrl 1c20800.pinctrl: request() failed for pin 232
[    2.790538] sun4i-pinctrl 1c20800.pinctrl: pin-232 (1c0b000.ethernet) status -517
[    2.798044] sun4i-pinctrl 1c20800.pinctrl: could not request pin 232 (PH8) from group PH8  on device 1c20800.pinctrl
[    2.808640] sun4i-emac 1c0b000.ethernet: Error applying setting, reverse things back
[    2.817346] sun4i-pinctrl 1c20800.pinctrl: Couldn't get bank PA regulator
[    2.824381] sun4i-pinctrl 1c20800.pinctrl: request() failed for pin 0
[    2.830922] sun4i-pinctrl 1c20800.pinctrl: pin-0 (1c50000.ethernet) status -517
[    2.838247] sun4i-pinctrl 1c20800.pinctrl: could not request pin 0 (PA0) from group PA0  on device 1c20800.pinctrl
[    2.848615] dwmac-sun8i 1c50000.ethernet: Error applying setting, reverse things back
[    2.869426] axp20x-i2c 0-0034: AXP20x variant AXP221 found
[    2.886593] vcc-3v3: supplied by regulator-dummy
[    2.892622] vdd-cpu: supplied by regulator-dummy
[    2.898405] vdd-sys: supplied by regulator-dummy
[    2.904232] dcdc4: supplied by regulator-dummy
[    2.909857] vcc-dram: supplied by regulator-dummy
[    2.914784] vcc-gmac-phy: failed to get the current voltage: -EPROBE_DEFER
[    2.921824] vcc-gmac-phy: supplied by vcc-3v3
[    2.927365] dc5ldo: supplied by vcc-dram
[    2.931966] tv: Bringing 700000uV into 3300000-3300000uV
[    2.937980] tv: supplied by regulator-dummy
[    2.942856] aldo2: Bringing 2500000uV into 3300000-3300000uV
[    2.949229] aldo2: supplied by regulator-dummy
[    2.955804] avcc-pll: supplied by regulator-dummy
[    2.962870] eldo1: supplied by regulator-dummy
[    2.968885] eldo2: supplied by regulator-dummy
[    2.974180] vcc-pe: Bringing 1200000uV into 1800000-1800000uV
[    2.981195] vcc-pe: supplied by regulator-dummy
[    2.986390] vcc-sd-alt: Bringing 700000uV into 1800000-1800000uV
[    2.994449] vcc-sd-alt: supplied by regulator-dummy
[    3.001275] dldo2: supplied by regulator-dummy
[    3.007181] dldo3: supplied by regulator-dummy
[    3.013003] dldo4: supplied by regulator-dummy
[    3.018272] rtc_ldo: supplied by regulator-dummy
[    3.024134] ldo_io0: supplied by regulator-dummy
[    3.029872] ldo_io1: supplied by regulator-dummy
[    3.035511] axp20x-adc axp22x-adc: DMA mask not set
[    3.042349] axp20x-battery-power-supply axp20x-battery-power-supply: DMA mask not set
[    3.052541] axp20x-i2c 0-0034: AXP20X driver loaded
[    3.060012] i2c i2c-1: using pinctrl states for GPIO recovery
[    3.065952] gpio-50 (scl): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    3.074895] i2c i2c-1: using generic GPIOs for recovery
[    3.084835] random: fast init done
[    3.109779] rtc-pcf85063 2-0051: registered as rtc0
[    3.124091] rtc-pcf85063 2-0051: setting system clock to 2024-12-24T17:47:44 UTC (1735062464)
[    3.133422] lm75 2-0048: supply vs not found, using dummy regulator
[    3.144243] lm75 2-0048: hwmon1: sensor 'lm75b'
[    3.181982] sun4i-usb-phy 1c13400.phy: phy0 dr_mode=3
[    3.189794] 1c28800.serial: ttyS2 at MMIO 0x1c28800 (irq = 53, base_baud = 1500000) is a Allwinner sun4i
[    3.200178] sun4i-mdio 1c0b080.mdio: supply phy not found, using dummy regulator
[    3.206830] sunxi-mmc 1c11000.mmc: initialized, max. request size: 2048 KB, uses new timings mode
[    3.208132] libphy: sun4i_mii_bus: probed
[    3.342197] mmc0: new DDR MMC card at address 0001
[    3.347915] mmcblk0: mmc0:0001 AS08FC 7.05 GiB
[    3.352949] mmcblk0boot0: mmc0:0001 AS08FC partition 1 4.00 MiB
[    3.359324] mmcblk0boot1: mmc0:0001 AS08FC partition 2 4.00 MiB
[    3.362682] sun4i-emac 1c0b000.ethernet: eth0: at (ptrval), IRQ 65 MAC: 00:85:01:01:00:8f
[    3.365537] mmcblk0rpmb: mmc0:0001 AS08FC partition 3 4.00 MiB, chardev (246:0)
[    3.374449] dwmac-sun8i 1c50000.ethernet: IRQ eth_wake_irq not found
[    3.387220] dwmac-sun8i 1c50000.ethernet: IRQ eth_lpi not found
[    3.393704] dwmac-sun8i 1c50000.ethernet: PTP uses main clock
[    3.399811] dwmac-sun8i 1c50000.ethernet: No HW DMA feature register supported
[    3.407053] dwmac-sun8i 1c50000.ethernet: RX Checksum Offload Engine supported
[    3.414323] dwmac-sun8i 1c50000.ethernet: COE Type 2
[    3.419313] dwmac-sun8i 1c50000.ethernet: TX Checksum insertion supported
[    3.426098] dwmac-sun8i 1c50000.ethernet: Normal descriptors
[    3.431768] dwmac-sun8i 1c50000.ethernet: Chain mode enabled
[    3.438111] libphy: stmmac: probed
[    3.445826]  mmcblk0: p1 p2 p3 p4 < p5 p6 >
[    3.701382] ehci-platform 1c14000.usb: EHCI Host Controller
[    3.706997] ehci-platform 1c14000.usb: new USB bus registered, assigned bus number 1
[    3.715166] ehci-platform 1c14000.usb: irq 37, io mem 0x01c14000
[    3.748778] ehci-platform 1c14000.usb: USB 2.0 started, EHCI 1.00
[    3.755879] hub 1-0:1.0: USB hub found
[    3.759750] hub 1-0:1.0: 1 port detected
[    3.764905] ehci-platform 1c19000.usb: EHCI Host Controller
[    3.770534] ehci-platform 1c19000.usb: new USB bus registered, assigned bus number 2
[    3.778536] ehci-platform 1c19000.usb: irq 39, io mem 0x01c19000
[    3.808778] ehci-platform 1c19000.usb: USB 2.0 started, EHCI 1.00
[    3.815779] hub 2-0:1.0: USB hub found
[    3.819622] hub 2-0:1.0: 1 port detected
[    3.824706] ehci-platform 1c1c000.usb: EHCI Host Controller
[    3.830334] ehci-platform 1c1c000.usb: new USB bus registered, assigned bus number 3
[    3.838293] ehci-platform 1c1c000.usb: irq 41, io mem 0x01c1c000
[    3.869256] ehci-platform 1c1c000.usb: USB 2.0 started, EHCI 1.00
[    3.876231] hub 3-0:1.0: USB hub found
[    3.880056] hub 3-0:1.0: 1 port detected
[    3.978983] ohci-platform 1c14400.usb: Generic Platform OHCI controller
[    3.985622] ohci-platform 1c14400.usb: new USB bus registered, assigned bus number 4
[    3.993596] ohci-platform 1c14400.usb: irq 38, io mem 0x01c14400
[    4.073663] hub 4-0:1.0: USB hub found
[    4.077469] hub 4-0:1.0: 1 port detected
[    4.082674] ohci-platform 1c19400.usb: Generic Platform OHCI controller
[    4.089358] ohci-platform 1c19400.usb: new USB bus registered, assigned bus number 5
[    4.097430] ohci-platform 1c19400.usb: irq 40, io mem 0x01c19400
[    4.173721] hub 5-0:1.0: USB hub found
[    4.177529] hub 5-0:1.0: 1 port detected
[    4.182781] ohci-platform 1c1c400.usb: Generic Platform OHCI controller
[    4.189469] ohci-platform 1c1c400.usb: new USB bus registered, assigned bus number 6
[    4.197266] usb 2-1: new high-speed USB device number 2 using ehci-platform
[    4.204547] ohci-platform 1c1c400.usb: irq 42, io mem 0x01c1c400
[    4.248795] usb 1-1: new high-speed USB device number 2 using ehci-platform
[    4.283692] hub 6-0:1.0: USB hub found
[    4.287498] hub 6-0:1.0: 1 port detected
[    4.293524] of_cfs_init
[    4.296113] of_cfs_init: OK
[    4.303584] ALSA device list:
[    4.306579]   No soundcards found.
[    4.320266] sunxi-mmc 1c0f000.mmc: initialized, max. request size: 16384 KB, uses new timings mode
[    4.340072] EXT4-fs (mmcblk0p2): INFO: recovery required on readonly filesystem
[    4.347401] EXT4-fs (mmcblk0p2): write access will be enabled during recovery
[    4.407981] EXT4-fs (mmcblk0p2): recovery complete
[    4.414442] EXT4-fs (mmcblk0p2): mounted filesystem with ordered data mode. Opts: (null)
[    4.422713] VFS: Mounted root (ext4 filesystem) readonly on device 179:2.
[    4.430314] devtmpfs: mounted
[    4.438154] Freeing unused kernel memory: 1024K
[    4.443007] Run /sbin/init as init process
[    4.475849] usb-storage 1-1:1.0: USB Mass Storage device detected
[    4.483819] scsi host0: usb-storage 1-1:1.0
[    4.704909] systemd[1]: systemd 247.3-7+deb11u6 running in system mode. (+PAM +AUDIT +SELINUX +IMA +APPARMOR +SMACK +SYSVINIT +UTMP +LIBCRYPTSETUP +GCRYPT +GNUTLS +ACL +XZ +LZ4 +ZSTD +SECCOMP +BLKID +ELFUTILS +KMOD +IDN2 -IDN +PCRE2 default-hierarchy=unified)
[    4.731455] systemd[1]: Detected architecture arm.

Welcome to Debian GNU/Linux 11 (bullseye)!

[    4.783476] systemd[1]: Set hostname to <wirenboard-AEAHHCRD>.
[    5.533363] systemd[1]: Queued start job for default target Graphical Interface.
[    5.542892] random: systemd: uninitialized urandom read (16 bytes read)
[    5.553725] systemd[1]: Created slice system-getty.slice.
[  OK  ] Created slice system-getty.slice.
[    5.589056] random: systemd: uninitialized urandom read (16 bytes read)
[    5.597652] systemd[1]: Created slice system-modprobe.slice.
[  OK  ] Created slice system-modprobe.slice.
[    5.639093] random: systemd: uninitialized urandom read (16 bytes read)
[    5.647823] systemd[1]: Created slice system-serial\x2dgetty.slice.
[  OK  ] Created slice system-serial\x2dgetty.slice.
[    5.690794] systemd[1]: Created slice system-systemd\x2dfsck.slice.
[  OK  ] Created slice system-systemd\x2dfsck.slice.
[    5.730409] systemd[1]: Created slice User and Session Slice.
[  OK  ] Created slice User and Session Slice.
[    5.769469] systemd[1]: Started Dispatch Password Requests to Console Directory Watch.
[  OK  ] Started Dispatch Password …ts to Console Directory Watch.
[    5.809328] systemd[1]: Started Forward Password Requests to Wall Directory Watch.
[  OK  ] Started Forward Password R…uests to Wall Directory Watch.
[    5.849304] systemd[1]: Condition check resulted in Arbitrary Executable File Formats File System Automount Point being skipped.
[    5.861341] systemd[1]: Reached target Local Encrypted Volumes.
[  OK  ] Reached target Local Encrypted Volumes.
[    5.899430] systemd[1]: Reached target Paths.
[  OK  ] Reached target Paths.
[    5.929023] systemd[1]: Reached target Remote File Systems.
[  OK  ] Reached target Remote File Systems.
[    5.968978] systemd[1]: Reached target Slices.
[  OK  ] Reached target Slices.
[    6.000251] systemd[1]: Listening on fsck to fsckd communication Socket.
[  OK  ] Listening on fsck to fsckd communication Socket.
[    6.039434] systemd[1]: Listening on initctl Compatibility Named Pipe.
[  OK  ] Listening on initctl Compatibility Named Pipe.
[    6.090119] systemd[1]: Condition check resulted in Journal Audit Socket being skipped.
[    6.099446] systemd[1]: Listening on Journal Socket (/dev/log).
[  OK  ] Listening on Journal Socket (/dev/log).
[    6.140067] systemd[1]: Listening on Journal Socket.
[  OK  ] Listening on Journal Socket.
[    6.177887] systemd[1]: Listening on udev Control Socket.
[  OK  ] Listening on udev Control Socket.
[    6.219816] systemd[1]: Listening on udev Kernel Socket.
[  OK  ] Listening on udev Kernel Socket.
[    6.259932] systemd[1]: Condition check resulted in Huge Pages File System being skipped.
[    6.274000] systemd[1]: Mounting POSIX Message Queue File System...
         Mounting POSIX Message Queue File System...
[    6.315089] systemd[1]: Mounting /sys/kernel/config...
         Mounting /sys/kernel/config...
[    6.355101] systemd[1]: Mounting Kernel Debug File System...
         Mounting Kernel Debug File System...
[    6.395758] systemd[1]: Mounting Kernel Trace File System...
         Mounting Kernel Trace File System...
[    6.437003] systemd[1]: Starting Create list of static device nodes for the current kernel...
         Starting Create list of st…odes for the current kernel...
[    6.486101] systemd[1]: Starting Load Kernel Module drm...
         Starting Load Kernel Module drm...
[    6.526241] systemd[1]: Starting Load Kernel Module fuse...
         Starting Load Kernel Module fuse...
[    6.554014] fuse: init (API version 7.32)
[    6.561542] systemd[1]: Condition check resulted in Set Up Additional Binary Formats being skipped.
[    6.577685] systemd[1]: Starting File System Check on Root Device...
         Starting File System Check on Root Device...
[    6.630231] systemd[1]: Starting Journal Service...
         Starting Journal Service...
[    6.646284] systemd[1]: Starting Load Kernel Modules...
         Starting Load Kernel Modules...
[    6.661466] systemd[1]: Starting Coldplug All udev Devices...
         Starting Coldplug All udev Devices...
[    6.684455] systemd[1]: Mounted POSIX Message Queue File System.
[  OK  ] Mounted POSIX Message Queue File Sy[    6.692369] systemd[1]: Mounted /sys/kernel/config.
stem.
[  OK  ] Mounted /sys/kernel/config.
[    6.703397] systemd[1]: Mounted Kernel Debug File System.
[  OK  ] Mounted Kernel Debug File System    6.714613] systemd[1]: Mounted Kernel Trace File System.
m.
[  OK  ] Mounted Kernel Trace File System.
[    6.781604] systemd[1]: Finished Create list of static device nodes for the current kernel.
[  OK  ] Finished Create list of st… nodes for the current kernel.
[    6.838076] systemd[1]: modprobe@drm.service: Succeeded.
[    6.845113] systemd[1]: Finished Load Kernel Module drm.
[  OK  ] Finished Load Kernel Module drm.
[    6.880836] systemd[1]: modprobe@fuse.service: Succeeded.
[    6.887804] systemd[1]: Finished Load Kernel Module fuse.
[  OK  ] Finished Load Kernel Module fuse.
[    6.930377] systemd[1]: Started Journal Service.
[  OK  ] Started Journal Service.
[  OK  ] Finished File System Check on Root Device.
[  OK  ] Finished Load Kernel Modules.
         Mounting FUSE Control File System...
[  OK  ] Started File System Check Daemon to report status.
         Starting Remount Root and Kernel File Systems...
         Starting Apply Kernel Variables...
[    7.212867] EXT4-fs (mmcblk0p2): re-mounted. Opts: discard,errors=remount-ro
[  OK  ] Mounted FUSE Control File System.
[  OK  ] Finished Remount Root and Kernel File Systems.
[  OK  ] Finished Apply Kernel Variables.
         Starting Load/Save Random Seed...
         Starting Create System Users...
[    7.435049] scsi 0:0:0:0: Direct-Access              USB DISK 2.0     PMAP PQ: 0 ANSI: 6
[    7.445370] sd 0:0:0:0: [sda] 15132672 512-byte logical blocks: (7.75 GB/7.22 GiB)
[    7.456815] sd 0:0:0:0: [sda] Write Protect is off
[    7.463634] sd 0:0:0:0: [sda] No Caching mode page found
[    7.469047] sd 0:0:0:0: [sda] Assuming drive cache: write through
[FAILED] Failed to start Create System Users.
See 'systemctl status systemd-sysusers.service' for details.
[  OK  ] Finished Coldplug All udev Devices.
[    7.569847]  sda: sda1 sda2
[    7.578363] sd 0:0:0:0: [sda] Attached SCSI removable disk
         Starting Helper to synchronize boot up for ifupdown...
         Starting Create Static Device Nodes in /dev...
[  OK  ] Finished Helper to synchronize boot up for ifupdown.
[  OK  ] Finished Create Static Device Nodes in /dev.
[  OK  ] Reached target Local File Systems (Pre).
[  OK  ] Set up automount mnt-sdcard.automount.
         Starting Rule-based Manage…for Device Events and Files...
[  OK  ] Started Rule-based Manager for Device Events and Files.
[    8.331841] Driver for 1-wire Dallas network protocol.
[    8.559363] usb_phy_generic usb_phy_generic.1.auto: supply vcc not found, using dummy regulator
[    8.822008] Bluetooth: Core ver 2.22
[    8.825751] NET: Registered protocol family 31
[    8.830296] Bluetooth: HCI device and connection manager initialized
[    8.835964] cfg80211: Loading compiled-in X.509 certificates for regulatory database
[    8.836690] Bluetooth: HCI socket layer initialized
[    8.836704] Bluetooth: L2CAP socket layer initialized
[    8.836742] Bluetooth: SCO socket layer initialized
[    8.878113] usbcore: registered new interface driver btusb
[    8.896843] Bluetooth: hci0: RTL: examining hci_ver=06 hci_rev=000b lmp_ver=06 lmp_subver=8723
[    8.906848] Bluetooth: hci0: RTL: rom_version status=0 version=1
[    8.912950] Bluetooth: hci0: RTL: loading rtl_bt/rtl8723b_fw.bin
[    8.923510] cfg80211: Loaded X.509 cert 'sforshee: 00b28ddf47aef9cea7'
[    8.926191] Bluetooth: hci0: RTL: loading rtl_bt/rtl8723b_config.bin
[    8.936604] bluetooth hci0: Direct firmware load for rtl_bt/rtl8723b_config.bin failed with error -2
[    8.940946] cfg80211: loaded regulatory.db is malformed or signature is missing/invalid
[    8.945943] Bluetooth: hci0: RTL: cfg_sz -2, total sz 22496
[  OK  ] Found device /dev/mmcblk0p5.
[  OK  ] Found device /dev/mmcblk0p6.
[    9.448502] RTL871X: module init start
[    9.452366] RTL871X: rtl8723bu BT-Coex version = BTCOEX20140507-4E40
[  OK  ] Found device /dev/ttyS0.
[    9.640246] RTL871X: rtw_ndev_init(wlan0)
[    9.645596] RTL871X: rtw_ndev_init(wlan1)
[    9.651523] usbcore: registered new interface driver rtl8723bu
[    9.657398] RTL871X: module init ret=0
[    9.763882] Bluetooth: hci0: RTL: fw version 0x0e2f9f73
[    9.770632] usbcore: registered new interface driver rtl8xxxu
[  OK  ] Reached target Hardware activated USB gadget.
[  OK  ] Listening on Load/Save RF …itch Status /dev/rfkill Watch.
         Activating swap /dev/mmcblk0p5...
         Starting File System Check on /dev/mmcblk0p6...
         Starting Create System Users...
         Starting Load/Save RF Kill Switch Status...
[  OK  ] Started Load/Save RF Kill Switch Status.
[FAILED] Failed to start Create System Users.
See 'systemctl status systemd-sysusers.service' for det[   10.278932] Adding 262140k swap on /dev/mmcblk0p5.  Priority:-2 extents:1 across:262140k SSDsc
ails.
[  OK  ] Activated swap /dev/mmcblk0p5.
[  OK  ] Reached target Swap.
[   10.338876] random: crng init done
[   10.342321] random: 7 urandom warning(s) missed due to ratelimiting
[  OK  ] Finished File System Check on /dev/mmcblk0p6.
[  OK  ] Finished Load/Save Random Seed.
         Mounting /mnt/data...
[   10.472401] EXT4-fs (mmcblk0p6): mounted filesystem with ordered data mode. Opts: discard
[  OK  ] Mounted /mnt/data.
         Mounting /var/log...
[  OK  ] Mounted /var/log.
[  OK  ] Reached target Local File Systems.
[  OK  ] Started ifup for eth0.
[  OK  ] Started ifup for eth1.
         Starting Flush Journal to Persistent Storage...
         Starting prepare mounts and symlinks to config[   10.752893] systemd-journald[142]: Received client request to flush runtime journal.
 files...
[   10.787269] systemd-journald[142]: File /var/log/journal/beb5c6e5945248129a7c187ae8f99c3f/system.journal corrupted or uncleanly shut down, renaming and replacing.
[  OK  ] Finished Flush Journal to Persistent Storage.
[   11.381093] sun4i-emac 1c0b000.ethernet eth0: Link is Up - 100Mbps/Full - flow control off
[   11.391194] IPv6: ADDRCONF(NETDEV_CHANGE): eth0: link becomes ready
[  OK  ] Finished prepare mounts and symlinks to config files.
         Starting Create Volatile Files and Directories...
[  OK  ] Finished Create Volatile Files and Directories.
         Starting Update UTMP about System Boot/Shutdown...
[  OK  ] Finished Update UTMP about System Boot/Shutdown.
[  OK  ] Reached target System Initialization.
[  OK  ] Started Daily apt download activities.
[  OK  ] Started Daily apt upgrade and clean activities.
[  OK  ] Started Periodic ext4 Onli…ata Check for All Filesystems.
[  OK  ] Started Discard unused blocks once a week.
[  OK  ] Started Daily rotation of log files.
[  OK  ] Started Daily Cleanup of Temporary Directories.
[  OK  ] Reached target Timers.
[  OK  ] Listening on Avahi mDNS/DNS-SD Stack Activation Socket.
[  OK  ] Listening on D-Bus System Message Bus Socket.
[  OK  ] Listening on fcgiwrap Socket.
[  OK  ] Listening on KNX Daemon (socket).
[  OK  ] Reached target Sockets.
[  OK  ] Reached target Basic System.
         Starting Bluetooth service...
[  OK  ] Started Regular background program processing daemon.
[  OK  ] Started D-Bus System Message Bus.
         Starting Network Manager...
         Starting Remove Stale Onli…t4 Metadata Check Snapshots...
         Starting Authorization Manager...
         Starting User Login Management...
[   12.850559] Bluetooth: BNEP (Ethernet Emulation) ver 1.3
[   12.856033] Bluetooth: BNEP filters: protocol multicast
[   12.856070] Bluetooth: BNEP socket layer initialized
[  OK  ] Started watch config files.
         Starting Initialize Wiren Board Device Tree overlays...
         Starting Avahi mDNS/DNS-SD Stack...
         Starting WPA supplicant...
[  OK  ] Started Avahi mDNS/DNS-SD Stack.
[  OK  ] Started Bluetooth service.
[  OK  ] Finished Remove Stale Onli…ext4 Metadata Check Snapshots.
[  OK  ] Started Authorization Manager.
[  OK  ] Started WPA supplicant.
[  OK  ] Started User Login Management.
[  OK  ] Reached target Bluetooth.
         Starting Modem Manager...
         Starting Hostname Service...
[FAILED] Failed to start Hostname Service.
See 'systemctl status systemd-hostnamed.service' for details.
[  OK  ] Started Modem Manager.
[  OK  ] Started Network Manager.
         Starting Network Manager Wait Online...
[   14.920115] dwmac-sun8i 1c50000.ethernet eth1: PHY [stmmac-1:00] driver [ICPlus IP101A/G] (irq=POLL)
[   14.931752] dwmac-sun8i 1c50000.ethernet eth1: No Safety Features support found
[   14.939221] dwmac-sun8i 1c50000.ethernet eth1: No MAC Management Counters available
[   14.946922] dwmac-sun8i 1c50000.ethernet eth1: PTP not supported by HW
[   14.959823] dwmac-sun8i 1c50000.ethernet eth1: configuring for phy/mii link mode
[FAILED] Failed to start Initialize…en Board Device Tree overlays.
See 'systemctl status wb-hwconf-manager.service' for details.
[DEPEND] Dependency failed for MQTT… for GPIO-controlled switches.
[DEPEND] Dependency failed for MQTT Driver for ADC.
         Starting Raise network interfaces...
[  OK  ] Started Network connection…rvice for Wiren Board devices.
         Starting Power on GSM modem...
         Starting KNXD Configurator for Wiren Board...
[  OK  ] Finished Raise network interfaces.
[  OK  ] Reached target Network.
         Starting dnsmasq - A light…DHCP and caching DNS server...
         Starting Access point and …rver for Wi-Fi and Ethernet...
         Starting KNX Daemon...
         Starting Mosquitto MQTT Broker...
[FAILED] Failed to start Network Time Service.
See 'systemctl status ntp.service' for details.
         Starting OpenBSD Secure Shell server...
         Starting Permit User Sessions...
[  OK  ] Started MQTT Driver for serial devices.
[  OK  ] Started Kernel 1-Wire MQTT driver for WB-HomA.
         Starting Compensation of s…e-tree (with opposite sign)...
[  OK  ] Started KNX Daemon.
[ INFO ] Skipped dnsmasq - A lightw…t DHCP and caching DNS server.
[ INFO ] Skipped Access point and a…server for Wi-Fi and Ethernet.
[  OK  ] Finished Permit User Sessions.
[ INFO ] Skipped Power on GSM modem.
[  OK  ] Started OpenBSD Secure Shell server.
[  OK  ] Finished Compensation of s…ice-tree (with opposite sign).
[  OK  ] Reached target Host and Network Name Lookups.
[  OK  ] Started Getty on tty1.
         Stopping KNX Daemon...
         Starting A high performanc… and a reverse proxy server...
[  OK  ] Started Serial Getty on ttyS0.
[  OK  ] Reached target Login Prompts.
[  OK  ] Stopped KNX Daemon.
         Starting KNX Daemon...
[  OK  ] Started KNX Daemon.
[  OK  ] Finished KNXD Configurator for Wiren Board.
[  OK  ] Started Mosquitto MQTT Broker.
         Starting Wiren Board Cloud Agent (default)...
[  OK  ] Started Wiren Board modbus devices manager.
[  OK  ] Started one-click diagnost… generating archive with data.
[  OK  ] Started Wiren Board configuration editor backend.
[  OK  ] Started Wiren Board database logger.
         Starting Wiren Board MQTT to IEC 60870-5-104 gateway...
[  OK  ] Started Wiren Board MQTT KNX bridge.
[  OK  ] Started Wiren Board journald to MQTT gateway.
[  OK  ] Started Wiren Board MQTT to Modbus gateway.
[  OK  ] Started metrics sender..
[  OK  ] Started Virtual MQTT devic…r Network Manager connections.
         Starting Wiren Board MQTT to OPC UA gateway...
[  OK  ] Started MQTT Rule engine for Wiren Board.
[  OK  ] Started Wiren Board firmware update service.
[  OK  ] Stopped Network connection…rvice for Wiren Board devices.
[  OK  ] Started Network connection…rvice for Wiren Board devices.
[  OK  ] Started Wiren Board Cloud Agent (default).
[  OK  ] Started A high performance…er and a reverse proxy server.
         Starting Initialize Wiren Board on successful boot...
         Starting USB Debug Network...
[  OK  ] Started Wiren Board MQTT to OPC UA gateway.
[  OK  ] Started Wiren Board MQTT to IEC 60870-5-104 gateway.
[   27.367646] Mass Storage Function, version: 2009/09/11
[   27.373019] LUN: removable file: (no medium)
[   27.471786] using random self ethernet address
[   27.476298] using random host ethernet address

Debian GNU/Linux 11 wirenboard-AEAHHCRD ttyS0

wirenboard-AEAHHCRD login: [   27.860140] dbg0: HOST MAC 1a:55:89:a2:69:44
[   27.864759] dbg0: MAC 1a:55:89:a2:69:43
[   34.408950] vcc-gmac-phy: disabling
[   34.412869] dc5ldo: disabling
[   34.416218] dldo4: disabling
[   34.419688] vdd-sd-power: disabling
[   34.423340] vcc-sd: disabling
[   39.799297] process '/usr/sbin/netplugd' started with executable stack