▒6304344 bytes read in 5615 ms (1.1 MiB/s)

MMC read: dev # 0, block # 2016, count 32 ... 32 blocks read: OK
Reading overlays list from eMMC
Reading factory fdt name from eMMC
Loading factory fdt imx6ul-wirenboard690
47776 bytes read in 105 ms (444.3 KiB/s)
485 bytes read in 146 ms (2.9 KiB/s)
Applying DT overlay wb6-nogsm
597 bytes read in 140 ms (3.9 KiB/s)
Applying DT overlay wb6-wifi-rtl8723bu
509 bytes read in 168 ms (2.9 KiB/s)
Applying DT overlay wb6-noradio
334 bytes read in 109 ms (2.9 KiB/s)
Applying DT overlay wb6-eth1
254 bytes read in 121 ms (2 KiB/s)
Applying DT overlay temp-industrial
Applying extra overlay
Booting from mmc ...
## Flattened Device Tree blob at 83000000
   Booting using the fdt blob at 0x83000000
   Loading Device Tree to bef4c000, end bef6efff ... OK

Starting kernel ...

U-Boot SPL 2017.03-wb1.3.0-g520058c326 (Jan 18 2022 - 10:56:38)
DRAM init ok, rows:16, ncs:1, size: 1024MB
.p0_mpdgctrl0   = 0x011b011b
.p0_mpdgctrl1   = 0x0e3f0e3f
.p0_mprddlctl   = 0x3f3f4143
.p0_mpwrdlctl   = 0x3f3f3732
.p0_mpwldectrl0 = 0x00110011
.p0_mpwldectrl1 = 0x00120012
Trying to boot from MMC1
Warning - USDHC2 controller not supporting

U-Boot 2017.03-wb1.3.0-g520058c326 (Jan 18 2022 - 10:56:38 +0000)

CPU:   Freescale i.MX6ULL rev1.1 792 MHz (running at 396 MHz)
CPU:   Industrial temperature grade (-40C to 105C) at 56C
Reset cause: POR
Model: Wiren Board rev. 6.1 (i.MX6UL)
Board: Wiren Board MX6UL
DRAM:  1 GiB
MMC:   FSL_SDHC: 0
Using default environment

In:    serial
Out:   serial
Err:   serial
Net:   No ethernet found.
Hit any key to stop autoboot:  0
=>
U-Boot SPL 2017.03-wb1.3.0-g520058c326 (Jan 18 2022 - 10:56:38)
DRAM init ok, rows:16, ncs:1, size: 1024MB
.p0_mpdgctrl0   = 0x011c011c
.p0_mpdgctrl1   = 0x0e3f0e3f
.p0_mprddlctl   = 0x3f3f4041
.p0_mpwrdlctl   = 0x3f3f3733
.p0_mpwldectrl0 = 0x00110011
.p0_mpwldectrl1 = 0x00120012
Trying to boot from MMC1
Warning - USDHC2 controller not supporting

U-Boot 2017.03-wb1.3.0-g520058c326 (Jan 18 2022 - 10:56:38 +0000)

CPU:   Freescale i.MX6ULL rev1.1 792 MHz (running at 396 MHz)
CPU:   Industrial temperature grade (-40C to 105C) at 55C
Reset cause: POR
Model: Wiren Board rev. 6.1 (i.MX6UL)
Board: Wiren Board MX6UL
DRAM:  1 GiB
MMC:   FSL_SDHC: 0
Using default environment

In:    serial
Out:   serial
Err:   serial
Net:   No ethernet found.
Hit any key to stop autoboot:  0
=>
U-Boot SPL 2017.03-wb1.3.0-g520058c326 (Jan 18 2022 - 10:56:38)
DRAM init ok, rows:16, ncs:1, size: 1024MB
.p0_mpdgctrl0   = 0x011a011a
.p0_mpdgctrl1   = 0x0e3f0e3f
.p0_mprddlctl   = 0x3f3f4141
.p0_mpwrdlctl   = 0x3f3f3a34
.p0_mpwldectrl0 = 0x00110011
.p0_mpwldectrl1 = 0x00120012
Trying to boot from MMC1
Warning - USDHC2 controller not supporting

U-Boot 2017.03-wb1.3.0-g520058c326 (Jan 18 2022 - 10:56:38 +0000)

CPU:   Freescale i.MX6ULL rev1.1 792 MHz (running at 396 MHz)
CPU:   Industrial temperature grade (-40C to 105C) at 55C
Reset cause: POR
Model: Wiren Board rev. 6.1 (i.MX6UL)
Board: Wiren Board MX6UL
DRAM:  1 GiB
MMC:   FSL_SDHC: 0
Using default environment

In:    serial
Out:   serial
Err:   serial
Net:   No ethernet found.
Hit any key to stop autoboot:  0
Checking if there is a USB storage with update file wb6_update.fit
dev: usb1_vbus @ regulator@0
starting USB...
USB0:   USB EHCI 1.00
USB1:   USB EHCI 1.00
scanning bus 0 for devices... 1 USB Device(s) found
scanning bus 1 for devices... EHCI timed out on TD - token=0x80008c80
unable to get device descriptor (error=-1)
1 USB Device(s) found
       scanning usb for storage devices... 0 Storage Device(s) found
No storage devices, perhaps not 'usb start'ed..?
No USB update detected, continuing boot
switch to partitions #0, OK
mmc0(part 0) is current device
SD/MMC found on device 0
323 bytes read in 61 ms (4.9 KiB/s)
Importing environment from 0x82000000...
Checking if uenvcmd is set ...
Running default loadzimage ...
6304344 bytes read in 5614 ms (1.1 MiB/s)

MMC read: dev # 0, block # 2016, count 32 ... 32 blocks read: OK
Reading overlays list from eMMC
Reading factory fdt name from eMMC
Loading factory fdt imx6ul-wirenboard690
47776 bytes read in 105 ms (444.3 KiB/s)
Applying extra overlay
Booting from mmc ...
## Flattened Device Tree blob at 83000000
   Booting using the fdt blob at 0x83000000
   Loading Device Tree to bef4c000, end bef6efff ... OK

Starting kernel ...

[    0.000000] Booting Linux on physical CPU 0x0
[    0.000000] Linux version 5.10.35-wb133 (jenkins@wbdevenv) (arm-linux-gnueabihf-gcc (Debian 10.2.1-6) 10.2.1 20210110, GNU ld (GNU Binutils for Debian) 2.35.2) #1 Tue Feb 21 08:07:14 UTC 2023
[    0.000000] CPU: ARMv7 Processor [410fc075] revision 5 (ARMv7), cr=10c53c7d
[    0.000000] CPU: div instructions available: patching division code
[    0.000000] CPU: PIPT / VIPT nonaliasing data cache, VIPT aliasing instruction cache
[    0.000000] OF: fdt: Machine model: Wiren Board rev. 6.9.0 (i.MX6UL/ULL)
[    0.000000] Memory policy: Data cache writeback
[    0.000000] cma: Reserved 16 MiB at 0xbf000000
[    0.000000] Zone ranges:
[    0.000000]   Normal   [mem 0x0000000080000000-0x00000000bfffffff]
[    0.000000] Movable zone start for each node
[    0.000000] Early memory node ranges
[    0.000000]   node   0: [mem 0x0000000080000000-0x00000000bfffffff]
[    0.000000] Initmem setup node 0 [mem 0x0000000080000000-0x00000000bfffffff]
[    0.000000] CPU: All CPU(s) started in SVC mode.
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 259840
[    0.000000] Kernel command line: console=ttymxc0,115200 root=/dev/mmcblk0p2 rootwait ro
[    0.000000] Dentry cache hash table entries: 131072 (order: 7, 524288 bytes, linear)
[    0.000000] Inode-cache hash table entries: 65536 (order: 6, 262144 bytes, linear)
[    0.000000] mem auto-init: stack:off, heap alloc:off, heap free:off
[    0.000000] Memory: 1008656K/1048576K available (8192K kernel code, 728K rwdata, 2776K rodata, 1024K init, 283K bss, 23536K reserved, 16384K cma-reserved)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=1, Nodes=1
[    0.000000] NR_IRQS: 16, nr_irqs: 16, preallocated irqs: 16
[    0.000000] random: get_random_bytes called from start_kernel+0x234/0x3dc with crng_init=0
[    0.000000] Switching to timer-based delay loop, resolution 41ns
[    0.000019] sched_clock: 32 bits at 24MHz, resolution 41ns, wraps every 89478484971ns
[    0.000060] clocksource: mxc_timer1: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 79635851949 ns
[    0.002779] Console: colour dummy device 80x30
[    0.002843] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=240000)
[    0.002879] pid_max: default: 32768 minimum: 301
[    0.003294] Mount-cache hash table entries: 2048 (order: 1, 8192 bytes, linear)
[    0.003338] Mountpoint-cache hash table entries: 2048 (order: 1, 8192 bytes, linear)
[    0.005066] CPU: Testing write buffer coherency: ok
[    0.006297] Setting up static identity map for 0x80100000 - 0x80100078
[    0.007304] devtmpfs: initialized
[    0.025082] VFP support v0.3: implementor 41 architecture 2 part 30 variant 7 rev 5
[    0.025601] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 19112604462750000 ns
[    0.025648] futex hash table entries: 256 (order: -1, 3072 bytes, linear)
[    0.027029] pinctrl core: initialized pinctrl subsystem
[    0.029004] NET: Registered protocol family 16
[    0.031318] DMA: preallocated 256 KiB pool for atomic coherent allocations
[    0.033303] thermal_sys: Registered thermal governor 'step_wise'
[    0.033580] cpuidle: using governor menu
[    0.221842] vdd1p1: supplied by regulator-dummy
[    0.233972] vdd3p0: supplied by regulator-dummy
[    0.246132] cpu: supplied by regulator-dummy
[    0.258301] vddsoc: supplied by regulator-dummy
[    0.601688] No ATAGs?
[    0.601748] hw-breakpoint: found 5 (+1 reserved) breakpoint and 4 watchpoint registers.
[    0.601769] hw-breakpoint: maximum watchpoint size is 8 bytes.
[    0.602371] debugfs: Directory 'dummy-iomuxc-gpr@20e4000' with parent 'regmap' already present!
[    0.603034] imx6ul-pinctrl 20e0000.pinctrl: initialized IMX pinctrl driver
[    0.604594] imx6ul-pinctrl 2290000.iomuxc-snvs: no groups defined in /soc/bus@2200000/iomuxc-snvs@2290000
[    0.604633] imx6ul-pinctrl 2290000.iomuxc-snvs: initialized IMX pinctrl driver
[    0.647353] mxs-dma 1804000.dma-apbh: initialized
[    0.652602] SCSI subsystem initialized
[    0.653123] usbcore: registered new interface driver usbfs
[    0.653252] usbcore: registered new interface driver hub
[    0.653442] usbcore: registered new device driver usb
[    0.654275] gpio-48 (i2c_rtc): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.654400] gpio-49 (i2c_rtc): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.655716] i2c-gpio i2c_rtc: using lines 48 (SDA) and 49 (SCL)
[    0.656633] gpio-76 (i2c_eeprom1): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.656760] gpio-67 (i2c_eeprom1): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.657362] i2c-gpio i2c_eeprom1: using lines 76 (SDA) and 67 (SCL)
[    0.658107] gpio-70 (i2c_eeprom2): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.658233] gpio-71 (i2c_eeprom2): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.658853] i2c-gpio i2c_eeprom2: using lines 70 (SDA) and 71 (SCL)
[    0.660434] gpio-30 (scl): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.660793] i2c i2c-1: IMX I2C adapter registered
[    0.661556] mc: Linux media interface: v0.10
[    0.661669] videodev: Linux video capture interface: v2.00
[    0.661803] pps_core: LinuxPPS API ver. 1 registered
[    0.661824] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.661872] PTP clock support registered
[    0.662474] Advanced Linux Sound Architecture Driver Initialized.
[    0.664726] clocksource: Switched to clocksource mxc_timer1
[    0.682507] NET: Registered protocol family 2
[    0.683789] tcp_listen_portaddr_hash hash table entries: 512 (order: 0, 4096 bytes, linear)
[    0.683887] TCP established hash table entries: 8192 (order: 3, 32768 bytes, linear)
[    0.684065] TCP bind hash table entries: 8192 (order: 3, 32768 bytes, linear)
[    0.684250] TCP: Hash tables configured (established 8192 bind 8192)
[    0.684471] UDP hash table entries: 512 (order: 1, 8192 bytes, linear)
[    0.684549] UDP-Lite hash table entries: 512 (order: 1, 8192 bytes, linear)
[    0.685045] NET: Registered protocol family 1
[    0.685987] RPC: Registered named UNIX socket transport module.
[    0.686026] RPC: Registered udp transport module.
[    0.686044] RPC: Registered tcp transport module.
[    0.686060] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.687148] hw perfevents: enabled with armv7_cortex_a7 PMU driver, 5 counters available
[    0.689951] Initialise system trusted keyrings
[    0.690405] workingset: timestamp_bits=14 max_order=18 bucket_order=4
[    0.702049] NFS: Registering the id_resolver key type
[    0.702127] Key type id_resolver registered
[    0.702146] Key type id_legacy registered
[    0.938843] Key type asymmetric registered
[    0.938882] Asymmetric key parser 'x509' registered
[    0.939005] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 247)
[    0.939031] io scheduler mq-deadline registered
[    0.939048] io scheduler kyber registered
[    0.951017] imx-sdma 20ec000.sdma: Direct firmware load for imx/sdma/sdma-imx6q.bin failed with error -2
[    0.951065] imx-sdma 20ec000.sdma: external firmware not found, using ROM firmware
[    0.955027] 2020000.serial: ttymxc0 at MMIO 0x2020000 (irq = 21, base_baud = 5000000) is a IMX
[    1.618256] printk: console [ttymxc0] enabled
[    1.624678] 21e8000.serial: ttymxc1 at MMIO 0x21e8000 (irq = 59, base_baud = 5000000) is a IMX
[    1.668704] imx_rngc 2284000.rng: Freescale RNGB registered (HW revision 2.129)
[    1.676135] random: fast init done
[    1.680085] random: crng init done
[    1.720282] brd: module loaded
[    1.738560] loop: module loaded
[    1.742057] at24 5-0050: supply vcc not found, using dummy regulator
[    1.753541] at24 5-0050: 256 byte 24c02 EEPROM, writable, 1 bytes/write
[    1.760561] at24 6-0050: supply vcc not found, using dummy regulator
[    1.771927] at24 6-0050: 256 byte 24c02 EEPROM, writable, 1 bytes/write
[    1.784363] libphy: Fixed MDIO Bus: probed
[    1.905418] pps pps0: new PPS source ptp0
[    1.911879] libphy: fec_enet_mii_bus: probed
[    1.920677] fec 20b4000.ethernet ethFEC0: registered PHC device 0
[    2.045407] pps pps1: new PPS source ptp1
[    2.086390] libphy: fec_enet_mii_bus: probed
[    2.091662] fec 2188000.ethernet ethFEC1: registered PHC device 1
[    2.098757] PPP generic driver version 2.4.2
[    2.103449] ehci_hcd: USB 2.0 'Enhanced' Host Controller (EHCI) Driver
[    2.110090] ehci-mxc: Freescale On-Chip EHCI Host driver
[    2.115865] usbcore: registered new interface driver usb-storage
[    2.122104] usbcore: registered new interface driver usbserial_generic
[    2.128778] usbserial: USB Serial support registered for generic
[    2.190465] rtc-pcf8563 4-0051: registered as rtc0
[    2.207302] rtc-pcf8563 4-0051: setting system clock to 2023-04-10T18:53:16 UTC (1681152796)
[    2.226079] snvs_rtc 20cc000.snvs:snvs-rtc-lp: registered as rtc1
[    2.232517] i2c /dev entries driver
[    2.239336] lm75 4-0048: supply vs not found, using dummy regulator
[    2.250963] lm75 4-0048: hwmon0: sensor 'lm75b'
[    2.371273] sdhci: Secure Digital Host Controller Interface driver
[    2.377556] sdhci: Copyright(c) Pierre Ossman
[    2.381928] sdhci-pltfm: SDHCI platform and OF driver helper
[    2.395936] ledtrig-cpu: registered to indicate activity on CPUs
[    2.403726] usbcore: registered new interface driver usbhid
[    2.409401] usbhid: USB HID core driver
[    2.424665] Initializing XFRM netlink socket
[    2.429121] mmc0: SDHCI controller on 2194000.mmc [2194000.mmc] using ADMA
[    2.437412] NET: Registered protocol family 10
[    2.445242] Segment Routing with IPv6
[    2.449378] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    2.457455] NET: Registered protocol family 17
[    2.462574] Key type dns_resolver registered
[    2.470970] registered taskstats version 1
[    2.475754] Loading compiled-in X.509 certificates
[    2.498150] imx_thermal 20c8000.anatop:tempmon: Industrial CPU temperature grade - max:105C critical:100C passive:95C
[    2.510109] of_cfs_init
[    2.512804] of_cfs_init: OK
[    2.520714] ALSA device list:
[    2.523730]   No soundcards found.
[    2.527517] Waiting for root device /dev/mmcblk0p2...
[    2.574805] mmc0: new DDR MMC card at address 0001
[    2.581049] mmcblk0: mmc0:0001 008GB0 7.28 GiB
[    2.586352] mmcblk0boot0: mmc0:0001 008GB0 partition 1 8.00 MiB
[    2.592867] mmcblk0boot1: mmc0:0001 008GB0 partition 2 8.00 MiB
[    2.599318] mmcblk0rpmb: mmc0:0001 008GB0 partition 3 4.00 MiB, chardev (245:0)
[    2.611542]  mmcblk0: p1 p2 p3 p4 < p5 p6 >
[    2.654519] EXT4-fs (mmcblk0p2): mounted filesystem with ordered data mode. Opts: (null)
[    2.663081] VFS: Mounted root (ext4 filesystem) readonly on device 179:2.
[    2.671792] devtmpfs: mounted
[    2.681487] Freeing unused kernel memory: 1024K
[    2.686959] Run /sbin/init as init process
/sbin/init: error while loading s[    2.755736] Kernel panic - not syncing: Attempted to kill init! exitcode=0x00007f00
[    2.766188] CPU: 0 PID: 1 Comm: init Not tainted 5.10.35-wb133 #1
[    2.772289] Hardware name: Freescale i.MX6 Ultralite (Device Tree)
[    2.778515] [<b010c8d8>] (unwind_backtrace) from [<b010a0b0>] (show_stack+0x10/0x14)
[    2.786288] [<b010a0b0>] (show_stack) from [<b08abc88>] (panic+0xe8/0x2f4)
[    2.793192] [<b08abc88>] (panic) from [<b011fe38>] (do_exit+0x960/0x9bc)
[    2.799917] [<b011fe38>] (do_exit) from [<b011fefc>] (do_group_exit+0x3c/0xa4)
[    2.807163] [<b011fefc>] (do_group_exit) from [<b011ff74>] (__wake_up_parent+0x0/0x14)
[    2.815099] Rebooting in 10 seconds..

U-Boot SPL 2017.03-wb1.3.0-g520058c326 (Jan 18 2022 - 10:56:38)
DRAM init ok, rows:16, ncs:1, size: 1024MB
.p0_mpdgctrl0   = 0x011f011f
.p0_mpdgctrl1   = 0x0e3f0e3f
.p0_mprddlctl   = 0x3f3f4243
.p0_mpwrdlctl   = 0x3f3f3834
.p0_mpwldectrl0 = 0x000f0011
.p0_mpwldectrl1 = 0x00120012
Trying to boot from MMC1
Warning - USDHC2 controller not supporting

U-Boot 2017.03-wb1.3.0-g520058c326 (Jan 18 2022 - 10:56:38 +0000)

CPU:   Freescale i.MX6ULL rev1.1 792 MHz (running at 396 MHz)
CPU:   Industrial temperature grade (-40C to 105C) at 56C
Reset cause: WDOG
Model: Wiren Board rev. 6.1 (i.MX6UL)
Board: Wiren Board MX6UL
DRAM:  1 GiB
MMC:   FSL_SDHC: 0
Using default environment

In:    serial
Out:   serial
Err:   serial
Net:   eth0: ethernet@02188000
Hit any key to stop autoboot:  0
Checking if there is a USB storage with update file wb6_update.fit
dev: usb1_vbus @ regulator@0
starting USB...
USB0:   USB EHCI 1.00
USB1:   USB EHCI 1.00
scanning bus 0 for devices... 1 USB Device(s) found
scanning bus 1 for devices... EHCI timed out on TD - token=0x80008c80
unable to get device descriptor (error=-1)
1 USB Device(s) found
       scanning usb for storage devices... 0 Storage Device(s) found
No storage devices, perhaps not 'usb start'ed..?
No USB update detected, continuing boot
switch to partitions #0, OK
mmc0(part 0) is current device
SD/MMC found on device 0
323 bytes read in 62 ms (4.9 KiB/s)
Importing environment from 0x82000000...
Checking if uenvcmd is set ...
Running default loadzimage ...
6304344 bytes read in 5614 ms (1.1 MiB/s)

MMC read: dev # 0, block # 2016, count 32 ... 32 blocks read: OK
Reading overlays list from eMMC
Reading factory fdt name from eMMC
Loading factory fdt imx6ul-wirenboard690
47776 bytes read in 105 ms (444.3 KiB/s)
485 bytes read in 147 ms (2.9 KiB/s)
Applying DT overlay wb6-nogsm
597 bytes read in 140 ms (3.9 KiB/s)
Applying DT overlay wb6-wifi-rtl8723bu
509 bytes read in 168 ms (2.9 KiB/s)
Applying DT overlay wb6-noradio
334 bytes read in 108 ms (2.9 KiB/s)
Applying DT overlay wb6-eth1
254 bytes read in 121 ms (2 KiB/s)
Applying DT overlay temp-industrial
Applying extra overlay
Booting from mmc ...
## Flattened Device Tree blob at 83000000
   Booting using the fdt blob at 0x83000000
   Loading Device Tree to bef4c000, end bef6efff ... OK

Starting kernel ...

U-Boot SPL 2017.03-wb1.3.0-g520058c326 (Jan 18 2022 - 10:56:38)
DRAM init ok, rows:16, ncs:1, size: 1024MB
.p0_mpdgctrl0   = 0x01180118
.p0_mpdgctrl1   = 0x0e3f0e3f
.p0_mprddlctl   = 0x3f3f4042
.p0_mpwrdlctl   = 0x3f3f3833
.p0_mpwldectrl0 = 0x00100011
.p0_mpwldectrl1 = 0x00120012
Trying to boot from MMC1
Warning - USDHC2 controller not supporting

U-Boot 2017.03-wb1.3.0-g520058c326 (Jan 18 2022 - 10:56:38 +0000)

CPU:   Freescale i.MX6ULL rev1.1 792 MHz (running at 396 MHz)
CPU:   Industrial temperature grade (-40C to 105C) at 55C
Reset cause: POR
Model: Wiren Board rev. 6.1 (i.MX6UL)
Board: Wiren Board MX6UL
DRAM:  1 GiB
MMC:   FSL_SDHC: 0
Using default environment

In:    serial
Out:   serial
Err:   serial
Net:   No ethernet found.
Hit any key to stop autoboot:  0
Checking if there is a USB storage with update file wb6_update.fit
dev: usb1_vbus @ regulator@0
starting USB...
USB0:   USB EHCI 1.00
USB1:   USB EHCI 1.00
scanning bus 0 for devices... 1 USB Device(s) found
scanning bus 1 for devices... EHCI timed out on TD - token=0x80008c80
unable to get device descriptor (error=-1)
1 USB Device(s) found
       scanning usb for storage devices... 0 Storage Device(s) found
No storage devices, perhaps not 'usb start'ed..?
No USB update detected, continuing boot
switch to partitions #0, OK
mmc0(part 0) is current device
SD/MMC found on device 0
323 bytes read in 61 ms (4.9 KiB/s)
Importing environment from 0x82000000...
Checking if uenvcmd is set ...
Running default loadzimage ...
6304344 bytes read in 5614 ms (1.1 MiB/s)

MMC read: dev # 0, block # 2016, count 32 ... 32 blocks read: OK
Reading overlays list from eMMC
Reading factory fdt name from eMMC
Loading factory fdt imx6ul-wirenboard690
47776 bytes read in 105 ms (444.3 KiB/s)
485 bytes read in 147 ms (2.9 KiB/s)
Applying DT overlay wb6-nogsm
597 bytes read in 141 ms (3.9 KiB/s)
Applying DT overlay wb6-wifi-rtl8723bu
509 bytes read in 168 ms (2.9 KiB/s)
Applying DT overlay wb6-noradio
334 bytes read in 108 ms (2.9 KiB/s)
Applying DT overlay wb6-eth1
254 bytes read in 121 ms (2 KiB/s)
Applying DT overlay temp-industrial
Applying extra overlay
Booting from mmc ...
## Flattened Device Tree blob at 83000000
   Booting using the fdt blob at 0x83000000
   Loading Device Tree to bef4c000, end bef6efff ... OK

Starting kernel ...

[    0.000000] Booting Linux on physical CPU 0x0
[    0.000000] Linux version 5.10.35-wb133 (jenkins@wbdevenv) (arm-linux-gnueabihf-gcc (Debian 10.2.1-6) 10.2.1 20210110, GNU ld (GNU Binutils for Debian) 2.35.2) #1 Tue Feb 21 08:07:14 UTC 2023
[    0.000000] CPU: ARMv7 Processor [410fc075] revision 5 (ARMv7), cr=10c53c7d
[    0.000000] CPU: div instructions available: patching division code
[    0.000000] CPU: PIPT / VIPT nonaliasing data cache, VIPT aliasing instruction cache
[    0.000000] OF: fdt: Machine model: Wiren Board rev. 6.9.0 (i.MX6UL/ULL)
[    0.000000] Memory policy: Data cache writeback
[    0.000000] cma: Reserved 16 MiB at 0xbf000000
[    0.000000] Zone ranges:
[    0.000000]   Normal   [mem 0x0000000080000000-0x00000000bfffffff]
[    0.000000] Movable zone start for each node
[    0.000000] Early memory node ranges
[    0.000000]   node   0: [mem 0x0000000080000000-0x00000000bfffffff]
[    0.000000] Initmem setup node 0 [mem 0x0000000080000000-0x00000000bfffffff]
[    0.000000] CPU: All CPU(s) started in SVC mode.
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 259840
[    0.000000] Kernel command line: console=ttymxc0,115200 root=/dev/mmcblk0p2 rootwait ro
[    0.000000] Dentry cache hash table entries: 131072 (order: 7, 524288 bytes, linear)
[    0.000000] Inode-cache hash table entries: 65536 (order: 6, 262144 bytes, linear)
[    0.000000] mem auto-init: stack:off, heap alloc:off, heap free:off
[    0.000000] Memory: 1008652K/1048576K available (8192K kernel code, 728K rwdata, 2776K rodata, 1024K init, 283K bss, 23540K reserved, 16384K cma-reserved)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=1, Nodes=1
[    0.000000] NR_IRQS: 16, nr_irqs: 16, preallocated irqs: 16
[    0.000000] random: get_random_bytes called from start_kernel+0x234/0x3dc with crng_init=0
[    0.000000] Switching to timer-based delay loop, resolution 41ns
[    0.000019] sched_clock: 32 bits at 24MHz, resolution 41ns, wraps every 89478484971ns
[    0.000057] clocksource: mxc_timer1: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 79635851949 ns
[    0.002804] Console: colour dummy device 80x30
[    0.002865] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=240000)
[    0.002903] pid_max: default: 32768 minimum: 301
[    0.003320] Mount-cache hash table entries: 2048 (order: 1, 8192 bytes, linear)
[    0.003365] Mountpoint-cache hash table entries: 2048 (order: 1, 8192 bytes, linear)
[    0.005083] CPU: Testing write buffer coherency: ok
[    0.006317] Setting up static identity map for 0x80100000 - 0x80100078
[    0.007323] devtmpfs: initialized
[    0.025306] VFP support v0.3: implementor 41 architecture 2 part 30 variant 7 rev 5
[    0.025827] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 19112604462750000 ns
[    0.025872] futex hash table entries: 256 (order: -1, 3072 bytes, linear)
[    0.027249] pinctrl core: initialized pinctrl subsystem
[    0.029251] NET: Registered protocol family 16
[    0.031554] DMA: preallocated 256 KiB pool for atomic coherent allocations
[    0.033579] thermal_sys: Registered thermal governor 'step_wise'
[    0.033865] cpuidle: using governor menu
[    0.221800] vdd1p1: supplied by regulator-dummy
[    0.233932] vdd3p0: supplied by regulator-dummy
[    0.246092] cpu: supplied by regulator-dummy
[    0.258260] vddsoc: supplied by regulator-dummy
[    0.601131] No ATAGs?
[    0.601192] hw-breakpoint: found 5 (+1 reserved) breakpoint and 4 watchpoint registers.
[    0.601211] hw-breakpoint: maximum watchpoint size is 8 bytes.
[    0.601815] debugfs: Directory 'dummy-iomuxc-gpr@20e4000' with parent 'regmap' already present!
[    0.602475] imx6ul-pinctrl 20e0000.pinctrl: initialized IMX pinctrl driver
[    0.604037] imx6ul-pinctrl 2290000.iomuxc-snvs: no groups defined in /soc/bus@2200000/iomuxc-snvs@2290000
[    0.604076] imx6ul-pinctrl 2290000.iomuxc-snvs: initialized IMX pinctrl driver
[    0.646928] mxs-dma 1804000.dma-apbh: initialized
[    0.652209] SCSI subsystem initialized
[    0.652686] usbcore: registered new interface driver usbfs
[    0.652811] usbcore: registered new interface driver hub
[    0.652946] usbcore: registered new device driver usb
[    0.653868] gpio-48 (i2c_rtc): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.653998] gpio-49 (i2c_rtc): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.655319] i2c-gpio i2c_rtc: using lines 48 (SDA) and 49 (SCL)
[    0.656204] gpio-76 (i2c_eeprom1): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.656332] gpio-67 (i2c_eeprom1): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.656921] i2c-gpio i2c_eeprom1: using lines 76 (SDA) and 67 (SCL)
[    0.657625] gpio-70 (i2c_eeprom2): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.657745] gpio-71 (i2c_eeprom2): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.658335] i2c-gpio i2c_eeprom2: using lines 70 (SDA) and 71 (SCL)
[    0.659921] gpio-30 (scl): enforced open drain please flag it properly in DT/ACPI DSDT/board file
[    0.660285] i2c i2c-1: IMX I2C adapter registered
[    0.661019] mc: Linux media interface: v0.10
[    0.661132] videodev: Linux video capture interface: v2.00
[    0.661264] pps_core: LinuxPPS API ver. 1 registered
[    0.661285] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.661340] PTP clock support registered
[    0.661970] Advanced Linux Sound Architecture Driver Initialized.
[    0.664201] clocksource: Switched to clocksource mxc_timer1
[    0.681919] NET: Registered protocol family 2
[    0.683193] tcp_listen_portaddr_hash hash table entries: 512 (order: 0, 4096 bytes, linear)
[    0.683294] TCP established hash table entries: 8192 (order: 3, 32768 bytes, linear)
[    0.683470] TCP bind hash table entries: 8192 (order: 3, 32768 bytes, linear)
[    0.683656] TCP: Hash tables configured (established 8192 bind 8192)
[    0.683874] UDP hash table entries: 512 (order: 1, 8192 bytes, linear)
[    0.683949] UDP-Lite hash table entries: 512 (order: 1, 8192 bytes, linear)
[    0.684440] NET: Registered protocol family 1
[    0.685375] RPC: Registered named UNIX socket transport module.
[    0.685413] RPC: Registered udp transport module.
[    0.685430] RPC: Registered tcp transport module.
[    0.685446] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.686524] hw perfevents: enabled with armv7_cortex_a7 PMU driver, 5 counters available
[    0.689331] Initialise system trusted keyrings
[    0.689783] workingset: timestamp_bits=14 max_order=18 bucket_order=4
[    0.701472] NFS: Registering the id_resolver key type
[    0.701561] Key type id_resolver registered
[    0.701581] Key type id_legacy registered
[    0.942515] Key type asymmetric registered
[    0.942555] Asymmetric key parser 'x509' registered
[    0.942683] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 247)
[    0.942706] io scheduler mq-deadline registered
[    0.942723] io scheduler kyber registered
[    0.954860] imx-sdma 20ec000.sdma: Direct firmware load for imx/sdma/sdma-imx6q.bin failed with error -2
[    0.954909] imx-sdma 20ec000.sdma: external firmware not found, using ROM firmware
[    0.958782] 2020000.serial: ttymxc0 at MMIO 0x2020000 (irq = 21, base_baud = 5000000) is a IMX
[    1.622079] printk: console [ttymxc0] enabled
[    1.628565] 21e8000.serial: ttymxc1 at MMIO 0x21e8000 (irq = 59, base_baud = 5000000) is a IMX
[    1.672406] imx_rngc 2284000.rng: Freescale RNGB registered (HW revision 2.129)
[    1.679837] random: fast init done
[    1.683793] random: crng init done
[    1.723847] brd: module loaded
[    1.742127] loop: module loaded
[    1.745732] at24 5-0050: supply vcc not found, using dummy regulator
[    1.757171] at24 5-0050: 256 byte 24c02 EEPROM, writable, 1 bytes/write
[    1.764133] at24 6-0050: supply vcc not found, using dummy regulator
[    1.775576] at24 6-0050: 256 byte 24c02 EEPROM, writable, 1 bytes/write
[    1.788031] libphy: Fixed MDIO Bus: probed
[    1.914900] pps pps0: new PPS source ptp0
[    1.921354] libphy: fec_enet_mii_bus: probed
[    1.930135] fec 20b4000.ethernet ethFEC0: registered PHC device 0
[    2.054897] pps pps1: new PPS source ptp1
[    2.095937] libphy: fec_enet_mii_bus: probed
[    2.101232] fec 2188000.ethernet ethFEC1: registered PHC device 1
[    2.108325] PPP generic driver version 2.4.2
[    2.113011] ehci_hcd: USB 2.0 'Enhanced' Host Controller (EHCI) Driver
[    2.119649] ehci-mxc: Freescale On-Chip EHCI Host driver
[    2.125408] usbcore: registered new interface driver usb-storage
[    2.131654] usbcore: registered new interface driver usbserial_generic
[    2.138329] usbserial: USB Serial support registered for generic
[    2.200070] rtc-pcf8563 4-0051: registered as rtc0
[    2.216920] rtc-pcf8563 4-0051: setting system clock to 2023-04-10T18:53:58 UTC (1681152838)
[    2.235696] snvs_rtc 20cc000.snvs:snvs-rtc-lp: registered as rtc1
[    2.242136] i2c /dev entries driver
[    2.248970] lm75 4-0048: supply vs not found, using dummy regulator
[    2.260650] lm75 4-0048: hwmon0: sensor 'lm75b'
[    2.380887] sdhci: Secure Digital Host Controller Interface driver
[    2.387169] sdhci: Copyright(c) Pierre Ossman
[    2.391540] sdhci-pltfm: SDHCI platform and OF driver helper
[    2.405549] ledtrig-cpu: registered to indicate activity on CPUs
[    2.413332] usbcore: registered new interface driver usbhid
[    2.419003] usbhid: USB HID core driver
[    2.434352] Initializing XFRM netlink socket
[    2.438742] mmc0: SDHCI controller on 2194000.mmc [2194000.mmc] using ADMA
[    2.447031] NET: Registered protocol family 10
[    2.454862] Segment Routing with IPv6
[    2.459025] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    2.467084] NET: Registered protocol family 17
[    2.472194] Key type dns_resolver registered
[    2.480626] registered taskstats version 1
[    2.485420] Loading compiled-in X.509 certificates
[    2.507766] imx_thermal 20c8000.anatop:tempmon: Industrial CPU temperature grade - max:105C critical:100C passive:95C
[    2.519721] of_cfs_init
[    2.522410] of_cfs_init: OK
[    2.530359] ALSA device list:
[    2.533374]   No soundcards found.
[    2.537150] Waiting for root device /dev/mmcblk0p2...
[    2.584473] mmc0: new DDR MMC card at address 0001
[    2.591820] mmcblk0: mmc0:0001 008GB0 7.28 GiB
[    2.597668] mmcblk0boot0: mmc0:0001 008GB0 partition 1 8.00 MiB
[    2.604781] mmcblk0boot1: mmc0:0001 008GB0 partition 2 8.00 MiB
[    2.611424] mmcblk0rpmb: mmc0:0001 008GB0 partition 3 4.00 MiB, chardev (245:0)
[    2.624372]  mmcblk0: p1 p2 p3 p4 < p5 p6 >
[    2.662982] EXT4-fs (mmcblk0p2): mounted filesystem with ordered data mode. Opts: (null)
[    2.671553] VFS: Mounted root (ext4 filesystem) readonly on device 179:2.
[    2.680022] devtmpfs: mounted
[    2.686289] Freeing unused kernel memory: 1024K
[    2.692069] Run /sbin/init as init process
/sbin/init: error while loading s[    2.762562] Kernel panic - not syncing: Attempted to kill init! exitcode=0x00007f00
[    2.773010] CPU: 0 PID: 1 Comm: init Not tainted 5.10.35-wb133 #1
[    2.779109] Hardware name: Freescale i.MX6 Ultralite (Device Tree)
[    2.785336] [<b010c8d8>] (unwind_backtrace) from [<b010a0b0>] (show_stack+0x10/0x14)
[    2.793105] [<b010a0b0>] (show_stack) from [<b08abc88>] (panic+0xe8/0x2f4)
[    2.800009] [<b08abc88>] (panic) from [<b011fe38>] (do_exit+0x960/0x9bc)
[    2.806736] [<b011fe38>] (do_exit) from [<b011fefc>] (do_group_exit+0x3c/0xa4)
[    2.813980] [<b011fefc>] (do_group_exit) from [<b011ff74>] (__wake_up_parent+0x0/0x14)
[    2.821916] Rebooting in 10 seconds..

U-Boot SPL 2017.03-wb1.3.0-g520058c326 (Jan 18 2022 - 10:56:38)
DRAM init ok, rows:16, ncs:1, size: 1024MB
.p0_mpdgctrl0   = 0x011e011b
.p0_mpdgctrl1   = 0x0e3f0e3f
.p0_mprddlctl   = 0x3f3f4244
.p0_mpwrdlctl   = 0x3f3f3833
.p0_mpwldectrl0 = 0x00100011
.p0_mpwldectrl1 = 0x00120012
Trying to boot from MMC1
Warning - USDHC2 controller not supporting

U-Boot 2017.03-wb1.3.0-g520058c326 (Jan 18 2022 - 10:56:38 +0000)

CPU:   Freescale i.MX6ULL rev1.1 792 MHz (running at 396 MHz)
CPU:   Industrial temperature grade (-40C to 105C) at 56C
Reset cause: WDOG
Model: Wiren Board rev. 6.1 (i.MX6UL)
Board: Wiren Board MX6UL
DRAM:  1 GiB
MMC:   FSL_SDHC: 0
Using default environment

In:    serial
Out:   serial
Err:   serial
Net:   eth0: ethernet@02188000
Hit any key to stop autoboot:  0
Checking if there is a USB storage with update file wb6_update.fit
dev: usb1_vbus @ regulator@0
starting USB...
USB0:   USB EHCI 1.00
USB1:   USB EHCI 1.00
scanning bus 0 for devices... 1 USB Device(s) found
scanning bus 1 for devices...