j........................
326 bytes read in 6 ms (52.7 KiB/s)
Importing environment from 0x42000000...
Checking if uenvcmd is set ...
test - minimal test like /bin/sh

Usage:
test [args..]
Running default loadzimage ...
6042192 bytes read in 132 ms (43.7 MiB/s)

MMC read: dev # 1, block # 2016, count 32 ... 32 blocks read: OK
Reading overlays list from eMMC
Reading factory fdt name from eMMC
Loading factory fdt sun8i-r40-wirenboard733
54704 bytes read in 10 ms (5.2 MiB/s)
254 bytes read in 3 ms (82 KiB/s)
Applying DT overlay temp-industrial
Applying extra overlay
Booting from mmc ...
Kernel image @ 0x42000000 [ 0x000000 - 0x5c3250 ]
## Flattened Device Tree blob at 43000000
   Booting using the fdt blob at 0x43000000
   Loading Device Tree to 49fdd000, end 49ffffff ... OK

Starting kernel ...

[    0.000000] Booting Linux on physical CPU 0x0
[    0.000000] Linux version 5.10.35-wb120+wb101 (jenkins@wbdevenv) (arm-linux-gnueabihf-gcc (Debian 10.2.1-6) 10.2.1 20210110, GNU ld (GNU Binutils for Debian) 2.35.2) #2 SMP Tue Nov 22 12:49:35 UTC 2022
[    0.000000] CPU: ARMv7 Processor [410fc075] revision 5 (ARMv7), cr=10c5387d
[    0.000000] CPU: div instructions available: patching division code
[    0.000000] CPU: PIPT / VIPT nonaliasing data cache, VIPT aliasing instruction cache
[    0.000000] OF: fdt: Machine model: Wiren Board rev. 7.3.3 (A40i)
[    0.000000] Memory policy: Data cache writealloc
[    0.000000] cma: Reserved 16 MiB at 0x7ec00000
[    0.000000] Zone ranges:
[    0.000000]   Normal   [mem 0x0000000040000000-0x000000006fffffff]
[    0.000000]   HighMem  [mem 0x0000000070000000-0x000000007fffffff]
[    0.000000] Movable zone start for each node
[    0.000000] Early memory node ranges
[    0.000000]   node   0: [mem 0x0000000040000000-0x000000007fffffff]
[    0.000000] Initmem setup node 0 [mem 0x0000000040000000-0x000000007fffffff]
[    0.000000] psci: probing for conduit method from DT.
[    0.000000] psci: Using PSCI v0.1 Function IDs from DT
[    0.000000] percpu: Embedded 19 pages/cpu s47884 r8192 d21748 u77824
[    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 260416
[    0.000000] Kernel command line: console=ttyS0,115200 root=/dev/mmcblk0p2 rootwait ro
[    0.000000] Dentry cache hash table entries: 131072 (order: 7, 524288 bytes, linear)
[    0.000000] Inode-cache hash table entries: 65536 (order: 6, 262144 bytes, linear)
[    0.000000] mem auto-init: stack:off, heap alloc:off, heap free:off
[    0.000000] Memory: 1006628K/1048576K available (9216K kernel code, 1430K rwdata, 3068K rodata, 1024K init, 293K bss, 25564K reserved, 16384K cma-reserved, 245748K highmem)
[    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
[    0.000000] ftrace: allocating 29913 entries in 59 pages
[    0.000000] ftrace: allocated 59 pages with 5 groups
[    0.000000] rcu: Hierarchical RCU implementation.
[    0.000000] rcu:     RCU event tracing is enabled.
[    0.000000] rcu:     RCU restricting CPUs from NR_CPUS=8 to nr_cpu_ids=4.
[    0.000000]  Rude variant of Tasks RCU enabled.
[    0.000000] rcu: RCU calculated value of scheduler-enlistment delay is 10 jiffies.
[    0.000000] rcu: Adjusting geometry for rcu_fanout_leaf=16, nr_cpu_ids=4
[    0.000000] NR_IRQS: 16, nr_irqs: 16, preallocated irqs: 16
[    0.000000] GIC: Using split EOI/Deactivate mode
[    0.000000] random: get_random_bytes called from start_kernel+0x660/0x840 with crng_init=0
[    0.000000] clocksource: timer: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 79635851949 ns
[    0.000000] arch_timer: cp15 timer(s) running at 24.00MHz (phys).
[    0.000000] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0x588fe9dc0, max_idle_ns: 440795202592 ns
[    0.000007] sched_clock: 56 bits at 24MHz, resolution 41ns, wraps every 4398046511097ns
[    0.000020] Switching to timer-based delay loop, resolution 41ns
[    0.000327] Console: colour dummy device 80x30
[    0.000394] Calibrating delay loop (skipped), value calculated using timer frequency.. 48.00 BogoMIPS (lpj=240000)
[    0.000422] pid_max: default: 32768 minimum: 301
[    0.000626] Mount-cache hash table entries: 2048 (order: 1, 8192 bytes, linear)
[    0.000652] Mountpoint-cache hash table entries: 2048 (order: 1, 8192 bytes, linear)
[    0.001689] CPU: Testing write buffer coherency: ok
[    0.002110] /cpus/cpu@0 missing clock-frequency property
[    0.002155] /cpus/cpu@1 missing clock-frequency property
[    0.002197] /cpus/cpu@2 missing clock-frequency property
[    0.002242] /cpus/cpu@3 missing clock-frequency property
[    0.002259] CPU0: thread -1, cpu 0, socket 0, mpidr 80000000
[    0.003191] Setting up static identity map for 0x40100000 - 0x40100060
[    0.003384] rcu: Hierarchical SRCU implementation.
[    0.004249] smp: Bringing up secondary CPUs ...
[    0.015319] CPU1: thread -1, cpu 1, socket 0, mpidr 80000001
[    0.026548] CPU2: thread -1, cpu 2, socket 0, mpidr 80000002
[    0.037662] CPU3: thread -1, cpu 3, socket 0, mpidr 80000003
[    0.037834] smp: Brought up 1 node, 4 CPUs
[    0.037869] SMP: Total of 4 processors activated (192.00 BogoMIPS).
[    0.037881] CPU: All CPU(s) started in HYP mode.
[    0.037893] CPU: Virtualization extensions available.
[    0.038837] devtmpfs: initialized
[    0.051537] VFP support v0.3: implementor 41 architecture 2 part 30 variant 7 rev 5
[    0.051835] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 19112604462750000 ns
[    0.051869] futex hash table entries: 1024 (order: 4, 65536 bytes, linear)
[    0.052824] pinctrl core: initialized pinctrl subsystem
[    0.054292] NET: Registered protocol family 16
[    0.056768] DMA: preallocated 256 KiB pool for atomic coherent allocations
[    0.058075] thermal_sys: Registered thermal governor 'step_wise'
[    0.058537] No ATAGs?
[    0.058755] hw-breakpoint: found 5 (+1 reserved) breakpoint and 4 watchpoint registers.
[    0.058773] hw-breakpoint: maximum watchpoint size is 8 bytes.
[    0.104980] SCSI subsystem initialized
[    0.105245] usbcore: registered new interface driver usbfs
[    0.105308] usbcore: registered new interface driver hub
[    0.105377] usbcore: registered new device driver usb
[    0.105733] mc: Linux media interface: v0.10
[    0.105783] videodev: Linux video capture interface: v2.00
[    0.105848] pps_core: LinuxPPS API ver. 1 registered
[    0.105862] pps_core: Software ver. 5.3.6 - Copyright 2005-2007 Rodolfo Giometti <giometti@linux.it>
[    0.105900] PTP clock support registered
[    0.106209] Advanced Linux Sound Architecture Driver Initialized.
[    0.107282] clocksource: Switched to clocksource arch_sys_counter
[    0.759271] NET: Registered protocol family 2
[    0.759982] tcp_listen_portaddr_hash hash table entries: 512 (order: 0, 6144 bytes, linear)
[    0.760040] TCP established hash table entries: 8192 (order: 3, 32768 bytes, linear)
[    0.760121] TCP bind hash table entries: 8192 (order: 4, 65536 bytes, linear)
[    0.760244] TCP: Hash tables configured (established 8192 bind 8192)
[    0.760406] UDP hash table entries: 512 (order: 2, 16384 bytes, linear)
[    0.760480] UDP-Lite hash table entries: 512 (order: 2, 16384 bytes, linear)
[    0.760765] NET: Registered protocol family 1
[    0.762017] RPC: Registered named UNIX socket transport module.
[    0.762042] RPC: Registered udp transport module.
[    0.762055] RPC: Registered tcp transport module.
[    0.762066] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.763666] hw perfevents: enabled with armv7_cortex_a7 PMU driver, 5 counters available
[    0.765228] Initialise system trusted keyrings
[    0.765519] workingset: timestamp_bits=14 max_order=18 bucket_order=4
[    0.774108] NFS: Registering the id_resolver key type
[    0.774166] Key type id_resolver registered
[    0.774180] Key type id_legacy registered
[    0.774766] Key type asymmetric registered
[    0.774787] Asymmetric key parser 'x509' registered
[    0.774926] bounce: pool size: 64 pages
[    0.774984] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 247)
[    0.775001] io scheduler mq-deadline registered
[    0.775015] io scheduler kyber registered
[    0.776113] sun4i-usb-phy 1c13400.phy: Couldn't request ID GPIO
[    0.858083] Serial: 8250/16550 driver, 8 ports, IRQ sharing disabled
[    0.872036] brd: module loaded
[    0.882748] loop: module loaded
[    0.888432] libphy: Fixed MDIO Bus: probed
[    0.889596] sun4i-mdio 1c0b080.mdio: supply phy not found, using dummy regulator
[    0.890246] libphy: sun4i_mii_bus: probed
[    0.892285] CAN device driver interface
[    0.894263] PPP generic driver version 2.4.2
[    0.894536] ehci_hcd: USB 2.0 'Enhanced' Host Controller (EHCI) Driver
[    0.894553] ehci-platform: EHCI generic platform driver
[    0.895576] ohci_hcd: USB 1.1 'Open' Host Controller (OHCI) Driver
[    0.895613] ohci-platform: OHCI generic platform driver
[    0.896659] usbcore: registered new interface driver usb-storage
[    0.896773] usbcore: registered new interface driver usbserial_generic
[    0.896813] usbserial: USB Serial support registered for generic
[    0.899001] sun6i-rtc 1c20400.rtc: registered as rtc1
[    0.899025] sun6i-rtc 1c20400.rtc: RTC enabled
[    0.899386] i2c /dev entries driver
[    0.905420] sunxi-wdt 1c20c90.watchdog: Watchdog enabled (timeout=16 sec, nowayout=0)
[    0.908402] ledtrig-cpu: registered to indicate activity on CPUs
[    0.909000] sun8i-ce 1c15000.crypto: Set mod clock to 300000000 (300 Mhz) from 24000000 (24 Mhz)
[    0.909361] sun8i-ce 1c15000.crypto: will run requests pump with realtime priority
[    0.909844] sun8i-ce 1c15000.crypto: will run requests pump with realtime priority
[    0.910070] sun8i-ce 1c15000.crypto: will run requests pump with realtime priority
[    0.910273] sun8i-ce 1c15000.crypto: will run requests pump with realtime priority
[    0.910434] sun8i-ce 1c15000.crypto: Register cbc(aes)
[    0.910637] sun8i-ce 1c15000.crypto: Register ecb(aes)
[    0.910837] sun8i-ce 1c15000.crypto: Register cbc(des3_ede)
[    0.911021] sun8i-ce 1c15000.crypto: Register ecb(des3_ede)
[    0.911239] sun8i-ce 1c15000.crypto: CryptoEngine Die ID 0
[    0.913016] usbcore: registered new interface driver usbhid
[    0.913033] usbhid: USB HID core driver
[    0.915581] iio-rescale a1-volt: using raw+scale source channel
[    0.915959] iio-rescale a2-volt: using raw+scale source channel
[    0.916288] iio-rescale a3-volt: using raw+scale source channel
[    0.916613] iio-rescale vin-volt: using raw+scale source channel
[    0.920079] NET: Registered protocol family 10
[    0.921233] Segment Routing with IPv6
[    0.921319] sit: IPv6, IPv4 and MPLS over IPv4 tunneling driver
[    0.922089] NET: Registered protocol family 17
[    0.922117] can: controller area network core
[    0.922222] NET: Registered protocol family 29
[    0.922239] can: raw protocol
[    0.922254] can: broadcast manager protocol
[    0.922275] can: netlink gateway - max_hops=1
[    0.922518] Key type dns_resolver registered
[    0.922608] Registering SWP/SWPB emulation handler
[    0.922723] registered taskstats version 1
[    0.922781] Loading compiled-in X.509 certificates
[    0.942665] sun4i-usb-phy 1c13400.phy: Couldn't request ID GPIO
[    0.947126] sun4i-pinctrl 1c20800.pinctrl: initialized sunXi PIO driver
[    0.948035] sun4i-pinctrl 1c20800.pinctrl: supply vcc-pb not found, using dummy regulator
[    0.952880] printk: console [ttyS0] disabled
[    0.953036] 1c28000.serial: ttyS0 at MMIO 0x1c28000 (irq = 52, base_baud = 1500000) is a Allwinner sun4i
[    1.906011] printk: console [ttyS0] enabled
[    1.911274] sun4i-pinctrl 1c20800.pinctrl: Couldn't get bank PI regulator
[    1.918136] sun4i-pinctrl 1c20800.pinctrl: request() failed for pin 274
[    1.924752] sun4i-pinctrl 1c20800.pinctrl: pin-274 (1c28800.serial) status -517
[    1.932093] sun4i-pinctrl 1c20800.pinctrl: could not request pin 274 (PI18) from group PI18  on device 1c20800.pinctrl
[    1.942805] dw-apb-uart 1c28800.serial: Error applying setting, reverse things back
[    1.951191] sun4i-mdio 1c0b080.mdio: supply phy not found, using dummy regulator
[    1.959297] libphy: sun4i_mii_bus: probed
[    1.964229] sun4i-pinctrl 1c20800.pinctrl: Couldn't get bank PH regulator
[    1.971080] sun4i-pinctrl 1c20800.pinctrl: request() failed for pin 236
[    1.977732] sun4i-pinctrl 1c20800.pinctrl: pin-236 (1c20800.pinctrl:236) status -517
[    1.987202] sun4i-pinctrl 1c20800.pinctrl: Couldn't get bank PH regulator
[    1.994030] sun4i-pinctrl 1c20800.pinctrl: request() failed for pin 232
[    2.000668] sun4i-pinctrl 1c20800.pinctrl: pin-232 (1c0b000.ethernet) status -517
[    2.008171] sun4i-pinctrl 1c20800.pinctrl: could not request pin 232 (PH8) from group PH8  on device 1c20800.pinctrl
[    2.018714] sun4i-emac 1c0b000.ethernet: Error applying setting, reverse things back
[    2.027134] sun4i-pinctrl 1c20800.pinctrl: Couldn't get bank PA regulator
[    2.033946] sun4i-pinctrl 1c20800.pinctrl: request() failed for pin 0
[    2.040402] sun4i-pinctrl 1c20800.pinctrl: pin-0 (1c50000.ethernet) status -517
[    2.047723] sun4i-pinctrl 1c20800.pinctrl: could not request pin 0 (PA0) from group PA0  on device 1c20800.pinctrl
[    2.058078] dwmac-sun8i 1c50000.ethernet: Error applying setting, reverse things back
[    2.072769] axp20x-i2c 0-0034: AXP20x variant AXP221 found
[    2.086811] input: axp20x-pek as /devices/platform/soc/1c2ac00.i2c/i2c-0/0-0034/axp221-pek/input/input0
[    2.106773] vcc-3v3: supplied by regulator-dummy
[    2.112412] vdd-cpu: supplied by regulator-dummy
[    2.117916] vdd-sys: supplied by regulator-dummy
[    2.123436] dcdc4: supplied by regulator-dummy
[    2.128821] vcc-dram: supplied by regulator-dummy
[    2.133696] vcc-gmac-phy: failed to get the current voltage: -EPROBE_DEFER
[    2.140716] vcc-gmac-phy: supplied by vcc-3v3
[    2.146124] dc5ldo: supplied by vcc-dram
[    2.150249] random: fast init done
[    2.153985] tv: Bringing 700000uV into 3300000-3300000uV
[    2.160007] tv: supplied by regulator-dummy
[    2.164782] aldo2: Bringing 2500000uV into 3300000-3300000uV
[    2.171112] aldo2: supplied by regulator-dummy
[    2.176899] avcc-pll: supplied by regulator-dummy
[    2.182571] eldo1: supplied by regulator-dummy
[    2.187968] eldo2: supplied by regulator-dummy
[    2.193050] vcc-pe: Bringing 1200000uV into 1800000-1800000uV
[    2.199930] vcc-pe: supplied by regulator-dummy
[    2.205062] vcc-sd-alt: Bringing 700000uV into 1800000-1800000uV
[    2.212099] vcc-sd-alt: supplied by regulator-dummy
[    2.217932] dldo2: supplied by regulator-dummy
[    2.223300] dldo3: supplied by regulator-dummy
[    2.228706] dldo4: supplied by regulator-dummy
[    2.233688] rtc_ldo: supplied by regulator-dummy
[    2.239216] ldo_io0: supplied by regulator-dummy
[    2.244730] ldo_io1: supplied by regulator-dummy
[    2.250128] axp20x-adc axp22x-adc: DMA mask not set
[    2.256787] axp20x-battery-power-supply axp20x-battery-power-supply: DMA mask not set
[    2.266831] axp20x-i2c 0-0034: AXP20X driver loaded
[    2.297147] rtc-pcf85063 2-0051: registered as rtc0
[    2.311446] rtc-pcf85063 2-0051: setting system clock to 2025-04-11T08:26:57 UTC (1744360017)
[    2.320525] lm75 2-0048: supply vs not found, using dummy regulator
[    2.331222] lm75 2-0048: hwmon1: sensor 'lm75b'
[    2.361766] sun4i-usb-phy 1c13400.phy: phy0 dr_mode=3
[    2.370354] 1c28800.serial: ttyS2 at MMIO 0x1c28800 (irq = 53, base_baud = 1500000) is a Allwinner sun4i
[    2.380782] sun4i-mdio 1c0b080.mdio: supply phy not found, using dummy regulator
[    2.388792] libphy: sun4i_mii_bus: probed
[    2.395570] sunxi-mmc 1c11000.mmc: initialized, max. request size: 2048 KB, uses new timings mode
[    2.511685] mmc0: new DDR MMC card at address 0001
[    2.517418] mmcblk0: mmc0:0001 DG4008 7.28 GiB
[    2.522332] mmcblk0boot0: mmc0:0001 DG4008 partition 1 4.00 MiB
[    2.528711] mmcblk0boot1: mmc0:0001 DG4008 partition 2 4.00 MiB
[    2.531066] sun4i-emac 1c0b000.ethernet: eth0: at (ptrval), IRQ 65 MAC: 00:85:01:01:3e:62
[    2.534929] mmcblk0rpmb: mmc0:0001 DG4008 partition 3 4.00 MiB, chardev (246:0)
[    2.543858] dwmac-sun8i 1c50000.ethernet: IRQ eth_wake_irq not found
[    2.556582] dwmac-sun8i 1c50000.ethernet: IRQ eth_lpi not found
[    2.563019] dwmac-sun8i 1c50000.ethernet: PTP uses main clock
[    2.569130] dwmac-sun8i 1c50000.ethernet: No HW DMA feature register supported
[    2.576371] dwmac-sun8i 1c50000.ethernet: RX Checksum Offload Engine supported
[    2.583643] dwmac-sun8i 1c50000.ethernet: COE Type 2
[    2.588633] dwmac-sun8i 1c50000.ethernet: TX Checksum insertion supported
[    2.595418] dwmac-sun8i 1c50000.ethernet: Normal descriptors
[    2.601090] dwmac-sun8i 1c50000.ethernet: Chain mode enabled
[    2.607457] libphy: stmmac: probed
[    2.612251]  mmcblk0: p1 p2 p3 p4 < p5 p6 >
[    2.869829] ehci-platform 1c14000.usb: EHCI Host Controller
[    2.875448] ehci-platform 1c14000.usb: new USB bus registered, assigned bus number 1
[    2.883630] ehci-platform 1c14000.usb: irq 37, io mem 0x01c14000
[    2.917285] ehci-platform 1c14000.usb: USB 2.0 started, EHCI 1.00
[    2.924419] hub 1-0:1.0: USB hub found
[    2.928283] hub 1-0:1.0: 1 port detected
[    2.933445] ehci-platform 1c19000.usb: EHCI Host Controller
[    2.939073] ehci-platform 1c19000.usb: new USB bus registered, assigned bus number 2
[    2.947075] ehci-platform 1c19000.usb: irq 39, io mem 0x01c19000
[    2.977286] ehci-platform 1c19000.usb: USB 2.0 started, EHCI 1.00
[    2.984296] hub 2-0:1.0: USB hub found
[    2.988121] hub 2-0:1.0: 1 port detected
[    2.993190] ehci-platform 1c1c000.usb: EHCI Host Controller
[    2.998812] ehci-platform 1c1c000.usb: new USB bus registered, assigned bus number 3
[    3.006806] ehci-platform 1c1c000.usb: irq 41, io mem 0x01c1c000
[    3.037721] ehci-platform 1c1c000.usb: USB 2.0 started, EHCI 1.00
[    3.044683] hub 3-0:1.0: USB hub found
[    3.048512] hub 3-0:1.0: 1 port detected
[    3.147370] ohci-platform 1c14400.usb: Generic Platform OHCI controller
[    3.154012] ohci-platform 1c14400.usb: new USB bus registered, assigned bus number 4
[    3.161976] ohci-platform 1c14400.usb: irq 38, io mem 0x01c14400
[    3.242161] hub 4-0:1.0: USB hub found
[    3.245982] hub 4-0:1.0: 1 port detected
[    3.251115] ohci-platform 1c19400.usb: Generic Platform OHCI controller
[    3.257776] ohci-platform 1c19400.usb: new USB bus registered, assigned bus number 5
[    3.265725] ohci-platform 1c19400.usb: irq 40, io mem 0x01c19400
[    3.342209] hub 5-0:1.0: USB hub found
[    3.346016] hub 5-0:1.0: 1 port detected
[    3.351128] ohci-platform 1c1c400.usb: Generic Platform OHCI controller
[    3.357802] ohci-platform 1c1c400.usb: new USB bus registered, assigned bus number 6
[    3.365595] usb 2-1: new high-speed USB device number 2 using ehci-platform
[    3.372876] ohci-platform 1c1c400.usb: irq 42, io mem 0x01c1c400
[    3.452212] hub 6-0:1.0: USB hub found
[    3.456021] hub 6-0:1.0: 1 port detected
[    3.462052] of_cfs_init
[    3.463425] sunxi-mmc 1c0f000.mmc: Got CD GPIO
[    3.464628] of_cfs_init: OK
[    3.476433] ALSA device list:
[    3.479467]   No soundcards found.
[    3.494423] sunxi-mmc 1c0f000.mmc: initialized, max. request size: 16384 KB, uses new timings mode
[    3.513256] EXT4-fs (mmcblk0p2): INFO: recovery required on readonly filesystem
[    3.520645] EXT4-fs (mmcblk0p2): write access will be enabled during recovery
[    3.549382] EXT4-fs (mmcblk0p2): orphan cleanup on readonly fs
[    3.555509] EXT4-fs (mmcblk0p2): 2 orphan inodes deleted
[    3.560870] EXT4-fs (mmcblk0p2): recovery complete
[    3.580774] EXT4-fs (mmcblk0p2): mounted filesystem with ordered data mode. Opts: (null)
[    3.588995] VFS: Mounted root (ext4 filesystem) readonly on device 179:2.
[    3.597082] devtmpfs: mounted
[    3.604732] Freeing unused kernel memory: 1024K
[    3.609545] Run /sbin/init as init process
[    3.829399] random: systemd: uninitialized urandom read (16 bytes read)
[    3.840864] systemd[1]: systemd 232 running in system mode. (+PAM +AUDIT +SELINUX +IMA +APPARMOR +SMACK +SYSVINIT +UTMP +LIBCRYPTSETUP +GCRYPT +GNUTLS +ACL +XZ +LZ4 +SECCOMP +BLKID +ELFUTILS +KMOD +IDN)
[    3.864209] systemd[1]: Detected architecture arm.

Welcome to Debian GNU/Linux 9 (stretch)!

[    3.898426] systemd[1]: Set hostname to <wirenboard-AX2XSEYE>.
[    3.932297] random: systemd: uninitialized urandom read (16 bytes read)
[    3.948209] random: systemd-sysv-ge: uninitialized urandom read (16 bytes read)
[    4.181744] systemd[1]: [/lib/systemd/system/wb-mqtt-w1.service:10] Unknown lvalue 'StartLimitIntervalSec' in section 'Service'
[    4.254957] systemd[1]: Listening on fsck to fsckd communication Socket.
[  OK  ] Listening on fsck to fsckd communication Socket.
[    4.297803] systemd[1]: Listening on udev Kernel Socket.
[  OK  ] Listening on udev Kernel Socket.
[    4.327692] systemd[1]: Listening on Syslog Socket.
[  OK  ] Listening on Syslog Socket.
[    4.357734] systemd[1]: Listening on Journal Socket.
[  OK  ] Listening on Journal Socket.
[    4.387616] systemd[1]: Reached target Remote File Systems.
[  OK  ] Reached target Remote File Systems.
[    4.417653] systemd[1]: Listening on /dev/initctl Compatibility Named Pipe.
[  OK  ] Listening on /dev/initctl Compatibility Named Pipe.
[  OK  ] Listening on udev Control Socket.
[  OK  ] Listening on Journal Socket (/dev/log).
[  OK  ] Started Dispatch Password Requests to Console Directory Watch.
[  OK  ] Started Forward Password Requests to Wall Directory Watch.
[  OK  ] Reached target Encrypted Volumes.
[  OK  ] Created slice User and Session Slice.
[  OK  ] Created slice System Slice.
[  OK  ] Created slice system-systemd\x2dfsck.slice.
[  OK  ] Created slice system-getty.slice.
         Starting File System Check on Root Device...
         Starting Journal Service...
[  OK  ] Created slice system-serial\x2dgetty.slice.
         Starting Load Kernel Modules...
         Mounting Debug File System...
         Mounting POSIX Message Queue File System...
[  OK  ] Reached target Slices.
         Mounting /sys/kernel/config...
[  OK  ] Created slice system-openvpn.slice.
         Starting Create list of required st…ce nodes for the current kernel...
[  OK  ] Mounted POSIX Message Queue File System.
[  OK  ] Mounted Debug File System.
[  OK  ] Mounted /sys/kernel/config.
[  OK  ] Started Journal Service.
[  OK  ] Started File System Check on Root Device.
[  OK  ] Started Load Kernel Modules.
[  OK  ] Started Create list of required sta…vice nodes for the current kernel.
[  OK  ] Started File System Check Daemon to report status.
         Starting Create Static Device Nodes in /dev...
         Starting Apply Kernel Variables...
         Starting Remount Root and Kernel File Systems...
[    5.421140] EXT4-fs (mmcblk0p2): re-mounted. Opts: errors=remount-ro
[  OK  ] Started Create Static Device Nodes in /dev.
[  OK  ] Started Apply Kernel Variables.
[  OK  ] Started Remount Root and Kernel File Systems.
         Starting Load/Save Random Seed...
         Starting udev Coldplug all Devices...
         Starting prepare partitions at first boot...
         Starting udev Kernel Device Manager...
[  OK  ] Started Load/Save Random Seed.
[  OK  ] Started udev Kernel Device Manager.
[  OK  ] Started prepare partitions at first boot.
[  OK  ] Reached target Local File Systems (Pre).
[    6.193588] Driver for 1-wire Dallas network protocol.
[  OK  ] Started udev Coldplug all Devices.
[    6.359451] usb_phy_generic usb_phy_generic.1.auto: supply vcc not found, using dummy regulator
[  OK  ] Found device /dev/ttyS0.
[    6.465342] cfg80211: Loading compiled-in X.509 certificates for regulatory database
[    6.476834] Bluetooth: Core ver 2.22
[    6.480621] NET: Registered protocol family 31
[    6.485097] Bluetooth: HCI device and connection manager initialized
[    6.491588] Bluetooth: HCI socket layer initialized
[    6.496509] Bluetooth: L2CAP socket layer initialized
[    6.501703] Bluetooth: SCO socket layer initialized
[  OK  ] Found device /dev/mmcblk0p6.
[    6.529210] usbcore: registered new interface driver btusb
[    6.537426] Bluetooth: hci0: RTL: examining hci_ver=06 hci_rev=000b lmp_ver=06 lmp_subver=8723
[    6.538180] cfg80211: Loaded X.509 cert 'sforshee: 00b28ddf47aef9cea7'
[    6.557504] Bluetooth: hci0: RTL: rom_version status=0 version=1
[    6.558111] platform regulatory.0: Direct firmware load for regulatory.db failed with error -2
[    6.563544] Bluetooth: hci0: RTL: loading rtl_bt/rtl8723b_fw.bin
[    6.578534] cfg80211: failed to load regulatory.db
[    6.587419] Bluetooth: hci0: RTL: loading rtl_bt/rtl8723b_config.bin
[    6.593955] bluetooth hci0: Direct firmware load for rtl_bt/rtl8723b_config.bin failed with error -2
[    6.603466] Bluetooth: hci0: RTL: cfg_sz -2, total sz 22496
[  OK  ] Found device /dev/mmcblk0p5.
         Activating swap /dev/mmcblk0p5...
         Starting File System Check on /dev/mmcblk0p6...
[    6.987986] Adding 262140k swap on /dev/mmcblk0p5.  Priority:-2 extents:1 across:262140k SS
[    7.001330] RTL871X: module init start
[    7.005145] RTL871X: rtl8723bu v4.3.6.11_12942.20141204_BTCOEX20140507-4E40
[    7.012227] RTL871X: rtl8723bu BT-Coex version = BTCOEX20140507-4E40
[  OK  ] Activated swap /dev/mmcblk0p5.
[  OK  ] Started File System Check on /dev/mmcblk0p6.
[    7.222840] RTL871X: rtw_ndev_init(wlan0)
[    7.230327] RTL871X: rtw_ndev_init(wlan1)
[    7.235831] usbcore: registered new interface driver rtl8723bu
[    7.241812] RTL871X: module init ret=0
[    7.345610] usbcore: registered new interface driver rtl8xxxu
[    7.430414] Bluetooth: hci0: RTL: fw version 0x0e2f9f73
[  OK  ] Listening on Load/Save RF Kill Switch Status /dev/rfkill Watch.
         Mounting /mnt/data...
[  OK  ] Reached target Swap.
[    7.969026] EXT4-fs (mmcblk0p6): mounted filesystem with ordered data mode. Opts: (null)
         Starting Load/Save RF Kill Switch Status...
[  OK  ] Mounted /mnt/data.
[  OK  ] Started Load/Save RF Kill Switch Status.
         Mounting /var/log...
[  OK  ] Mounted /var/log.
[  OK  ] Reached target Local File Systems.
[  OK  ] Started ifup for eth1.
         Starting prepare mounts and symlinks to config files...
[  OK  ] Started ifup for wlan0.
[  OK  ] Started ifup for eth0.
         Starting Flush Journal to Persistent Storage...
[    8.429316] systemd-journald[118]: Received request to flush runtime journal from PID 1
[    8.471553] systemd-journald[118]: File /var/log/journal/c084018070af24d075c42c6463613f91/system.journal corrupted or uncleanly shut down, renaming and replacing.
[  OK  ] Started Flush Journal to Persistent Storage.
[  OK  ] Started prepare mounts and symlinks to config files.
         Starting Create Volatile Files and Directories...
[FAILED] Failed to start Create Volatile Files and Directories.
See 'systemctl status systemd-tmpfiles-setup.service' for details.
         Starting Update UTMP about System Boot/Shutdown...
[  OK  ] Reached target System Time Synchronized.
[  OK  ] Started Update UTMP about System Boot/Shutdown.
[    9.282574] RTL871X: RTW_ADAPTIVITY_EN_
[    9.282607] AUTO, chplan:0x20, Regulation:3,3
[    9.291040] RTL871X: RTW_ADAPTIVITY_MODE_
[    9.291052] NORMAL
[  OK  ] Reached target System Initialization.
[  OK  ] Listening on D-Bus System Message Bus Socket.
[  OK  ] Listening on PC/SC Smart Card Daemon Activation Socket.
[  OK  ] Started Daily Cleanup of Temporary Directories.
[  OK  ] Started Daily apt download activities.
[  OK  ] Listening on Avahi mDNS/DNS-SD Stack Activation Socket.
[  OK  ] Started Daily apt upgrade and clean activities.
[  OK  ] Reached target Timers.
[  OK  ] Started Monitor directories with device templates for wb-mqtt-serial.
[  OK  ] Reached target Paths.
[  OK  ] Listening on KNX Daemon (socket).
[  OK  ] Reached target Sockets.
[  OK  ] Reached target Basic System.
[  OK  ] Started Regular background program processing daemon.
[  OK  ] Started Cgroup management daemon.
         Starting System Logging Service...
[    9.812878] new mount options do not match the existing superblock, will be ignored
         Starting Mosquitto MQTT v3.1/v3.1.1 Broker...
         Starting initialize filesystems at first boot...
[  OK  ] Started watch config files.
         Starting Initialize Wiren Board Device Tree overlays...
[  OK  ] Started D-Bus System Message Bus.
[   12.099416] RTL871X: nolinked power save enter
[   12.148866] dwmac-sun8i 1c50000.ethernet eth1: PHY [stmmac-1:00] driver [ICPlus IP101A/G] (irq=POLL)
[   12.164503] dwmac-sun8i 1c50000.ethernet eth1: No Safety Features support found
[   12.171978] dwmac-sun8i 1c50000.ethernet eth1: No MAC Management Counters available
[   12.179729] dwmac-sun8i 1c50000.ethernet eth1: PTP not supported by HW
[   12.196623] dwmac-sun8i 1c50000.ethernet eth1: configuring for phy/mii link mode
[   33.777348] vcc-gmac-phy: disabling
[   33.781220] dc5ldo: disabling
[   33.784543] dldo4: disabling
[   33.787835] vdd-sd-power: disabling
[   33.791361] vcc-sd: disabling
         Starting OpenVPN connection to tun0...
         Starting OpenVPN connection to tun3...
         Starting Restore /etc/resolv.conf i…fore the ppp link was shut down...
         Starting Bluetooth service...
[  OK  ] Started Generates wb-mqtt-serial UI schema for wb-mqtt-confed.
         Starting Restore local date from Wiren Board GSM RTC...
         Starting Login Service...
[  OK  ] Started System Logging Service.
[FAILED] Failed to start Mosquitto MQTT v3.1/v3.1.1 Broker.
See 'systemctl status mosquitto.service' for details.
[DEPEND] Dependency failed for MQTT Rule engine for Wiren Board.
[  OK  ] Started initialize filesystems at first boot.
[  OK  ] Started OpenVPN connection to tun0.
[  OK  ] Started OpenVPN connection to tun3.
[  OK  ] Started Restore /etc/resolv.conf if…before the ppp link was shut down.
[  OK  ] Started Restore local date from Wiren Board GSM RTC.
[   38.845825] random: crng init done
[   38.849273] random: 7 urandom warning(s) missed due to ratelimiting
[   39.577950] 1c29000.serial: ttyS4 at MMIO 0x1c29000 (irq = 130, base_baud = 1500000) is a Allwinner sun4i
[  OK  ] Started Initialize Wiren Board Device Tree overlays.
[FAILED] Failed to start Login Service.
See 'systemctl status systemd-logind.service' for details.
[FAILED] Failed to start Bluetooth service.
See 'systemctl status bluetooth.service' for details.